FSP Configuration
  Board "Custom User Board (Any Device)"
  R7FA4M2AC3CNE
    part_number: R7FA4M2AC3CNE
    rom_size_bytes: 393216
    ram_size_bytes: 131072
    data_flash_size_bytes: 8192
    package_style: QFN
    package_pins: 48
    
  RA4M2
    series: 4
    
  RA4M2 Family
    Security: Exceptions: Exception Response: Non-Maskable Interrupt
    Security: Exceptions: BusFault, HardFault, and NMI Target: Secure State
    Security: System Reset Request Accessibility: Secure State
    Security: Exceptions: Prioritize Secure Exceptions: Disabled
    Security: Cache Accessibility: Both Secure and Non-Secure State
    Security: System Reset Status Accessibility: Both Secure and Non-Secure State
    Security: Battery Backup Accessibility: Both Secure and Non-Secure State
    Security: SRAM Accessibility: SRAM Protection: Both Secure and Non-Secure State
    Security: SRAM Accessibility: SRAM ECC: Both Secure and Non-Secure State
    Security: SRAM Accessibility: Standby RAM: Regions 7-0 are all Secure.
    Security: BUS Accessibility: Bus Security Attribution Register A: Both Secure and Non-Secure State
    Security: BUS Accessibility: Bus Security Attribution Register B: Both Secure and Non-Secure State
    Security: Uninitialized Non-Secure Application Fallback: Enable Uninitialized Non-Secure Application Fallback
    Startup C-Cache Line Size: 32 Bytes
    OFS0 register settings: Independent WDT: Start Mode: IWDT is Disabled
    OFS0 register settings: Independent WDT: Timeout Period: 2048 cycles
    OFS0 register settings: Independent WDT: Dedicated Clock Frequency Divisor: 128
    OFS0 register settings: Independent WDT: Window End Position:  0% (no window end position)
    OFS0 register settings: Independent WDT: Window Start Position: 100% (no window start position)
    OFS0 register settings: Independent WDT: Reset Interrupt Request Select: Reset is enabled
    OFS0 register settings: Independent WDT: Stop Control: Stop counting when in Sleep, Snooze mode, or Software Standby
    OFS0 register settings: WDT: Start Mode Select: Stop WDT after a reset (register-start mode)
    OFS0 register settings: WDT: Timeout Period: 16384 cycles
    OFS0 register settings: WDT: Clock Frequency Division Ratio: 128
    OFS0 register settings: WDT: Window End Position:  0% (no window end position)
    OFS0 register settings: WDT: Window Start Position: 100% (no window start position)
    OFS0 register settings: WDT: Reset Interrupt Request: Reset
    OFS0 register settings: WDT: Stop Control: Stop counting when entering Sleep mode
    OFS1 register settings: Voltage Detection 0 Circuit Start: Voltage monitor 0 reset is disabled after reset
    OFS1 register settings: Voltage Detection 0 Level: 2.80 V
    OFS1 register settings: HOCO Oscillation Enable: HOCO oscillation is disabled after reset
    Block Protection Settings (BPS): BPS0: 
    Permanent Block Protection Settings (PBPS): PBPS0: 
    Clocks: HOCO FLL Function: Disabled
    Main Oscillator Wait Time: 8163 cycles
    
  RA Common
    Main stack size (bytes): 0x1000
    Heap size (bytes): 0
    MCU Vcc (mV): 3300
    Parameter checking: Disabled
    Assert Failures: Return FSP_ERR_ASSERTION
    Error Log: No Error Log
    Clock Registers not Reset Values during Startup: Disabled
    Main Oscillator Populated: Populated
    PFS Protect: Enabled
    C Runtime Initialization : Enabled
    Early BSP Initialization : Disabled
    Main Oscillator Clock Source: Crystal or Resonator
    Subclock Populated: Populated
    Subclock Drive (Drive capacitance availability varies by MCU): Standard/Normal mode
    Subclock Stabilization Time (ms): 1000
    
  Clocks
    XTAL 24000000Hz
    HOCO 20MHz
    PLL Src: XTAL
    PLL Div /3
    PLL Mul x25.0
    PLL2 Src: XTAL
    PLL2 Div /2
    PLL2 Mul x20.0
    Clock Src: PLL
    CLKOUT Disabled
    UCLK Src: PLL2
    ICLK Div /2
    PCLKA Div /2
    PCLKB Div /4
    PCLKC Div /4
    PCLKD Div /2
    FCLK Div /4
    CLKOUT Div /1
    UCLK Div /5
    
  Pin Configurations
    R7FA4M2AC3CNE.pincfg -> g_bsp_pin_cfg
      AVCC0 42 ANALOG0_AVCC0 - - - - - - - - IO "Read only" - 
      AVSS0 43 ANALOG0_AVSS0 - - - - - - - - IO "Read only" - 
      P000 48 - - - - Disabled - - "ADC0: AN000; ICU0: IRQ06" - なし - - 
      P001 47 - - - - Disabled - - "ADC0: AN001; ICU0: IRQ07" - なし - - 
      P002 46 ADC0_AN002 - - - "Analog mode" - None "ADC0: AN002; ICU0: IRQ08" "MOTOR TEMP" IO - - 
      P013 40 - - - - Disabled - - "ADC0: AN011; ANALOG0: VREFL" - なし - - 
      P014 39 - - - - Disabled - - "ADC0: AN012; DAC0: DA0" - なし - - 
      P015 38 ADC0_AN013 - - - "Analog mode" - None "ADC0: AN013; DAC1: DA1; ICU0: IRQ13" "HVAMP TEMP" IO - - 
      P100 36 GPT5_GTIOC5B - Low None "Peripheral mode" CMOS None "AGT0: AGTIO0; GPT_POEG0: GTETRGA; GPT5: GTIOC5B; ICU0: IRQ02; QSPI0: QSPCLK; SCI0: RXD0; SCI0: SCL0; SCI1: SCK1" M_PWM IO - - 
      P101 35 GPIO - Low None "Output mode (Initial Low)" CMOS - "AGT0: AGTEE0; GPT_POEG1: GTETRGB; GPT5: GTIOC5A; ICU0: IRQ01; QSPI0: QIO1; SCI0: SDA0; SCI0: TXD0; SCI1: CTSRTS1" LED IO - - 
      P102 34 GPIO - Low - "Output mode (Initial High)" CMOS - "ADC0: ADTRG0; AGT0: AGTO0; CAN0: CRX0; GPT_OPS0: GTOWLO; GPT2: GTIOC2B; QSPI0: QIO0; SCI0: SCK0" M_DIR IO - - 
      P103 33 GPIO - Low - "Output mode (Initial High)" CMOS - "AGT2: AGTIO2; CAN0: CTX0; GPT_OPS0: GTOWUP; GPT2: GTIOC2A; QSPI0: QIO3; SCI0: CTSRTS0" M_EN IO - - 
      P104 32 - - - - Disabled - - "AGT2: AGTEE2; GPT_POEG1: GTETRGB; GPT1: GTIOC1B; ICU0: IRQ01; QSPI0: QIO2" - なし - - 
      P108 25 DEBUG0_SWDIO - Low - "Peripheral mode" CMOS None "AGT3: AGTOA3; DEBUG0: SWDIO; DEBUG0: TMS; GPT_OPS0: GTOULO; GPT0: GTIOC0B; SCI9: CTSRTS9; SPI0: SSLA0" SWDIO IO - - 
      P109 26 DEBUG0_TRACESWO - Low - "Peripheral mode" CMOS None "AGT3: AGTOB3; CGC0: CLKOUT; DEBUG0: TDO; DEBUG0: TRACESWO; GPT_OPS0: GTOVUP; GPT1: GTIOC1A; SCI9: SDA9; SCI9: TXD9; SPI0: MOSIA" SWO IO - - 
      P110 27 GPIO - Low None "Output mode (Initial High)" CMOS - "AGT3: AGTEE3; DEBUG0: TDI; GPT_OPS0: GTOVLO; GPT1: GTIOC1B; ICU0: IRQ03; SCI2: CTSRTS2; SCI9: RXD9; SCI9: SCL9; SPI0: MISOA" "TAD2141 CS" IO - - 
      P111 28 SCI2_SCK2 - Low None "Peripheral mode" CMOS None "AGT5: AGTOA5; GPT3: GTIOC3A; ICU0: IRQ04; SCI2: SCK2; SCI9: SCK9; SPI0: RSPCKA" "TAD2141 CLK" IO - - 
      P112 29 - - - - Disabled - - "AGT5: AGTOB5; GPT3: GTIOC3B; QSPI0: QSSL; SCI1: SCK1; SCI2: SDA2; SCI2: TXD2; SPI0: SSLA0; SSI0: SSIBCK0" - なし - - 
      P200 21 - - - - Disabled - - "ICU0: NMI" - なし - - 
      P201 20 - - - - Disabled - - "SYSTEM0: MD" - なし - - 
      P206 18 SCI4_RXD4 - Low None "Peripheral mode" CMOS None "CTSU0: TS02; GPT_OPS0: GTIU; ICU0: IRQ00; IIC1: SDA1; SCI4: RXD4; SCI4: SCL4; SCI9: CTS9; SDHI0: SD0DAT2; SPI0: SSLA1; SSI0: SSIDATA0; USB_FS0: USB_VBUSEN" "SERVO RX" IO - - 
      P207 17 SCI4_TXD4 - Low - "Peripheral mode" CMOS None "CTSU0: TSCAP; QSPI0: QSSL; SCI4: SDA4; SCI4: TXD4; SPI0: SSLA2" "SERVO TX" IO - - 
      P212 8 - - - - Disabled - - "AGT1: AGTEE1; CGC0: EXTAL; GPT_POEG3: GTETRGD; GPT0: GTIOC0B; ICU0: IRQ03; SCI1: RXD1; SCI1: SCL1" - なし - - 
      P213 7 - - - - Disabled - - "AGT2: AGTEE2; CGC0: XTAL; GPT_POEG2: GTETRGC; GPT0: GTIOC0A; ICU0: IRQ02; SCI1: SDA1; SCI1: TXD1" - なし - - 
      P300 24 DEBUG0_SWCLK - Low - "Peripheral mode" CMOS None "DEBUG0: SWCLK; DEBUG0: TCK; GPT_OPS0: GTOUUP; GPT0: GTIOC0A; SPI0: SSLA1" SWCLK IO - - 
      P301 23 SCI2_RXD2 - Low None "Peripheral mode" CMOS None "AGT0: AGTIO0; GPT_OPS0: GTOULO; GPT4: GTIOC4B; ICU0: IRQ06; SCI2: RXD2; SCI2: SCL2; SCI9: CTSRTS9; SPI0: SSLA2" "TAD2141 MISO" IO - - 
      P302 22 SCI2_TXD2 - Low None "Peripheral mode" CMOS None "GPT_OPS0: GTOUUP; GPT4: GTIOC4A; ICU0: IRQ05; SCI2: SDA2; SCI2: TXD2; SPI0: SSLA3" "TAD2141 MOSI" IO - - 
      P402 1 GPIO - Low None "Output mode (Initial High)" CMOS - "AGT0: AGTIO0; AGT1: AGTIO1; AGT2: AGTIO2; AGT3: AGTIO3; CAC0: CACREF; CAN0: CRX0; ICU0: IRQ04; RTC0: RTCIC0; SCI4: CTS4; SSI_COMMON0: AUDIO_CLK" ENC_EN IO - - 
      P407 12 GPIO - Low - "Output mode (Initial Low)" CMOS - "ADC0: ADTRG0; AGT0: AGTIO0; CTSU0: TS03; GPT6: GTIOC6A; IIC0: SDA0; RTC0: RTCOUT; SCI4: CTSRTS4; SPI0: SSLA3; USB_FS0: USB_VBUS" "SERVO DELAY SEL" IO - - 
      P408 11 SCI3_SCL3 - Medium None "Peripheral mode" "n-ch open drain" None "AGT2: AGTOB2; CTSU0: TS04; GPT_OPS0: GTOWLO; GPT6: GTIOC6B; ICU0: IRQ07; IIC0: SCL0; SCI3: RXD3; SCI3: SCL3; SCI4: CTS4; USB_FS0: USB_ID" - IO - - 
      P409 10 SCI3_SDA3 - Low None "Peripheral mode" "n-ch open drain" None "AGT2: AGTOA2; CTSU0: TS05; GPT_OPS0: GTOWUP; ICU0: IRQ06; SCI3: SDA3; SCI3: TXD3; USB_FS0: USB_EXICEN" - IO - - 
      P500 37 - - - - Disabled - - "ADC0: AN016; AGT0: AGTOA0; CAC0: CACREF; GPT_OPS0: GTIU; QSPI0: QSPCLK; USB_FS0: USB_VBUSEN" - なし - - 
      RES 19 SYSTEM0_RES - - - - - - - - IO "Read only" - 
      USBDM 14 USB_FS0_USB_DM - - - - - - - - IO "Read only" - 
      USBDP 15 USB_FS0_USB_DP - - - - - - - - IO "Read only" - 
      VBATT 2 SYSTEM0_VBATT - - - - - - - - IO "Read only" - 
      VCC 9 SYSTEM0_VCC - - - - - - - - IO "Read only" - 
      VCC 30 SYSTEM0_VCC - - - - - - - - IO "Read only" - 
      VCCUSB 16 USB_FS0_VCC_USB - - - - - - - - IO "Read only" - 
      VCL0 3 SYSTEM0_VCL0 - - - - - - - - IO "Read only" - 
      VREFH 41 ANALOG0_VREFH - - - - - - - - IO "Read only" - 
      VREFH0 45 ANALOG0_VREFH0 - - - - - - - - IO "Read only" - 
      VREFL0 44 ANALOG0_VREFL0 - - - - - - - - IO "Read only" - 
      VSS 6 SYSTEM0_VSS - - - - - - - - IO "Read only" - 
      VSS 31 SYSTEM0_VSS - - - - - - - - IO "Read only" - 
      VSSUSB 13 USB_FS0_VSS_USB - - - - - - - - IO "Read only" - 
      XCIN 4 CGC0_XCIN - - - - - - - - IO "Read only" - 
      XCOUT 5 CGC0_XCOUT - - - - - - - - IO "Read only" - 
    
  User Events
    
  User Event Links
    
  Module "I/O Port (r_ioport)"
    Parameter Checking: Default (BSP)
    
  Module "UART (r_sci_uart)"
    Parameter Checking: Default (BSP)
    FIFO Support: Enable
    DTC Support: Enable
    Flow Control Support: Disable
    RS-485 Support: Disable
    
  Module "I2C Master (r_sci_i2c)"
    Parameter Checking: Default (BSP)
    DTC on Transmission and Reception: Disabled
    10-bit slave addressing: Disabled
    
  Module "SPI (r_sci_spi)"
    Parameter Checking: Default (BSP)
    DTC Support: Enabled
    
  Module "Transfer (r_dtc)"
    Parameter Checking: Default (BSP)
    Linker section to keep DTC vector table: .fsp_dtc_vector_table
    
  Module "Timer, General PWM (r_gpt)"
    Parameter Checking: Default (BSP)
    Pin Output Support: Enabled
    Write Protect Enable: Disabled
    Clock Source: PCLKD
    
  Module "Timer, Low-Power (r_agt)"
    Parameter Checking: Default (BSP)
    Pin Output Support: Disabled
    Pin Input Support: Disabled
    
  Module "ADC (r_adc)"
    Parameter Checking: Default (BSP)
    
  Module "Flash (r_flash_hp)"
    Parameter Checking: Default (BSP)
    Code Flash Programming Enable: Disabled
    Data Flash Programming Enable: Enabled
    
  Module "CRC (r_crc)"
    Parameter Checking: Default (BSP)
    
  Module "Realtime Clock (r_rtc)"
    Parameter Checking: Default (BSP)
    Set Source Clock in Open: Disabled
    
  HAL
    Instance "g_ioport I/O Port (r_ioport)"
      Name: g_ioport
      1st Port ELC Trigger Source: Disabled
      2nd Port ELC Trigger Source: Disabled
      3rd Port ELC Trigger Source: Disabled
      4th Port ELC Trigger Source: Disabled
      Pin Configuration Name: g_bsp_pin_cfg
      
    Instance "g_uart4 UART (r_sci_uart)"
      General: Name: g_uart4
      General: Channel: 4
      General: Data Bits: 8bits
      General: Parity: None
      General: Stop Bits: 1bit
      Baud: Baud Rate: 2000000
      Baud: Baud Rate Modulation: Enabled
      Baud: Max Error (%): 3
      Flow Control: CTS/RTS Selection: Hardware RTS
      Flow Control: Software RTS Port: Disabled
      Flow Control: Software RTS Pin: Disabled
      Extra: Clock Source: Internal Clock
      Extra: Start bit detection: Falling Edge
      Extra: Noise Filter: Disable
      Extra: Receive FIFO Trigger Level: Max
      Extra: RS-485: DE Pin: Disable
      Extra: RS-485: DE Pin Polarity: Active High
      Extra: RS-485: DE Port Number: Disabled
      Extra: RS-485: DE Pin Number: Disabled
      Interrupts: Callback: user_uart_callback
      Interrupts: Receive Interrupt Priority: Priority 9
      Interrupts: Transmit Data Empty Interrupt Priority: Priority 9
      Interrupts: Transmit End Interrupt Priority: Priority 9
      Interrupts: Error Interrupt Priority: Priority 9
      
    Instance "g_i2c3 I2C Master (r_sci_i2c)"
      Name: g_i2c3
      Channel: 3
      Slave Address : 0x40
      Address Mode: 7-Bit
      Rate: Fast-mode
      SDA Output Delay (nano seconds): 300
      Noise filter setting: Use clock signal divided by 1 with noise filter
      Bit Rate Modulation: Enable
      Callback: sci_i2c_master_callback
      Interrupt Priority Level: Priority 11
      RX Interrupt Priority Level [Only used when DTC is enabled]: Disabled
      
    Instance "g_spi2 SPI (r_sci_spi)"
      Name: g_spi2
      Channel: 2
      Operating Mode: Master
      Clock Phase: Data sampling on odd edge, data variation on even edge
      Clock Polarity: Low when idle
      Mode Fault Error: Disable
      Bit Order: MSB First
      Callback: sci_spi_callback
      Receive Interrupt Priority: Priority 12
      Transmit Interrupt Priority: Priority 12
      Transmit End Interrupt Priority: Priority 12
      Error Interrupt Priority: Priority 12
      Bitrate: 10000000
      Bitrate Modulation: Enabled
      
      Instance "g_transfer0 Transfer (r_dtc) SCI2 TXI (Transmit data empty)"
        Name: g_transfer0
        Mode: Normal
        Transfer Size: 1 Byte
        Destination Address Mode: Fixed
        Source Address Mode: Incremented
        Repeat Area (Unused in Normal Mode): Source
        Destination Pointer: NULL
        Source Pointer: NULL
        Interrupt Frequency: After all transfers have completed
        Number of Transfers: 0
        Number of Blocks (Valid only in Block Mode): 0
        Number of Transfer Descriptors: 1
        Activation Source: SCI2 TXI (Transmit data empty)
        
      Instance "g_transfer1 Transfer (r_dtc) SCI2 RXI (Received data full)"
        Name: g_transfer1
        Mode: Normal
        Transfer Size: 1 Byte
        Destination Address Mode: Incremented
        Source Address Mode: Fixed
        Repeat Area (Unused in Normal Mode): Destination
        Destination Pointer: NULL
        Source Pointer: NULL
        Interrupt Frequency: After all transfers have completed
        Number of Transfers: 0
        Number of Blocks (Valid only in Block Mode): 0
        Number of Transfer Descriptors: 1
        Activation Source: SCI2 RXI (Received data full)
        
    Instance "g_timer5 Timer, General PWM (r_gpt)"
      General: Name: g_timer5
      General: Channel: 5
      General: Mode: PWM
      General: Period: 1000
      General: Period Unit: Raw Counts
      Output: Custom Waveform: GTIOA: Initial Output Level: Pin Level Low
      Output: Custom Waveform: GTIOA: Cycle End Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOA: Compare Match Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOA: Retain Output Level at Count Stop: Disabled
      Output: Custom Waveform: GTIOB: Initial Output Level: Pin Level Low
      Output: Custom Waveform: GTIOB: Cycle End Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOB: Compare Match Output Level: Pin Level Retain
      Output: Custom Waveform: GTIOB: Retain Output Level at Count Stop: Disabled
      Output: Custom Waveform: Custom Waveform Enable: Disabled
      Output: Duty Cycle Percent (only applicable in PWM mode): 50
      Output: GTIOCA Output Enabled: False
      Output: GTIOCA Stop Level: Pin Level Low
      Output: GTIOCB Output Enabled: True
      Output: GTIOCB Stop Level: Pin Level Low
      Input: Count Up Source: 
      Input: Count Down Source: 
      Input: Start Source: 
      Input: Stop Source: 
      Input: Clear Source: 
      Input: Capture A Source: 
      Input: Capture B Source: 
      Input: Noise Filter A Sampling Clock Select: No Filter
      Input: Noise Filter B Sampling Clock Select: No Filter
      Interrupts: Callback: NULL
      Interrupts: Overflow/Crest Interrupt Priority: Disabled
      Interrupts: Capture A Interrupt Priority: Disabled
      Interrupts: Capture B Interrupt Priority: Disabled
      Interrupts: Underflow/Trough Interrupt Priority: Disabled
      Extra Features: Extra Features: Disabled
      Extra Features: Output Disable: POEG Link: POEG Channel 0
      Extra Features: Output Disable: Output Disable POEG Trigger: 
      Extra Features: ADC Trigger: Start Event Trigger (Channels with GTINTAD only): 
      Extra Features: Dead Time (Value range varies with Channel): Dead Time Count Up (Raw Counts): 0
      Extra Features: Dead Time (Value range varies with Channel): Dead Time Count Down (Raw Counts) (Channels with GTDVD only): 0
      Extra Features: ADC Trigger (Channels with GTADTRA only): ADC A Compare Match (Raw Counts): 0
      Extra Features: ADC Trigger (Channels with GTADTRB only): ADC B Compare Match (Raw Counts): 0
      Extra Features: Interrupt Skipping (Channels with GTITC only): Interrupt to Count: None
      Extra Features: Interrupt Skipping (Channels with GTITC only): Interrupt Skip Count: 0
      Extra Features: Interrupt Skipping (Channels with GTITC only): Skip ADC Events: None
      Extra Features: Output Disable: GTIOCA Disable Setting: Disable Prohibited
      Extra Features: Output Disable: GTIOCB Disable Setting: Disable Prohibited
      
    Instance "g_timer0 Timer, Low-Power (r_agt)"
      General: Name: g_timer0
      General: Counter Bit Width: AGT 16-bit
      General: Channel: 0
      General: Mode: Periodic
      General: Period: 1
      General: Period Unit: Milliseconds
      Output: Duty Cycle Percent (only applicable in PWM mode): 50
      General: Count Source: PCLKB
      Output: AGTOA Output: Disabled
      Output: AGTOB Output: Disabled
      Output: AGTO Output: Disabled
      Input: Measurement Mode: Measure Disabled
      Input: Input Filter: No Filter
      Input: Enable Pin: Enable Pin Not Used
      Input: Trigger Edge: Trigger Edge Rising
      Interrupts: Callback: rgt0_callback
      Interrupts: Underflow Interrupt Priority: Priority 15
      
    Instance "g_adc0 ADC (r_adc)"
      General: Name: g_adc0
      General: Unit: 0
      General: Resolution: 12-Bit
      General: Alignment: Right
      General: Clear after read: On
      General: Mode: Continuous Scan
      General: Double-trigger: Disabled
      Input: Channel Scan Mask (channel availability varies by MCU): Channel 2, Channel 13, Temperature Sensor
      Input: Group B Scan Mask (channel availability varies by MCU): 
      Interrupts: Normal/Group A Trigger: Software
      Interrupts: Group B Trigger: Disabled
      Interrupts: Group Priority (Valid only in Group Scan Mode): Group A cannot interrupt Group B
      Input: Add/Average Count: Average four samples
      Input: Reference Voltage control: VREFH0/VREFH
      Input: Addition/Averaging Mask (channel availability varies by MCU and unit): Channel 3, Channel 15, Temperature Sensor
      Input: Sample and Hold: Sample and Hold Channels (Available only on selected MCUs): 
      Input: Sample and Hold: Sample Hold States (Applies only to channels 0, 1, 2): 24
      Input: Window Compare: Window Mode: Disabled
      Input: Window Compare: Event Output: OR
      Input: Window Compare: Window A: Enable: Disabled
      Input: Window Compare: Window A: Channels to compare (channel availability varies by MCU and unit): 
      Input: Window Compare: Window A: Channel comparison mode (channel availability varies by MCU and unit): 
      Input: Window Compare: Window A: Lower Reference: 0
      Input: Window Compare: Window A: Upper Reference: 0
      Input: Window Compare: Window B: Enable: Disabled
      Input: Window Compare: Window B: Channel to compare (channel availability varies by MCU and unit): Channel 0
      Input: Window Compare: Window B: Comparison mode: Less Than or Outside Window
      Input: Window Compare: Window B: Lower Reference: 0
      Input: Window Compare: Window B: Upper Reference: 0
      Interrupts: Callback: NULL
      Interrupts: Scan End Interrupt Priority: Disabled
      Interrupts: Scan End Group B Interrupt Priority: Disabled
      Interrupts: Window Compare A Interrupt Priority: Disabled
      Interrupts: Window Compare B Interrupt Priority: Disabled
      Extra: ADC Ring Buffer: Disabled
      
    Instance "g_flash0 Flash (r_flash_hp)"
      Name: g_flash0
      Data Flash Background Operation: Disabled
      Callback: NULL
      Flash Ready Interrupt Priority: Disabled
      Flash Error Interrupt Priority: Disabled
      
    Instance "g_crc0 CRC (r_crc)"
      Name: g_crc0
      CRC Polynomial: CRC-16
      Bit Order: MSB
      Snoop Address: Not Supported
      
    Instance "g_rtc0 Realtime Clock (r_rtc)"
      Name: g_rtc0
      Clock Source: LOCO
      Frequency Comparision Value (LOCO): 255
      Automatic Adjustment Mode: Enabled
      Automatic Adjustment Period: 10 Seconds
      Adjustment Type (Plus-Minus): NONE
      Error Adjustment Value: 0
      Callback: NULL
      Alarm Interrupt Priority: Disabled
      Period Interrupt Priority: Disabled
      Carry Interrupt Priority: Priority 12
      
