T2C60 000:002.162   SEGGER J-Link V7.86b Log File
T2C60 000:002.483   DLL Compiled: Mar  1 2023 16:53:12
T2C60 000:002.529   Logging started @ 2023-05-03 00:50
T2C60 000:002.573 - 2.595ms
T2C60 000:002.628 JLINK_GetDLLVersion()
T2C60 000:002.675 - 0.069ms returns 78602
T2C60 000:004.705 JLINK_OpenEx(...)
T2C60 000:023.025   Firmware: J-Link V11 compiled Mar 28 2023 16:59:55
T2C60 000:023.622   Firmware: J-Link V11 compiled Mar 28 2023 16:59:55
T2C60 000:028.003   Hardware: V11.00
T2C60 000:028.115   S/N: 851005873
T2C60 000:028.186   OEM: SEGGER
T2C60 000:028.261   Feature(s): RDI, FlashBP, FlashDL, JFlash, GDB
T2C60 000:032.114   USB speed mode: High speed (480 MBit/s)
T2C60 000:032.660   TELNET listener socket opened on port 19021
T2C60 000:033.173   WEBSRV WEBSRV_Init(): Starting webserver thread(s)
T2C60 000:033.759   WEBSRV Webserver running on local port 19080
T2C60 000:447.020 - 442.427ms returns "O.K."
T2C60 000:447.769 JLINK_ExecCommand("ProjectFile=C:\Users\T.Uemitsu\e2_studio\workspace\JP200_bootloader/JP200_bootloader.elf.jlink", ...). 
T2C60 000:549.070 - 101.335ms returns 0x00
T2C60 000:550.445 JLINK_ExecCommand("device=R7FA4M2AC", ...). 
T2C60 000:551.028   Flash bank @ 0x60000000: SFL: Parsing sectorization info from ELF file
T2C60 000:551.100     FlashDevice.SectorInfo[0]: .SectorSize = 0x00010000, .SectorStartAddr = 0x00000000
T2C60 000:551.170   OFL: Init() N/A
T2C60 000:551.258   OFL: UnInit() N/A
T2C60 000:551.323   OFL: EraseSector() N/A
T2C60 000:551.389   OFL: ProgramPage() N/A
T2C60 000:551.454   OFL: EraseChip() N/A
T2C60 000:551.553   OFL: BlankCheck() N/A
T2C60 000:551.619   OFL: Verify() N/A
T2C60 000:551.685   OFL: SEGGER_FL_Erase() present @ offset 0x000004DD
T2C60 000:551.750   OFL: SEGGER_FL_Program() present @ offset 0x000004C1
T2C60 000:551.816   OFL: SEGGER_FL_Read() N/A
T2C60 000:551.881   OFL: SEGGER_OPEN_Read() N/A
T2C60 000:551.946   OFL: SEGGER_FL_CalcCRC() present @ offset 0x00000505
T2C60 000:552.011   OFL: SEGGER_FL_Start() present @ offset 0x0000051D
T2C60 000:552.076   OFL: SEGGER_FL_GetFlashInfo() present @ offset 0x000001B9
T2C60 000:552.141   OFL: SEGGER_FL_Verify() N/A
T2C60 000:552.219   OFL: SEGGER_FL_CheckBlank() present @ offset 0x000004F1
T2C60 000:552.294   OFL: SEGGER_FL_Prepare() present @ offset 0x000001DD
T2C60 000:552.359   OFL: SEGGER_FL_Restore() present @ offset 0x0000038D
T2C60 000:552.424   OFL: SEGGER_FL_EraseChip() N/A
T2C60 000:556.794   Device "R7FA4M2AC" selected.
T2C60 000:558.788 - 8.285ms returns 0x00
T2C60 000:558.861 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 000:559.148   ConfigTargetSettings() start
T2C60 000:559.234    J-Link Script File: Executing ConfigTargetSettings()
T2C60 000:559.279   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 000:639.502   ConfigTargetSettings() end - Took 80ms
T2C60 000:640.661   InitTarget() start
T2C60 000:640.741    J-Link Script File: Executing InitTarget()
T2C60 000:640.787   JTAG selected. Identifying JTAG Chain...
T2C60 000:642.144   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 000:642.640   Error: Scanning JTAG chain failed.
T2C60 000:642.715   InitTarget() end - Took 1ms
T2C60 000:642.781   Connect failed. Resetting via Reset pin and trying again.
T2C60 000:703.601   ConfigTargetSettings() start
T2C60 000:703.714    J-Link Script File: Executing ConfigTargetSettings()
T2C60 000:703.759   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 000:777.496   ConfigTargetSettings() end - Took 73ms
T2C60 000:777.579   InitTarget() start
T2C60 000:777.644    J-Link Script File: Executing InitTarget()
T2C60 000:777.690   JTAG selected. Identifying JTAG Chain...
T2C60 000:779.209   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 000:779.788   Error: Scanning JTAG chain failed.
T2C60 000:779.864   InitTarget() end - Took 2ms
T2C60 000:779.929 - 221.089ms returns 1
T2C60 000:780.000 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T2C60 000:780.311   ConfigTargetSettings() start
T2C60 000:780.397    J-Link Script File: Executing ConfigTargetSettings()
T2C60 000:780.442   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 000:864.376   ConfigTargetSettings() end - Took 84ms
T2C60 000:864.477   InitTarget() start
T2C60 000:864.552    J-Link Script File: Executing InitTarget()
T2C60 000:864.598   JTAG selected. Identifying JTAG Chain...
T2C60 000:866.050   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 000:866.686   Error: Scanning JTAG chain failed.
T2C60 000:866.799   InitTarget() end - Took 2ms
T2C60 000:866.864   Connect failed. Resetting via Reset pin and trying again.
T2C60 000:929.083   ConfigTargetSettings() start
T2C60 000:929.208    J-Link Script File: Executing ConfigTargetSettings()
T2C60 000:929.253   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 001:008.605   ConfigTargetSettings() end - Took 79ms
T2C60 001:008.687   InitTarget() start
T2C60 001:008.753    J-Link Script File: Executing InitTarget()
T2C60 001:008.798   JTAG selected. Identifying JTAG Chain...
T2C60 001:010.135   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 001:010.728   Error: Scanning JTAG chain failed.
T2C60 001:010.840   InitTarget() end - Took 3ms
T2C60 001:010.909 - 230.935ms returns 1
T2C60 001:011.045 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 001:011.297   ConfigTargetSettings() start
T2C60 001:011.381    J-Link Script File: Executing ConfigTargetSettings()
T2C60 001:011.426   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 001:088.702   ConfigTargetSettings() end - Took 76ms
T2C60 001:088.836   InitTarget() start
T2C60 001:088.935    J-Link Script File: Executing InitTarget()
T2C60 001:089.064   JTAG selected. Identifying JTAG Chain...
T2C60 001:090.376   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 001:090.838   Error: Scanning JTAG chain failed.
T2C60 001:090.918   InitTarget() end - Took 3ms
T2C60 001:090.986   Connect failed. Resetting via Reset pin and trying again.
T2C60 001:152.651   ConfigTargetSettings() start
T2C60 001:152.780    J-Link Script File: Executing ConfigTargetSettings()
T2C60 001:152.826   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 001:238.941   ConfigTargetSettings() end - Took 86ms
T2C60 001:239.269   InitTarget() start
T2C60 001:239.363    J-Link Script File: Executing InitTarget()
T2C60 001:239.430   JTAG selected. Identifying JTAG Chain...
T2C60 001:240.717   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 001:241.213   Error: Scanning JTAG chain failed.
T2C60 001:241.316   InitTarget() end - Took 2ms
T2C60 001:241.406 - 230.392ms returns 1
T2C60 001:241.564 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 001:241.785   ConfigTargetSettings() start
T2C60 001:241.882    J-Link Script File: Executing ConfigTargetSettings()
T2C60 001:241.946   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 001:353.575   ConfigTargetSettings() end - Took 112ms
T2C60 001:353.677   InitTarget() start
T2C60 001:353.747    J-Link Script File: Executing InitTarget()
T2C60 001:353.794   JTAG selected. Identifying JTAG Chain...
T2C60 001:355.052   TotalIRLen = ?, IRPrint = 0x..000000000000000000000001
T2C60 001:355.497   Error: Scanning JTAG chain failed.
T2C60 001:355.580   InitTarget() end - Took 2ms
T2C60 001:355.656   Connect failed. Resetting via Reset pin and trying again.
T2C60 001:417.326   ConfigTargetSettings() start
T2C60 001:417.453    J-Link Script File: Executing ConfigTargetSettings()
T2C60 001:417.510   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 001:497.908   ConfigTargetSettings() end - Took 80ms
T2C60 001:497.998   InitTarget() start
T2C60 001:498.067    J-Link Script File: Executing InitTarget()
T2C60 001:498.115   JTAG selected. Identifying JTAG Chain...
T2C60 001:499.566   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 001:500.078   Error: Scanning JTAG chain failed.
T2C60 001:500.177   InitTarget() end - Took 2ms
T2C60 001:500.270 - 258.735ms returns 1
T2C60 001:500.398 JLINK_ReadMem(0x400E001C, 0x4 Bytes, ...)
T2C60 001:500.615   ConfigTargetSettings() start
T2C60 001:500.708    J-Link Script File: Executing ConfigTargetSettings()
T2C60 001:500.768   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 001:587.496   ConfigTargetSettings() end - Took 87ms
T2C60 001:587.577   InitTarget() start
T2C60 001:587.643    J-Link Script File: Executing InitTarget()
T2C60 001:587.688   JTAG selected. Identifying JTAG Chain...
T2C60 001:588.969   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 001:589.473   Error: Scanning JTAG chain failed.
T2C60 001:589.674   InitTarget() end - Took 1ms
T2C60 001:589.741   Connect failed. Resetting via Reset pin and trying again.
T2C60 001:651.423   ConfigTargetSettings() start
T2C60 001:651.545    J-Link Script File: Executing ConfigTargetSettings()
T2C60 001:651.590   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 001:727.833   ConfigTargetSettings() end - Took 76ms
T2C60 001:727.946   InitTarget() start
T2C60 001:728.032    J-Link Script File: Executing InitTarget()
T2C60 001:728.093   JTAG selected. Identifying JTAG Chain...
T2C60 001:729.329   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 001:729.831   Error: Scanning JTAG chain failed.
T2C60 001:729.927   InitTarget() end - Took 2ms
T2C60 001:730.016 - 229.647ms returns 1
T2C60 001:730.357 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 001:730.597   ConfigTargetSettings() start
T2C60 001:730.688    J-Link Script File: Executing ConfigTargetSettings()
T2C60 001:730.746   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 001:824.055   ConfigTargetSettings() end - Took 93ms
T2C60 001:824.135   InitTarget() start
T2C60 001:824.200    J-Link Script File: Executing InitTarget()
T2C60 001:824.245   JTAG selected. Identifying JTAG Chain...
T2C60 001:825.660   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 001:826.269   Error: Scanning JTAG chain failed.
T2C60 001:826.371   InitTarget() end - Took 3ms
T2C60 001:826.437   Connect failed. Resetting via Reset pin and trying again.
T2C60 001:887.825   ConfigTargetSettings() start
T2C60 001:887.950    J-Link Script File: Executing ConfigTargetSettings()
T2C60 001:888.000   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 001:963.515   ConfigTargetSettings() end - Took 75ms
T2C60 001:963.606   InitTarget() start
T2C60 001:963.671    J-Link Script File: Executing InitTarget()
T2C60 001:963.717   JTAG selected. Identifying JTAG Chain...
T2C60 001:965.120   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 001:965.704   Error: Scanning JTAG chain failed.
T2C60 001:965.781   InitTarget() end - Took 3ms
T2C60 001:965.847 - 235.512ms returns 1
T2C60 001:965.919 JLINK_ReadMem(0x400E0018, 0x4 Bytes, ...)
T2C60 001:966.258   ConfigTargetSettings() start
T2C60 001:966.333    J-Link Script File: Executing ConfigTargetSettings()
T2C60 001:966.377   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 002:040.557   ConfigTargetSettings() end - Took 73ms
T2C60 002:040.635   InitTarget() start
T2C60 002:040.701    J-Link Script File: Executing InitTarget()
T2C60 002:040.746   JTAG selected. Identifying JTAG Chain...
T2C60 002:042.242   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 002:042.914   Error: Scanning JTAG chain failed.
T2C60 002:043.031   InitTarget() end - Took 3ms
T2C60 002:043.097   Connect failed. Resetting via Reset pin and trying again.
T2C60 002:103.897   ConfigTargetSettings() start
T2C60 002:104.013    J-Link Script File: Executing ConfigTargetSettings()
T2C60 002:104.058   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 002:158.492   ConfigTargetSettings() end - Took 54ms
T2C60 002:158.577   InitTarget() start
T2C60 002:158.642    J-Link Script File: Executing InitTarget()
T2C60 002:158.689   JTAG selected. Identifying JTAG Chain...
T2C60 002:160.220   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 002:160.809   Error: Scanning JTAG chain failed.
T2C60 002:160.912   InitTarget() end - Took 3ms
T2C60 002:160.978 - 195.081ms returns 1
T2C60 002:161.137 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 002:161.456   ConfigTargetSettings() start
T2C60 002:161.530    J-Link Script File: Executing ConfigTargetSettings()
T2C60 002:161.574   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 002:211.244   ConfigTargetSettings() end - Took 49ms
T2C60 002:211.324   InitTarget() start
T2C60 002:211.389    J-Link Script File: Executing InitTarget()
T2C60 002:211.472   JTAG selected. Identifying JTAG Chain...
T2C60 002:213.077   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 002:213.687   Error: Scanning JTAG chain failed.
T2C60 002:213.792   InitTarget() end - Took 3ms
T2C60 002:213.858   Connect failed. Resetting via Reset pin and trying again.
T2C60 002:274.611   ConfigTargetSettings() start
T2C60 002:274.728    J-Link Script File: Executing ConfigTargetSettings()
T2C60 002:274.773   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 002:328.608   ConfigTargetSettings() end - Took 54ms
T2C60 002:328.688   InitTarget() start
T2C60 002:328.754    J-Link Script File: Executing InitTarget()
T2C60 002:328.800   JTAG selected. Identifying JTAG Chain...
T2C60 002:330.209   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 002:330.813   Error: Scanning JTAG chain failed.
T2C60 002:330.929   InitTarget() end - Took 2ms
T2C60 002:331.005 - 169.898ms returns 1
T2C60 002:331.084 JLINK_ReadMem(0x400E0020, 0x4 Bytes, ...)
T2C60 002:331.336   ConfigTargetSettings() start
T2C60 002:331.421    J-Link Script File: Executing ConfigTargetSettings()
T2C60 002:331.466   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 002:382.969   ConfigTargetSettings() end - Took 52ms
T2C60 002:383.047   InitTarget() start
T2C60 002:383.112    J-Link Script File: Executing InitTarget()
T2C60 002:383.157   JTAG selected. Identifying JTAG Chain...
T2C60 002:384.674   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 002:385.268   Error: Scanning JTAG chain failed.
T2C60 002:385.367   InitTarget() end - Took 3ms
T2C60 002:385.432   Connect failed. Resetting via Reset pin and trying again.
T2C60 002:447.012   ConfigTargetSettings() start
T2C60 002:447.127    J-Link Script File: Executing ConfigTargetSettings()
T2C60 002:447.183   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 002:497.427   ConfigTargetSettings() end - Took 50ms
T2C60 002:497.503   InitTarget() start
T2C60 002:497.568    J-Link Script File: Executing InitTarget()
T2C60 002:497.614   JTAG selected. Identifying JTAG Chain...
T2C60 002:498.945   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 002:499.523   Error: Scanning JTAG chain failed.
T2C60 002:499.610   InitTarget() end - Took 2ms
T2C60 002:499.675 - 168.612ms returns 1
T2C60 002:499.840 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 002:500.085   ConfigTargetSettings() start
T2C60 002:500.279    J-Link Script File: Executing ConfigTargetSettings()
T2C60 002:500.324   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 002:550.813   ConfigTargetSettings() end - Took 50ms
T2C60 002:551.039   InitTarget() start
T2C60 002:551.144    J-Link Script File: Executing InitTarget()
T2C60 002:551.196   JTAG selected. Identifying JTAG Chain...
T2C60 002:552.640   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 002:553.276   Error: Scanning JTAG chain failed.
T2C60 002:553.386   InitTarget() end - Took 3ms
T2C60 002:553.451   Connect failed. Resetting via Reset pin and trying again.
T2C60 002:615.740   ConfigTargetSettings() start
T2C60 002:615.850    J-Link Script File: Executing ConfigTargetSettings()
T2C60 002:615.896   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 002:667.970   ConfigTargetSettings() end - Took 52ms
T2C60 002:668.050   InitTarget() start
T2C60 002:668.115    J-Link Script File: Executing InitTarget()
T2C60 002:668.160   JTAG selected. Identifying JTAG Chain...
T2C60 002:669.527   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 002:670.121   Error: Scanning JTAG chain failed.
T2C60 002:670.237   InitTarget() end - Took 2ms
T2C60 002:670.302 - 170.483ms returns 1
T2C60 002:670.373 JLINK_ReadMem(0x400E0028, 0x4 Bytes, ...)
T2C60 002:670.720   ConfigTargetSettings() start
T2C60 002:670.794    J-Link Script File: Executing ConfigTargetSettings()
T2C60 002:670.839   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 002:721.122   ConfigTargetSettings() end - Took 50ms
T2C60 002:721.199   InitTarget() start
T2C60 002:721.264    J-Link Script File: Executing InitTarget()
T2C60 002:721.309   JTAG selected. Identifying JTAG Chain...
T2C60 002:722.617   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 002:723.114   Error: Scanning JTAG chain failed.
T2C60 002:723.207   InitTarget() end - Took 2ms
T2C60 002:723.298   Connect failed. Resetting via Reset pin and trying again.
T2C60 002:784.031   ConfigTargetSettings() start
T2C60 002:784.153    J-Link Script File: Executing ConfigTargetSettings()
T2C60 002:784.198   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 002:834.231   ConfigTargetSettings() end - Took 50ms
T2C60 002:834.330   InitTarget() start
T2C60 002:834.395    J-Link Script File: Executing InitTarget()
T2C60 002:834.441   JTAG selected. Identifying JTAG Chain...
T2C60 002:835.774   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 002:836.228   Error: Scanning JTAG chain failed.
T2C60 002:836.329   InitTarget() end - Took 2ms
T2C60 002:836.394 - 166.042ms returns 1
T2C60 002:836.514 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 002:836.710   ConfigTargetSettings() start
T2C60 002:836.782    J-Link Script File: Executing ConfigTargetSettings()
T2C60 002:836.828   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 002:886.854   ConfigTargetSettings() end - Took 50ms
T2C60 002:886.933   InitTarget() start
T2C60 002:886.998    J-Link Script File: Executing InitTarget()
T2C60 002:887.044   JTAG selected. Identifying JTAG Chain...
T2C60 002:888.452   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 002:888.926   Error: Scanning JTAG chain failed.
T2C60 002:889.007   InitTarget() end - Took 2ms
T2C60 002:889.072   Connect failed. Resetting via Reset pin and trying again.
T2C60 002:949.642   ConfigTargetSettings() start
T2C60 002:949.758    J-Link Script File: Executing ConfigTargetSettings()
T2C60 002:949.803   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 003:002.645   ConfigTargetSettings() end - Took 53ms
T2C60 003:002.742   InitTarget() start
T2C60 003:002.810    J-Link Script File: Executing InitTarget()
T2C60 003:002.857   JTAG selected. Identifying JTAG Chain...
T2C60 003:004.313   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 003:004.784   Error: Scanning JTAG chain failed.
T2C60 003:004.882   InitTarget() end - Took 2ms
T2C60 003:004.970 - 168.485ms returns 1
T2C60 003:005.044 JLINK_ReadMem(0x400E0024, 0x4 Bytes, ...)
T2C60 003:005.255   ConfigTargetSettings() start
T2C60 003:005.349    J-Link Script File: Executing ConfigTargetSettings()
T2C60 003:005.408   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 003:055.522   ConfigTargetSettings() end - Took 50ms
T2C60 003:055.628   InitTarget() start
T2C60 003:055.726    J-Link Script File: Executing InitTarget()
T2C60 003:055.783   JTAG selected. Identifying JTAG Chain...
T2C60 003:057.063   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 003:057.491   Error: Scanning JTAG chain failed.
T2C60 003:057.595   InitTarget() end - Took 2ms
T2C60 003:057.666   Connect failed. Resetting via Reset pin and trying again.
T2C60 003:119.424   ConfigTargetSettings() start
T2C60 003:119.555    J-Link Script File: Executing ConfigTargetSettings()
T2C60 003:119.606   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 003:170.924   ConfigTargetSettings() end - Took 51ms
T2C60 003:171.003   InitTarget() start
T2C60 003:171.068    J-Link Script File: Executing InitTarget()
T2C60 003:171.114   JTAG selected. Identifying JTAG Chain...
T2C60 003:172.510   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 003:172.972   Error: Scanning JTAG chain failed.
T2C60 003:173.108   InitTarget() end - Took 2ms
T2C60 003:173.204 - 168.188ms returns 1
T2C60 003:173.586 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 003:173.923   ConfigTargetSettings() start
T2C60 003:174.011    J-Link Script File: Executing ConfigTargetSettings()
T2C60 003:174.057   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 003:226.951   ConfigTargetSettings() end - Took 53ms
T2C60 003:227.034   InitTarget() start
T2C60 003:227.101    J-Link Script File: Executing InitTarget()
T2C60 003:227.148   JTAG selected. Identifying JTAG Chain...
T2C60 003:228.440   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 003:228.908   Error: Scanning JTAG chain failed.
T2C60 003:228.987   InitTarget() end - Took 2ms
T2C60 003:229.060   Connect failed. Resetting via Reset pin and trying again.
T2C60 003:289.760   ConfigTargetSettings() start
T2C60 003:289.888    J-Link Script File: Executing ConfigTargetSettings()
T2C60 003:289.944   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 003:344.103   ConfigTargetSettings() end - Took 54ms
T2C60 003:344.215   InitTarget() start
T2C60 003:344.295    J-Link Script File: Executing InitTarget()
T2C60 003:344.351   JTAG selected. Identifying JTAG Chain...
T2C60 003:345.686   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 003:346.153   Error: Scanning JTAG chain failed.
T2C60 003:346.246   InitTarget() end - Took 2ms
T2C60 003:346.312 - 172.748ms returns 1
T2C60 003:346.381 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T2C60 003:346.602   ConfigTargetSettings() start
T2C60 003:346.687    J-Link Script File: Executing ConfigTargetSettings()
T2C60 003:346.732   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 003:395.084   ConfigTargetSettings() end - Took 48ms
T2C60 003:395.163   InitTarget() start
T2C60 003:395.228    J-Link Script File: Executing InitTarget()
T2C60 003:395.275   JTAG selected. Identifying JTAG Chain...
T2C60 003:396.683   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 003:397.289   Error: Scanning JTAG chain failed.
T2C60 003:397.396   InitTarget() end - Took 2ms
T2C60 003:397.473   Connect failed. Resetting via Reset pin and trying again.
T2C60 003:459.719   ConfigTargetSettings() start
T2C60 003:459.841    J-Link Script File: Executing ConfigTargetSettings()
T2C60 003:459.887   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 003:510.557   ConfigTargetSettings() end - Took 50ms
T2C60 003:510.689   InitTarget() start
T2C60 003:510.776    J-Link Script File: Executing InitTarget()
T2C60 003:510.838   JTAG selected. Identifying JTAG Chain...
T2C60 003:512.195   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 003:512.710   Error: Scanning JTAG chain failed.
T2C60 003:512.838   InitTarget() end - Took 2ms
T2C60 003:512.947 - 166.598ms returns 1
T2C60 003:513.093 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 003:513.374   ConfigTargetSettings() start
T2C60 003:513.467    J-Link Script File: Executing ConfigTargetSettings()
T2C60 003:513.514   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 003:566.513   ConfigTargetSettings() end - Took 53ms
T2C60 003:566.610   InitTarget() start
T2C60 003:566.714    J-Link Script File: Executing InitTarget()
T2C60 003:566.760   JTAG selected. Identifying JTAG Chain...
T2C60 003:568.240   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 003:568.857   Error: Scanning JTAG chain failed.
T2C60 003:568.975   InitTarget() end - Took 2ms
T2C60 003:569.040   Connect failed. Resetting via Reset pin and trying again.
T2C60 003:629.863   ConfigTargetSettings() start
T2C60 003:629.978    J-Link Script File: Executing ConfigTargetSettings()
T2C60 003:630.023   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 003:680.962   ConfigTargetSettings() end - Took 51ms
T2C60 003:681.051   InitTarget() start
T2C60 003:681.127    J-Link Script File: Executing InitTarget()
T2C60 003:681.173   JTAG selected. Identifying JTAG Chain...
T2C60 003:682.555   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 003:683.106   Error: Scanning JTAG chain failed.
T2C60 003:683.207   InitTarget() end - Took 2ms
T2C60 003:683.272 - 170.200ms returns 1
T2C60 003:683.341 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T2C60 003:683.598   ConfigTargetSettings() start
T2C60 003:683.682    J-Link Script File: Executing ConfigTargetSettings()
T2C60 003:683.727   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 003:733.618   ConfigTargetSettings() end - Took 50ms
T2C60 003:733.700   InitTarget() start
T2C60 003:733.765    J-Link Script File: Executing InitTarget()
T2C60 003:733.811   JTAG selected. Identifying JTAG Chain...
T2C60 003:735.141   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 003:735.647   Error: Scanning JTAG chain failed.
T2C60 003:735.786   InitTarget() end - Took 2ms
T2C60 003:735.864   Connect failed. Resetting via Reset pin and trying again.
T2C60 003:798.076   ConfigTargetSettings() start
T2C60 003:798.206    J-Link Script File: Executing ConfigTargetSettings()
T2C60 003:798.254   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 003:848.080   ConfigTargetSettings() end - Took 50ms
T2C60 003:848.158   InitTarget() start
T2C60 003:848.223    J-Link Script File: Executing InitTarget()
T2C60 003:848.269   JTAG selected. Identifying JTAG Chain...
T2C60 003:849.764   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 003:850.413   Error: Scanning JTAG chain failed.
T2C60 003:850.525   InitTarget() end - Took 2ms
T2C60 003:850.590 - 167.270ms returns 1
T2C60 003:851.034 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 003:851.337   ConfigTargetSettings() start
T2C60 003:851.412    J-Link Script File: Executing ConfigTargetSettings()
T2C60 003:851.465   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 003:901.078   ConfigTargetSettings() end - Took 49ms
T2C60 003:901.156   InitTarget() start
T2C60 003:901.221    J-Link Script File: Executing InitTarget()
T2C60 003:901.267   JTAG selected. Identifying JTAG Chain...
T2C60 003:902.628   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 003:903.215   Error: Scanning JTAG chain failed.
T2C60 003:903.317   InitTarget() end - Took 2ms
T2C60 003:903.382   Connect failed. Resetting via Reset pin and trying again.
T2C60 003:964.897   ConfigTargetSettings() start
T2C60 003:965.019    J-Link Script File: Executing ConfigTargetSettings()
T2C60 003:965.064   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 004:015.917   ConfigTargetSettings() end - Took 51ms
T2C60 004:016.000   InitTarget() start
T2C60 004:016.067    J-Link Script File: Executing InitTarget()
T2C60 004:016.114   JTAG selected. Identifying JTAG Chain...
T2C60 004:017.608   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 004:018.185   Error: Scanning JTAG chain failed.
T2C60 004:018.291   InitTarget() end - Took 2ms
T2C60 004:018.356 - 167.344ms returns 1
T2C60 004:018.426 JLINK_ReadMem(0x400E001C, 0x4 Bytes, ...)
T2C60 004:018.727   ConfigTargetSettings() start
T2C60 004:018.813    J-Link Script File: Executing ConfigTargetSettings()
T2C60 004:018.858   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 004:070.892   ConfigTargetSettings() end - Took 52ms
T2C60 004:070.971   InitTarget() start
T2C60 004:071.036    J-Link Script File: Executing InitTarget()
T2C60 004:071.082   JTAG selected. Identifying JTAG Chain...
T2C60 004:072.550   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 004:073.075   Error: Scanning JTAG chain failed.
T2C60 004:073.167   InitTarget() end - Took 3ms
T2C60 004:073.276   Connect failed. Resetting via Reset pin and trying again.
T2C60 004:134.111   ConfigTargetSettings() start
T2C60 004:134.227    J-Link Script File: Executing ConfigTargetSettings()
T2C60 004:134.275   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 004:184.538   ConfigTargetSettings() end - Took 50ms
T2C60 004:184.616   InitTarget() start
T2C60 004:184.681    J-Link Script File: Executing InitTarget()
T2C60 004:184.726   JTAG selected. Identifying JTAG Chain...
T2C60 004:186.192   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 004:186.766   Error: Scanning JTAG chain failed.
T2C60 004:186.876   InitTarget() end - Took 3ms
T2C60 004:186.941 - 168.537ms returns 1
T2C60 004:187.021 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 004:187.306   ConfigTargetSettings() start
T2C60 004:187.427    J-Link Script File: Executing ConfigTargetSettings()
T2C60 004:187.472   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 004:250.217   ConfigTargetSettings() end - Took 62ms
T2C60 004:250.327   InitTarget() start
T2C60 004:250.416    J-Link Script File: Executing InitTarget()
T2C60 004:250.482   JTAG selected. Identifying JTAG Chain...
T2C60 004:251.794   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 004:252.311   Error: Scanning JTAG chain failed.
T2C60 004:252.407   InitTarget() end - Took 2ms
T2C60 004:252.497   Connect failed. Resetting via Reset pin and trying again.
T2C60 004:314.263   ConfigTargetSettings() start
T2C60 004:314.388    J-Link Script File: Executing ConfigTargetSettings()
T2C60 004:314.432   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 004:367.686   ConfigTargetSettings() end - Took 52ms
T2C60 004:367.774   InitTarget() start
T2C60 004:367.945    J-Link Script File: Executing InitTarget()
T2C60 004:367.994   JTAG selected. Identifying JTAG Chain...
T2C60 004:369.312   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 004:369.788   Error: Scanning JTAG chain failed.
T2C60 004:369.871   InitTarget() end - Took 2ms
T2C60 004:369.939 - 182.941ms returns 1
T2C60 004:370.063 JLINK_ReadMem(0x400E0018, 0x4 Bytes, ...)
T2C60 004:370.310   ConfigTargetSettings() start
T2C60 004:370.390    J-Link Script File: Executing ConfigTargetSettings()
T2C60 004:370.436   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 004:421.336   ConfigTargetSettings() end - Took 51ms
T2C60 004:421.414   InitTarget() start
T2C60 004:421.479    J-Link Script File: Executing InitTarget()
T2C60 004:421.525   JTAG selected. Identifying JTAG Chain...
T2C60 004:423.030   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 004:423.671   Error: Scanning JTAG chain failed.
T2C60 004:423.759   InitTarget() end - Took 3ms
T2C60 004:423.824   Connect failed. Resetting via Reset pin and trying again.
T2C60 004:484.451   ConfigTargetSettings() start
T2C60 004:484.577    J-Link Script File: Executing ConfigTargetSettings()
T2C60 004:484.621   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 004:534.840   ConfigTargetSettings() end - Took 50ms
T2C60 004:534.929   InitTarget() start
T2C60 004:534.994    J-Link Script File: Executing InitTarget()
T2C60 004:535.040   JTAG selected. Identifying JTAG Chain...
T2C60 004:536.453   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 004:537.058   Error: Scanning JTAG chain failed.
T2C60 004:537.134   InitTarget() end - Took 2ms
T2C60 004:537.200 - 167.158ms returns 1
T2C60 004:537.282 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 004:537.540   ConfigTargetSettings() start
T2C60 004:537.624    J-Link Script File: Executing ConfigTargetSettings()
T2C60 004:537.669   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 004:587.281   ConfigTargetSettings() end - Took 49ms
T2C60 004:587.360   InitTarget() start
T2C60 004:587.426    J-Link Script File: Executing InitTarget()
T2C60 004:587.483   JTAG selected. Identifying JTAG Chain...
T2C60 004:589.005   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 004:589.592   Error: Scanning JTAG chain failed.
T2C60 004:589.698   InitTarget() end - Took 3ms
T2C60 004:589.773   Connect failed. Resetting via Reset pin and trying again.
T2C60 004:651.921   ConfigTargetSettings() start
T2C60 004:652.050    J-Link Script File: Executing ConfigTargetSettings()
T2C60 004:652.096   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 004:703.624   ConfigTargetSettings() end - Took 51ms
T2C60 004:703.715   InitTarget() start
T2C60 004:703.781    J-Link Script File: Executing InitTarget()
T2C60 004:703.827   JTAG selected. Identifying JTAG Chain...
T2C60 004:705.447   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 004:706.039   Error: Scanning JTAG chain failed.
T2C60 004:706.136   InitTarget() end - Took 3ms
T2C60 004:706.201 - 168.941ms returns 1
T2C60 004:706.270 JLINK_ReadMem(0x400E0020, 0x4 Bytes, ...)
T2C60 004:706.555   ConfigTargetSettings() start
T2C60 004:706.729    J-Link Script File: Executing ConfigTargetSettings()
T2C60 004:706.883   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 004:758.963   ConfigTargetSettings() end - Took 52ms
T2C60 004:759.058   InitTarget() start
T2C60 004:759.146    J-Link Script File: Executing InitTarget()
T2C60 004:759.194   JTAG selected. Identifying JTAG Chain...
T2C60 004:760.426   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 004:760.938   Error: Scanning JTAG chain failed.
T2C60 004:761.035   InitTarget() end - Took 2ms
T2C60 004:761.102   Connect failed. Resetting via Reset pin and trying again.
T2C60 004:823.404   ConfigTargetSettings() start
T2C60 004:823.560    J-Link Script File: Executing ConfigTargetSettings()
T2C60 004:823.618   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 004:872.994   ConfigTargetSettings() end - Took 49ms
T2C60 004:873.072   InitTarget() start
T2C60 004:873.137    J-Link Script File: Executing InitTarget()
T2C60 004:873.183   JTAG selected. Identifying JTAG Chain...
T2C60 004:874.620   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 004:875.215   Error: Scanning JTAG chain failed.
T2C60 004:875.322   InitTarget() end - Took 2ms
T2C60 004:875.399 - 169.150ms returns 1
T2C60 004:875.860 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 004:876.226   ConfigTargetSettings() start
T2C60 004:876.300    J-Link Script File: Executing ConfigTargetSettings()
T2C60 004:876.355   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 004:926.184   ConfigTargetSettings() end - Took 50ms
T2C60 004:926.265   InitTarget() start
T2C60 004:926.342    J-Link Script File: Executing InitTarget()
T2C60 004:926.397   JTAG selected. Identifying JTAG Chain...
T2C60 004:927.899   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 004:928.470   Error: Scanning JTAG chain failed.
T2C60 004:928.547   InitTarget() end - Took 3ms
T2C60 004:928.612   Connect failed. Resetting via Reset pin and trying again.
T2C60 004:990.398   ConfigTargetSettings() start
T2C60 004:990.538    J-Link Script File: Executing ConfigTargetSettings()
T2C60 004:990.586   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 005:042.133   ConfigTargetSettings() end - Took 51ms
T2C60 005:042.231   InitTarget() start
T2C60 005:042.299    J-Link Script File: Executing InitTarget()
T2C60 005:042.349   JTAG selected. Identifying JTAG Chain...
T2C60 005:043.677   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 005:044.125   Error: Scanning JTAG chain failed.
T2C60 005:044.219   InitTarget() end - Took 2ms
T2C60 005:044.286 - 168.448ms returns 1
T2C60 005:044.463 JLINK_ReadMem(0x400E0028, 0x4 Bytes, ...)
T2C60 005:044.709   ConfigTargetSettings() start
T2C60 005:044.792    J-Link Script File: Executing ConfigTargetSettings()
T2C60 005:044.846   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 005:101.332   ConfigTargetSettings() end - Took 57ms
T2C60 005:101.415   InitTarget() start
T2C60 005:101.481    J-Link Script File: Executing InitTarget()
T2C60 005:101.526   JTAG selected. Identifying JTAG Chain...
T2C60 005:102.819   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 005:103.412   Error: Scanning JTAG chain failed.
T2C60 005:103.506   InitTarget() end - Took 2ms
T2C60 005:103.571   Connect failed. Resetting via Reset pin and trying again.
T2C60 005:165.147   ConfigTargetSettings() start
T2C60 005:165.317    J-Link Script File: Executing ConfigTargetSettings()
T2C60 005:165.378   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 005:217.596   ConfigTargetSettings() end - Took 52ms
T2C60 005:217.675   InitTarget() start
T2C60 005:217.740    J-Link Script File: Executing InitTarget()
T2C60 005:217.787   JTAG selected. Identifying JTAG Chain...
T2C60 005:219.160   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 005:219.733   Error: Scanning JTAG chain failed.
T2C60 005:219.830   InitTarget() end - Took 3ms
T2C60 005:219.907 - 175.474ms returns 1
T2C60 005:219.995 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 005:220.275   ConfigTargetSettings() start
T2C60 005:220.361    J-Link Script File: Executing ConfigTargetSettings()
T2C60 005:220.412   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 005:273.516   ConfigTargetSettings() end - Took 53ms
T2C60 005:273.665   InitTarget() start
T2C60 005:273.781    J-Link Script File: Executing InitTarget()
T2C60 005:273.856   JTAG selected. Identifying JTAG Chain...
T2C60 005:275.481   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 005:276.003   Error: Scanning JTAG chain failed.
T2C60 005:276.410   InitTarget() end - Took 3ms
T2C60 005:276.501   Connect failed. Resetting via Reset pin and trying again.
T2C60 005:337.199   ConfigTargetSettings() start
T2C60 005:337.319    J-Link Script File: Executing ConfigTargetSettings()
T2C60 005:337.364   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 005:391.139   ConfigTargetSettings() end - Took 53ms
T2C60 005:391.224   InitTarget() start
T2C60 005:391.291    J-Link Script File: Executing InitTarget()
T2C60 005:391.338   JTAG selected. Identifying JTAG Chain...
T2C60 005:392.627   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 005:393.157   Error: Scanning JTAG chain failed.
T2C60 005:393.232   InitTarget() end - Took 2ms
T2C60 005:393.298 - 173.324ms returns 1
T2C60 005:393.368 JLINK_ReadMem(0x400E0024, 0x4 Bytes, ...)
T2C60 005:393.642   ConfigTargetSettings() start
T2C60 005:393.731    J-Link Script File: Executing ConfigTargetSettings()
T2C60 005:393.776   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 005:442.396   ConfigTargetSettings() end - Took 48ms
T2C60 005:442.474   InitTarget() start
T2C60 005:442.538    J-Link Script File: Executing InitTarget()
T2C60 005:442.605   JTAG selected. Identifying JTAG Chain...
T2C60 005:443.995   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 005:444.588   Error: Scanning JTAG chain failed.
T2C60 005:444.701   InitTarget() end - Took 3ms
T2C60 005:444.766   Connect failed. Resetting via Reset pin and trying again.
T2C60 005:506.067   ConfigTargetSettings() start
T2C60 005:506.182    J-Link Script File: Executing ConfigTargetSettings()
T2C60 005:506.227   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 005:557.189   ConfigTargetSettings() end - Took 51ms
T2C60 005:557.292   InitTarget() start
T2C60 005:557.378    J-Link Script File: Executing InitTarget()
T2C60 005:557.481   JTAG selected. Identifying JTAG Chain...
T2C60 005:558.850   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 005:559.392   Error: Scanning JTAG chain failed.
T2C60 005:559.557   InitTarget() end - Took 3ms
T2C60 005:559.644 - 166.304ms returns 1
T2C60 005:559.968 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 005:560.240   ConfigTargetSettings() start
T2C60 005:560.317    J-Link Script File: Executing ConfigTargetSettings()
T2C60 005:560.362   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 005:610.696   ConfigTargetSettings() end - Took 50ms
T2C60 005:610.774   InitTarget() start
T2C60 005:610.839    J-Link Script File: Executing InitTarget()
T2C60 005:610.885   JTAG selected. Identifying JTAG Chain...
T2C60 005:612.379   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 005:612.974   Error: Scanning JTAG chain failed.
T2C60 005:613.087   InitTarget() end - Took 2ms
T2C60 005:613.152   Connect failed. Resetting via Reset pin and trying again.
T2C60 005:673.928   ConfigTargetSettings() start
T2C60 005:674.053    J-Link Script File: Executing ConfigTargetSettings()
T2C60 005:674.098   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 005:727.590   ConfigTargetSettings() end - Took 53ms
T2C60 005:727.691   InitTarget() start
T2C60 005:727.776    J-Link Script File: Executing InitTarget()
T2C60 005:727.840   JTAG selected. Identifying JTAG Chain...
T2C60 005:729.175   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 005:729.658   Error: Scanning JTAG chain failed.
T2C60 005:729.744   InitTarget() end - Took 2ms
T2C60 005:729.812 - 169.866ms returns 1
T2C60 005:729.873 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T2C60 005:730.125   ConfigTargetSettings() start
T2C60 005:730.217    J-Link Script File: Executing ConfigTargetSettings()
T2C60 005:730.264   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 005:784.870   ConfigTargetSettings() end - Took 55ms
T2C60 005:784.949   InitTarget() start
T2C60 005:785.014    J-Link Script File: Executing InitTarget()
T2C60 005:785.059   JTAG selected. Identifying JTAG Chain...
T2C60 005:786.493   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 005:787.110   Error: Scanning JTAG chain failed.
T2C60 005:787.225   InitTarget() end - Took 2ms
T2C60 005:787.289   Connect failed. Resetting via Reset pin and trying again.
T2C60 005:849.050   ConfigTargetSettings() start
T2C60 005:849.157    J-Link Script File: Executing ConfigTargetSettings()
T2C60 005:849.202   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 005:898.544   ConfigTargetSettings() end - Took 49ms
T2C60 005:898.622   InitTarget() start
T2C60 005:898.688    J-Link Script File: Executing InitTarget()
T2C60 005:898.733   JTAG selected. Identifying JTAG Chain...
T2C60 005:900.375   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T2C60 005:900.945   Error: Scanning JTAG chain failed.
T2C60 005:901.053   InitTarget() end - Took 3ms
T2C60 005:901.117 - 171.265ms returns 1
T2C60 005:901.491 JLINK_TIF_GetAvailable(...)
T2C60 005:901.734 - 0.283ms
T2C60 005:901.801 JLINK_TIF_Select(JLINKARM_TIF_SWD)
T2C60 005:903.412 - 1.644ms returns 0x00
T2C60 005:903.474 JLINK_SetSpeed(4000)
T2C60 005:903.734 - 0.298ms
T2C60 005:903.800 JLINK_SetEndian(ARM_ENDIAN_LITTLE)
T2C60 005:903.845 - 0.066ms returns 0
T2C60 005:903.901 JLINK_SetInitRegsOnReset(OFF)
T2C60 005:903.956 - 0.076ms returns 1
T2C60 005:904.002 JLINK_SetResetType(JLINKARM_RESET_TYPE_NO_RESET)
T2C60 005:904.045 - 0.064ms returns JLINKARM_RESET_TYPE_NORMAL
T2C60 005:904.092 JLINK_ExecCommand("EnableFlashBPs", ...). 
T2C60 005:904.139 - 0.022ms returns 0x00
T2C60 005:904.186 JLINK_ExecCommand("SetAllowFlashCache = 1", ...). 
T2C60 005:904.234 - 0.023ms returns 0x01
T2C60 005:904.280 JLINK_ExecCommand("SetRestartOnClose = 0", ...). 
T2C60 005:904.328 - 0.023ms returns 0x01
T2C60 005:904.374 JLINK_EnableSoftBPs(ON)
T2C60 005:904.417 - 0.064ms
T2C60 005:904.462 JLINK_Connect()
T2C60 005:904.769   ConfigTargetSettings() start
T2C60 005:904.843    J-Link Script File: Executing ConfigTargetSettings()
T2C60 005:904.899   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T2C60 005:954.339   ConfigTargetSettings() end - Took 50ms
T2C60 005:954.420   InitTarget() start
T2C60 005:954.486    J-Link Script File: Executing InitTarget()
T2C60 005:954.532   SWD selected. Executing JTAG -> SWD switching sequence.
T2C60 005:956.293   DAP initialized successfully.
T2C60 005:956.385   Determining TrustZone configuration...
T2C60 005:957.363     Secure Debug: Enabled (SSD)
T2C60 005:957.437   Determining currently configured transfer type by reading the AHB-AP CSW register.
T2C60 005:958.124     --> Correct transfer type configured. Done.
T2C60 005:958.197   InitTarget() end - Took 4ms
T2C60 005:958.650   Found SW-DP with ID 0x6BA02477
T2C60 005:960.234   DPIDR: 0x6BA02477
T2C60 005:960.305   CoreSight SoC-400 or earlier
T2C60 005:960.372   Scanning AP map to find all available APs
T2C60 005:961.015   AP[2]: Stopped AP scan as end of AP map has been reached
T2C60 005:961.086   AP[0]: AHB-AP (IDR: 0x84770001)
T2C60 005:961.153   AP[1]: APB-AP (IDR: 0x54770002)
T2C60 005:961.227   Iterating through AP map to find AHB-AP to use
T2C60 005:961.704   AP[0]: Core found
T2C60 005:961.775   AP[0]: AHB-AP ROM base: 0xE00FE000
T2C60 005:962.074   CPUID register: 0x410FD214. Implementer code: 0x41 (ARM)
T2C60 005:962.146   Feature set: Mainline
T2C60 005:962.431   Cache: No cache
T2C60 005:962.482   Found Cortex-M33 r0p4, Little endian.
T2C60 005:962.822   -- Max. mem block: 0x00004E50
T2C60 005:963.482   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T2C60 005:963.803   CPU_WriteMem(4 bytes @ 0xE000EDF0)
T2C60 005:964.101   CPU_ReadMem(4 bytes @ 0xE0002000)
T2C60 005:964.386   FPUnit: 8 code (BP) slots and 0 literal slots
T2C60 005:964.459   CPU_ReadMem(4 bytes @ 0xE000EDFC)
T2C60 005:964.750   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T2C60 005:965.051   CPU_ReadMem(4 bytes @ 0xE0001000)
T2C60 005:965.337   CPU_ReadMem(4 bytes @ 0xE0001000)
T2C60 005:965.652   CPU_ReadMem(4 bytes @ 0xE0001028)
T2C60 005:965.964   CPU_ReadMem(4 bytes @ 0xE0001038)
T2C60 005:966.254   CPU_ReadMem(4 bytes @ 0xE0001048)
T2C60 005:966.581   CPU_ReadMem(4 bytes @ 0xE0001058)
T2C60 005:966.867   CPU_WriteMem(4 bytes @ 0xE0001000)
T2C60 005:967.236   CPU_ReadMem(4 bytes @ 0xE000ED88)
T2C60 005:967.532   CPU_WriteMem(4 bytes @ 0xE000ED88)
T2C60 005:967.872   CPU_ReadMem(4 bytes @ 0xE000ED88)
T2C60 005:968.162   CPU_WriteMem(4 bytes @ 0xE000ED88)
T2C60 005:968.454   CPU_ReadMem(4 bytes @ 0xE000EFB8)
T2C60 005:968.752   Security extension: implemented
T2C60 005:968.824   Secure debug: enabled
T2C60 005:968.889   CoreSight components:
T2C60 005:968.955   ROMTbl[0] @ E00FE000
T2C60 005:969.021   CPU_ReadMem(64 bytes @ 0xE00FE000)
T2C60 005:969.506   CPU_ReadMem(32 bytes @ 0xE0044FE0)
T2C60 005:969.903   CPU_ReadMem(4 bytes @ 0xE0044FBC)
T2C60 005:970.205   CPU_ReadMem(4 bytes @ 0xE0044FCC)
T2C60 005:970.502   [0][0]: E0044000 CID B105900D PID 005BB906 DEVARCH 00000000 DEVTYPE 14 CTI (?)
T2C60 005:970.575   CPU_ReadMem(32 bytes @ 0xE0047FE0)
T2C60 005:970.963   CPU_ReadMem(4 bytes @ 0xE0047FBC)
T2C60 005:971.252   CPU_ReadMem(4 bytes @ 0xE0047FCC)
T2C60 005:971.555   [0][1]: E0047000 CID B105900D PID 003BB908 DEVARCH 00000000 DEVTYPE 12 CSTF
T2C60 005:971.627   CPU_ReadMem(32 bytes @ 0xE0048FE0)
T2C60 005:972.015   CPU_ReadMem(4 bytes @ 0xE0048FBC)
T2C60 005:972.307   CPU_ReadMem(4 bytes @ 0xE0048FCC)
T2C60 005:972.602   [0][2]: E0048000 CID B105900D PID 001BB961 DEVARCH 00000000 DEVTYPE 21 ETB
T2C60 005:972.674   CPU_ReadMem(32 bytes @ 0xE0049FE0)
T2C60 005:973.056   [0][3]: E0049000 CID B105F00D PID 001BB101 TSG
T2C60 005:973.128   CPU_ReadMem(32 bytes @ 0xE0040FE0)
T2C60 005:973.502   CPU_ReadMem(4 bytes @ 0xE0040FBC)
T2C60 005:973.805   CPU_ReadMem(4 bytes @ 0xE0040FCC)
T2C60 005:974.109   [0][4]: E0040000 CID B105900D PID 000BBD21 DEVARCH 00000000 DEVTYPE 11 TPIU
T2C60 005:974.182   CPU_ReadMem(32 bytes @ 0xE00FFFE0)
T2C60 005:974.556   [0][5]: E00FF000 CID B105100D PID 000BB4C9 ROM Table
T2C60 005:974.627   ROMTbl[1] @ E00FF000
T2C60 005:974.695   CPU_ReadMem(64 bytes @ 0xE00FF000)
T2C60 005:975.197   CPU_ReadMem(32 bytes @ 0xE000EFE0)
T2C60 005:975.588   CPU_ReadMem(4 bytes @ 0xE000EFBC)
T2C60 005:975.882   CPU_ReadMem(4 bytes @ 0xE000EFCC)
T2C60 005:976.310   [1][0]: E000E000 CID B105900D PID 000BBD21 DEVARCH 47702A04 DEVTYPE 00 Cortex-M33
T2C60 005:976.383   CPU_ReadMem(32 bytes @ 0xE0001FE0)
T2C60 005:976.785   CPU_ReadMem(4 bytes @ 0xE0001FBC)
T2C60 005:977.100   CPU_ReadMem(4 bytes @ 0xE0001FCC)
T2C60 005:977.430   [1][1]: E0001000 CID B105900D PID 000BBD21 DEVARCH 47701A02 DEVTYPE 00 DWT
T2C60 005:977.503   CPU_ReadMem(32 bytes @ 0xE0002FE0)
T2C60 005:978.053   CPU_ReadMem(4 bytes @ 0xE0002FBC)
T2C60 005:978.325   CPU_ReadMem(4 bytes @ 0xE0002FCC)
T2C60 005:978.677   [1][2]: E0002000 CID B105900D PID 000BBD21 DEVARCH 47701A03 DEVTYPE 00 FPB
T2C60 005:978.750   CPU_ReadMem(32 bytes @ 0xE0000FE0)
T2C60 005:979.299   CPU_ReadMem(4 bytes @ 0xE0000FBC)
T2C60 005:979.605   CPU_ReadMem(4 bytes @ 0xE0000FCC)
T2C60 005:979.927   [1][3]: E0000000 CID B105900D PID 000BBD21 DEVARCH 47701A01 DEVTYPE 43 ITM
T2C60 005:980.007   CPU_ReadMem(32 bytes @ 0xE0041FE0)
T2C60 005:980.514   CPU_ReadMem(4 bytes @ 0xE0041FBC)
T2C60 005:980.847   CPU_ReadMem(4 bytes @ 0xE0041FCC)
T2C60 005:981.184   [1][5]: E0041000 CID B105900D PID 002BBD21 DEVARCH 47724A13 DEVTYPE 13 ETM
T2C60 005:981.257   CPU_ReadMem(32 bytes @ 0xE0042FE0)
T2C60 005:981.658   CPU_ReadMem(4 bytes @ 0xE0042FBC)
T2C60 005:982.052   CPU_ReadMem(4 bytes @ 0xE0042FCC)
T2C60 005:982.431   [1][6]: E0042000 CID B105900D PID 000BBD21 DEVARCH 47701A14 DEVTYPE 14 CSS600-CTI
T2C60 005:982.509 - 78.072ms returns 0x00
T2C60 005:982.572 JLINK_ResetPullsRESET(ON)
T2C60 005:982.618 - 0.068ms
T2C60 005:982.667 JLINK_Halt()
T2C60 005:985.232 - 2.592ms returns 0x00
T2C60 005:985.289 JLINK_IsHalted()
T2C60 005:985.554 - 0.292ms returns TRUE
T2C60 005:985.610 JLINK_Reset()
T2C60 005:985.670   CPU_WriteMem(4 bytes @ 0xE000EDF0)
T2C60 005:985.962   CPU_ReadMem(4 bytes @ 0xE000ED44)
T2C60 005:986.252   CPU_ReadMem(4 bytes @ 0xE000EE08)
T2C60 005:986.553   CPU_WriteMem(4 bytes @ 0xE000EE08)
T2C60 005:986.850   Reset: ARMv8M core with Security Extension enabled detected.
T2C60 005:986.923   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T2C60 005:987.205   Reset: Halt core after reset via DEMCR.VC_CORERESET.
T2C60 005:987.599   Reset: Reset device via AIRCR.SYSRESETREQ.
T2C60 005:987.672   CPU_WriteMem(4 bytes @ 0xE000ED0C)
T2C60 006:040.218   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T2C60 006:040.657   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T2C60 006:041.039   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T2C60 006:046.984   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T2C60 006:050.224   CPU_WriteMem(4 bytes @ 0xE0002000)
T2C60 006:050.614   CPU_ReadMem(4 bytes @ 0xE000EDFC)
T2C60 006:051.036   CPU_ReadMem(4 bytes @ 0xE0001000)
T2C60 006:051.429   CPU_ReadMem(4 bytes @ 0xE000EE08)
T2C60 006:051.788 - 66.205ms
T2C60 006:051.867 JLINK_SetEndian(ARM_ENDIAN_LITTLE)
T2C60 006:051.913 - 0.068ms returns 0
T2C60 006:052.010 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 006:052.065   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T2C60 006:052.367   Data:  03 00 13 00
T2C60 006:052.439   Debug reg: DHCSR
T2C60 006:052.505 - 0.518ms returns 0
T2C60 006:052.813 JLINK_ReadMem(0x010080F0, 0x10 Bytes, ...)
T2C60 006:052.924   CPU_ReadMem(16 bytes @ 0x010080F0)
T2C60 006:053.253   Data:  52 37 46 41 34 4D 32 41 43 33 43 4E 45 20 20 20
T2C60 006:053.330 - 0.539ms returns 0
T2C60 006:053.386 JLINK_IsHalted()
T2C60 006:053.433 - 0.069ms returns TRUE
T2C60 006:053.810 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 006:053.869   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T2C60 006:054.157   Data:  03 00 13 00
T2C60 006:054.230   Debug reg: DHCSR
T2C60 006:054.296 - 0.508ms returns 0
T2C60 006:054.346 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T2C60 006:054.399   CPU_ReadMem(4 bytes @ 0x400E002C)
T2C60 006:054.676   Data:  01 00 00 00
T2C60 006:054.748 - 0.424ms returns 0
T2C60 006:054.803 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T2C60 006:054.854   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T2C60 006:055.152   Data:  03 00 13 00
T2C60 006:055.223   Debug reg: DHCSR
T2C60 006:055.290 - 0.510ms returns 0
T2C60 006:055.341 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T2C60 006:055.392   CPU_ReadMem(4 bytes @ 0x400E002C)
T2C60 006:055.681   Data:  01 00 00 00
T2C60 006:055.753 - 0.435ms returns 0
T2C60 006:055.806 JLINK_MeasureCPUSpeed(RAMAddr = 0xFFFFFFFF)
T2C60 006:055.857   CPU_ReadMem(16 bytes @ 0x2000D000)
T2C60 006:056.215   CPU_ReadMem(64 bytes @ 0x2000D000)
T2C60 006:056.715    -- Updating C cache (64 bytes @ 0x2000D000)
T2C60 006:056.797    -- Read from C cache (6 bytes @ 0x2000D000)
T2C60 006:056.864   CPU_ReadMem(4 bytes @ 0xE000ED90)
T2C60 006:057.157   CPU_ReadMem(4 bytes @ 0xE000ED94)
T2C60 006:057.582   CPU_WriteMem(16 bytes @ 0x2000D000)
T2C60 006:058.006   CPU_WriteMem(6 bytes @ 0x2000D000)
T2C60 006:058.373   CPU_ReadMem(64 bytes @ 0x2000D000)
T2C60 006:059.047    -- Updating C cache (64 bytes @ 0x2000D000)
T2C60 006:059.120    -- Read from C cache (6 bytes @ 0x2000D000)
T2C60 006:059.199   CPU_ReadMem(4 bytes @ 0xE000EE08)
T2C60 006:059.505   CPU_WriteMem(4 bytes @ 0xE0002008)
T2C60 006:059.578   CPU_WriteMem(4 bytes @ 0xE000200C)
T2C60 006:059.646   CPU_WriteMem(4 bytes @ 0xE0002010)
T2C60 006:059.713   CPU_WriteMem(4 bytes @ 0xE0002014)
T2C60 006:059.781   CPU_WriteMem(4 bytes @ 0xE0002018)
T2C60 006:059.848   CPU_WriteMem(4 bytes @ 0xE000201C)
T2C60 006:059.915   CPU_WriteMem(4 bytes @ 0xE0002020)
T2C60 006:059.982   CPU_WriteMem(4 bytes @ 0xE0002024)
T2C60 006:061.157   CPU_WriteMem(4 bytes @ 0xE0001004)
T2C60 006:066.877   CPU_ReadMem(4 bytes @ 0xE0001004)
T2C60 006:067.273   CPU_ReadMem(4 bytes @ 0xE000EE08)
T2C60 006:067.627   CPU_WriteMem(4 bytes @ 0xE0002008)
T2C60 006:067.978   CPU_WriteMem(4 bytes @ 0xE000200C)
T2C60 006:068.292   CPU_WriteMem(4 bytes @ 0xE0002010)
T2C60 006:068.597   CPU_WriteMem(4 bytes @ 0xE0002014)
T2C60 006:068.919   CPU_WriteMem(4 bytes @ 0xE0002018)
T2C60 006:069.208   CPU_WriteMem(4 bytes @ 0xE000201C)
T2C60 006:069.502   CPU_WriteMem(4 bytes @ 0xE0002020)
T2C60 006:069.805   CPU_WriteMem(4 bytes @ 0xE0002024)
T2C60 006:070.101   CPU_ReadMem(4 bytes @ 0xE000EE08)
T2C60 006:070.377   CPU_ReadMem(4 bytes @ 0xE000EE08)
T2C60 006:070.723   CPU_WriteMem(4 bytes @ 0xE0001004)
T2C60 006:096.232   CPU_ReadMem(4 bytes @ 0xE0001004)
T2C60 006:096.679   CPU_WriteMem(6 bytes @ 0x2000D000)
T2C60 006:097.132   ClockFreq: 2083200 Hz
T2C60 006:097.206 - 41.421ms returns 2083200
T2C60 006:097.271 JLINK_ReadReg(XPSR)
T2C60 006:097.332   CPU_ReadMem(4 bytes @ 0xE000EE08)
T2C60 006:097.689 - 0.461ms returns 0xF9000000
T3234 006:172.163 JLINK_ReadReg(XPSR)
T3234 006:172.267   CPU_ReadMem(4 bytes @ 0xE000EE08)
T3234 006:172.618 - 0.491ms returns 0xF9000000
T3234 006:220.203 JLINK_ReadReg(XPSR)
T3234 006:220.347   CPU_ReadMem(4 bytes @ 0xE000EE08)
T3234 006:220.740 - 0.576ms returns 0xF9000000
T3234 006:534.125 JLINK_ReadReg(XPSR)
T3234 006:534.252   CPU_ReadMem(4 bytes @ 0xE000EE08)
T3234 006:534.860 - 0.788ms returns 0xF9000000
T3234 006:585.745 JLINK_SetEndian(ARM_ENDIAN_LITTLE)
T3234 006:585.878 - 0.166ms returns 0
T3234 006:586.308 JLINK_BeginDownload(Flags = 0x00000000)
T3234 006:586.394 - 0.115ms
T3234 006:606.103 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T3234 006:606.241   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T3234 006:607.038   Data:  03 00 13 00
T3234 006:607.183   Debug reg: DHCSR
T3234 006:611.175 - 5.106ms returns 0
T3234 006:613.945 JLINK_WriteMem(0x00000000, 0xBC0 Bytes, ...)
T3234 006:614.062   Data:  A0 34 00 20 25 36 00 00 95 34 00 00 21 36 00 00 ...
T3234 006:614.664   completely In flash
T3234 006:614.802 - 0.889ms returns 0xBC0
T3234 006:615.783 JLINK_WriteMem(0x00000BC0, 0xBB0 Bytes, ...)
T3234 006:615.863   Data:  7C 45 00 00 88 45 00 00 00 06 00 20 18 12 00 20 ...
T3234 006:615.974   completely In flash
T3234 006:616.062 - 0.311ms returns 0xBB0
T3234 006:616.805 JLINK_WriteMem(0x00001770, 0xBB0 Bytes, ...)
T3234 006:616.929   Data:  2D 23 B0 EE 47 8A F0 EE 67 8A 05 93 DB E5 27 46 ...
T3234 006:617.043   completely In flash
T3234 006:617.146 - 0.372ms returns 0xBB0
T3234 006:617.863 JLINK_WriteMem(0x00002320, 0xBB0 Bytes, ...)
T3234 006:617.962   Data:  0C F4 70 6C 4C EA 00 0C 4C F0 07 00 98 82 4C F0 ...
T3234 006:618.065   completely In flash
T3234 006:618.163 - 0.330ms returns 0xBB0
T3234 006:620.766 JLINK_WriteMem(0x00002ED0, 0xBB0 Bytes, ...)
T3234 006:621.005   Data:  84 42 09 D8 04 20 E8 E7 07 20 30 BC 70 47 08 20 ...
T3234 006:621.183   completely In flash
T3234 006:621.326 - 0.598ms returns 0xBB0
T3234 006:622.594 JLINK_WriteMem(0x00003A80, 0xBE0 Bytes, ...)
T3234 006:623.011   Data:  94 EA 0C 0F 95 EA 0C 0F 00 F0 DE F8 2C 44 81 EA ...
T3234 006:623.511   completely In flash
T3234 006:623.884 - 1.372ms returns 0xBE0
T3234 006:627.755 JLINK_WriteMem(0x00004660, 0x128 Bytes, ...)
T3234 006:627.982   Data:  00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 ...
T3234 006:628.202   completely In flash
T3234 006:628.550 - 2.669ms returns 0x128
T3234 006:632.311 JLINK_WriteMem(0x00004788, 0x8 Bytes, ...)
T3234 006:632.492   Data:  34 F9 FF 7F 01 00 00 00
T3234 006:632.603   completely In flash
T3234 006:632.695 - 0.414ms returns 0x8
T3234 006:633.879 JLINK_WriteMem(0x00004790, 0x624 Bytes, ...)
T3234 006:634.028   Data:  4F F4 2A 43 16 49 B1 F8 84 C0 A1 F8 84 30 B1 F8 ...
T3234 006:634.125   completely In flash
T3234 006:634.215 - 0.365ms returns 0x624
T3234 006:635.587 JLINK_WriteMem(0x0100A100, 0x10 Bytes, ...)
T3234 006:635.785   Data:  FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF
T3234 006:636.522   completely In flash
T3234 006:636.632 - 1.074ms returns 0x10
T3234 006:638.575 JLINK_WriteMem(0x0100A134, 0x4 Bytes, ...)
T3234 006:638.690   Data:  FF FF FF FF
T3234 006:638.795   completely In flash
T3234 006:639.067 - 0.524ms returns 0x4
T3234 006:642.346 JLINK_WriteMem(0x0100A200, 0xD0 Bytes, ...)
T3234 006:642.477   Data:  FF FD FF FF FF FF FF FF FF FF FF FF FF FF FF FF ...
T3234 006:642.596   completely In flash
T3234 006:642.691 - 0.376ms returns 0xD0
T3234 006:650.479 JLINK_EndDownload()
T3234 006:650.954   CPU_ReadMem(4 bytes @ 0xE000ED90)
T3234 006:651.699   CPU_ReadMem(4 bytes @ 0xE000ED94)
T3234 006:652.286    -- --------------------------------------
T3234 006:652.391   Flash bank @ 0x0100A100: Default: L2 verify disabled because algorithm performs L1 verify
T3234 006:652.477    -- Start of determining dirty areas in flash cache
T3234 006:652.573    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A100 if necessary
T3234 006:652.670    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A130 if necessary
T3234 006:652.977    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A200 if necessary
T3234 006:653.676    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A210 if necessary
T3234 006:654.802    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A220 if necessary
T3234 006:654.890    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A230 if necessary
T3234 006:654.959    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A240 if necessary
T3234 006:655.026    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A250 if necessary
T3234 006:655.093    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A260 if necessary
T3234 006:655.161    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A270 if necessary
T3234 006:655.227    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A280 if necessary
T3234 006:655.295    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A290 if necessary
T3234 006:655.377    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A2A0 if necessary
T3234 006:655.446    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A2B0 if necessary
T3234 006:655.513    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A2C0 if necessary
T3234 006:655.581    -- End of determining dirty areas
T3234 006:655.648    -- Start of preparing flash programming
T3234 006:655.715    -- Calculating RAM usage
T3234 006:655.792    -- RAM usage = 3476 Bytes
T3234 006:655.863    -- Preserving CPU registers
T3234 006:665.171    -- Determining CPU clock frequency
T3234 006:713.156    -- Preparing target
T3234 006:713.306    -- Preserving target RAM temporarily used for programming
T3234 006:725.259    -- Downloading RAMCode
T3234 006:739.443    -- Preparing RAMCode
T3234 006:746.127    -- CPU frequency = 100000 kHz
T3234 006:746.254    -- End of preparing flash programming
T3234 006:746.567   Looking for J-Link GUI Server exe at: C:\Users\T.Uemitsu\.eclipse\com.renesas.platform_780075259\DebugComp\RA\ARM\Segger_v7.86.2\JLinkGUIServer.exe
T3234 006:747.071   Looking for J-Link GUI Server exe at: C:\Program Files\SEGGER\JLink\JLinkGUIServer.exe
T3234 006:747.363   Forking J-Link GUI Server: C:\Program Files\SEGGER\JLink\JLinkGUIServer.exe
T3234 006:811.607   J-Link GUI Server info: "J-Link GUI server V7.88 "
T3234 006:940.471    -- CPU is running at 100000 kHz.
T3234 006:940.678    -- Start of comparing flash
T3234 006:940.831    -- CRC check was estimated as fastest method
T3234 007:103.137    -- Comparing range 0x100A100 - 0x100A10F (1 Sector, 16 Bytes), using multi-block CRC calculation
T3234 007:115.822    -- All CRCs match
T3234 007:117.056    -- Comparing range 0x100A130 - 0x100A13F (1 Sector, 16 Bytes), using multi-block CRC calculation
T3234 007:121.812    -- All CRCs match
T3234 007:122.561    -- Comparing range 0x100A200 - 0x100A2CF (13 Sectors, 208 Bytes), using multi-block CRC calculation
T3234 007:130.382    -- All CRCs match
T3234 007:131.006    -- Comparing range 0x100A100 - 0x100A10F (1 Sector, 16 Bytes), using alternative multi-block CRC calculation
T3234 007:134.227    -- All CRCs match
T3234 007:134.778    -- Comparing range 0x100A130 - 0x100A13F (1 Sector, 16 Bytes), using alternative multi-block CRC calculation
T3234 007:138.474    -- All CRCs match
T3234 007:139.212    -- Comparing range 0x100A200 - 0x100A2CF (13 Sectors, 208 Bytes), using alternative multi-block CRC calculation
T3234 007:146.796    -- All CRCs match
T3234 007:146.986    -- End of comparing flash
T3234 007:147.073    -- Start of erasing sectors
T3234 007:147.142    -- End of erasing sectors
T3234 007:147.219    -- Start of flash programming
T3234 007:147.287    -- End of flash programming
T3234 007:147.354    -- Start of restoring
T3234 007:147.422    -- Restoring RAMCode
T3234 007:151.731    -- Restoring target memory
T3234 007:163.530    -- Restore target
T3234 007:163.651    -- Restoring CPU registers
T3234 007:163.985    -- End of restoring
T3234 007:164.070    -- Bank 0 @ 0x0100A100: Skipped. Contents already match
T3234 007:164.145    -- Bank 0 @ 0x0100A100: Skipped. Contents already match
T3234 007:182.031    -- --------------------------------------
T3234 007:182.738   Flash bank @ 0x00000000: Default: L2 verify disabled because algorithm performs L1 verify
T3234 007:182.833    -- Start of determining dirty areas in flash cache
T3234 007:182.921    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x00000000 if necessary
T3234 007:183.007    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x00002000 if necessary
T3234 007:183.094    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x00004000 if necessary
T3234 007:183.305    -- End of determining dirty areas
T3234 007:183.392    -- Start of preparing flash programming
T3234 007:183.478    -- Calculating RAM usage
T3234 007:183.575    -- RAM usage = 4500 Bytes
T3234 007:183.663    -- Preserving CPU registers
T3234 007:183.805    -- Determining CPU clock frequency
T3234 007:224.286    -- Preparing target
T3234 007:224.445    -- Preserving target RAM temporarily used for programming
T3234 007:239.972    -- Downloading RAMCode
T3234 007:254.816    -- Preparing RAMCode
T3234 007:262.154    -- CPU frequency = 100000 kHz
T3234 007:262.415    -- End of preparing flash programming
T3234 007:268.448    -- CPU is running at 100000 kHz.
T3234 007:268.586    -- Start of comparing flash
T3234 007:268.681    -- CRC check was estimated as fastest method
T3234 007:294.376    -- Comparing range 0x0000 - 0x5FFF (3 Sectors, 24 KB), using multi-block CRC calculation
T3234 007:309.891    -- All CRCs match
T3234 007:312.393    -- Comparing range 0x0000 - 0x5FFF (3 Sectors, 24 KB), using alternative multi-block CRC calculation
T3234 007:322.147    -- All CRCs match
T3234 007:322.279    -- End of comparing flash
T3234 007:322.353    -- Start of erasing sectors
T3234 007:322.424    -- End of erasing sectors
T3234 007:322.493    -- Start of flash programming
T3234 007:322.560    -- End of flash programming
T3234 007:322.627    -- Start of restoring
T3234 007:322.695    -- Restoring RAMCode
T3234 007:327.277    -- Restoring target memory
T3234 007:342.879    -- Restore target
T3234 007:343.348    -- Restoring CPU registers
T3234 007:343.992    -- End of restoring
T3234 007:344.322    -- Bank 1 @ 0x00000000: Skipped. Contents already match
T3234 007:344.461    -- Bank 1 @ 0x00000000: Skipped. Contents already match
T3234 007:375.487 - 725.132ms returns 0 (0x0)
T3234 007:376.046 JLINK_WriteReg(R15 (PC), 0x00003624)
T3234 007:376.141 - 0.128ms returns 0
T3234 007:376.211 JLINK_WriteReg(XPSR, 0x01000000)
T3234 007:376.278 - 0.098ms returns 0
T3234 007:376.349 JLINK_ResetPullsRESET(ON)
T3234 007:376.408 - 0.090ms
T3234 007:376.652 JLINK_Halt()
T3234 007:377.186 - 0.637ms returns 0x00
T3234 007:377.416 JLINK_IsHalted()
T3234 007:377.579 - 0.233ms returns TRUE
T3234 007:379.028 JLINK_Reset()
T3234 007:379.320   CPU_WriteMem(4 bytes @ 0xE000EDF0)
T3234 007:380.059   CPU_ReadMem(4 bytes @ 0xE000ED44)
T3234 007:380.996   CPU_ReadMem(4 bytes @ 0xE000EE08)
T3234 007:381.399   CPU_WriteMem(4 bytes @ 0xE000EE08)
T3234 007:381.731   Reset: ARMv8M core with Security Extension enabled detected.
T3234 007:381.855   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T3234 007:382.261   Reset: Halt core after reset via DEMCR.VC_CORERESET.
T3234 007:382.727   Reset: Reset device via AIRCR.SYSRESETREQ.
T3234 007:382.877   CPU_WriteMem(4 bytes @ 0xE000ED0C)
T3234 007:436.986   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T3234 007:437.333   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T3234 007:437.647   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T3234 007:443.152   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T3234 007:446.800   CPU_WriteMem(4 bytes @ 0xE0002000)
T3234 007:447.135   CPU_ReadMem(4 bytes @ 0xE000EDFC)
T3234 007:447.452   CPU_ReadMem(4 bytes @ 0xE0001000)
T3234 007:447.811   CPU_ReadMem(4 bytes @ 0xE000EE08)
T3234 007:448.325 - 69.325ms
T3234 007:448.386 JLINK_SetEndian(ARM_ENDIAN_LITTLE)
T3234 007:448.433 - 0.068ms returns 0
T3234 007:449.445 JLINK_ResetPullsRESET(ON)
T3234 007:449.537 - 0.118ms
T3234 007:449.590 JLINK_Halt()
T3234 007:449.641 - 0.074ms returns 0x00
T3234 007:449.691 JLINK_IsHalted()
T3234 007:449.745 - 0.081ms returns TRUE
T3234 007:449.799 JLINK_Reset()
T3234 007:449.858   CPU_WriteMem(4 bytes @ 0xE000EDF0)
T3234 007:450.216   CPU_ReadMem(4 bytes @ 0xE000ED44)
T3234 007:450.562   CPU_ReadMem(4 bytes @ 0xE000EE08)
T3234 007:450.956   CPU_WriteMem(4 bytes @ 0xE000EE08)
T3234 007:451.331   Reset: ARMv8M core with Security Extension enabled detected.
T3234 007:451.410   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T3234 007:451.817   Reset: Halt core after reset via DEMCR.VC_CORERESET.
T3234 007:452.499   Reset: Reset device via AIRCR.SYSRESETREQ.
T3234 007:452.572   CPU_WriteMem(4 bytes @ 0xE000ED0C)
T3234 007:505.314   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T3234 007:505.703   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T3234 007:506.027   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T3234 007:511.484   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T3234 007:514.968   CPU_WriteMem(4 bytes @ 0xE0002000)
T3234 007:515.333   CPU_ReadMem(4 bytes @ 0xE000EDFC)
T3234 007:515.684   CPU_ReadMem(4 bytes @ 0xE0001000)
T3234 007:516.012   CPU_ReadMem(4 bytes @ 0xE000EE08)
T3234 007:516.346 - 66.583ms
T3234 007:516.423 JLINK_SetEndian(ARM_ENDIAN_LITTLE)
T3234 007:516.479 - 0.077ms returns 0
T3234 007:546.071 JLINK_ReadMem(0x00003624, 0x4 Bytes, ...)
T3234 007:546.181    -- Read from flash cache (4 bytes @ 0x00003624)
T3234 007:546.289   Data:  08 B5 00 F0
T3234 007:546.374 - 0.336ms returns 0
T3234 007:553.893 JLINK_ReadReg(XPSR)
T3234 007:554.035   CPU_ReadMem(4 bytes @ 0xE000EE08)
T3234 007:554.419 - 0.581ms returns 0xF9000000
T3234 008:194.410 JLINK_ReadReg(XPSR)
T3234 008:194.813 - 0.449ms returns 0xF9000000
T3234 008:196.040 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T3234 008:196.139 - 0.126ms returns 0x08
T3234 008:196.195 JLINK_GetNumWPUnits()
T3234 008:196.244 - 0.073ms returns 4
T3234 008:196.296 JLINK_GetNumWPUnits()
T3234 008:196.343 - 0.070ms returns 4
T3234 008:196.403 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T3234 008:196.454 - 0.073ms returns 0x08
T3234 008:196.508 JLINK_GetNumWPUnits()
T3234 008:196.560 - 0.074ms returns 4
T3234 008:196.608 JLINK_GetNumWPUnits()
T3234 008:196.671 - 0.087ms returns 4
T3234 008:196.732 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T3234 008:196.779 - 0.069ms returns 0x08
T3234 008:196.827 JLINK_GetNumWPUnits()
T3234 008:196.872 - 0.067ms returns 4
T3234 008:196.919 JLINK_GetNumWPUnits()
T3234 008:196.964 - 0.084ms returns 4
T3234 008:197.107 JLINK_SetBPEx(Addr = 0x00001CEC, Type = 0xFFFFFF00)
T3234 008:197.182 - 0.106ms returns 0x00000001
T3234 008:197.257 JLINK_ClrBPEx(BPHandle = 0x00000001)
T3234 008:197.322 - 0.096ms returns 0x00
T3234 008:200.427 JLINK_SetBPEx(Addr = 0x00001CEC, Type = 0xFFFFFF00)
T3234 008:200.573 - 0.183ms returns 0x00000002
T3234 008:262.769 JLINK_ReadRegs(NumRegs = 22, Indexes: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 86, 87, 20)
T3234 008:262.919    -- R0=0x00, R1=0x00, R2=0x00, R3=0x00, R4=0x00, R5=0x00, R6=0x00, R7=0x00, R8=0xF0, R9=0x270F, R10=0x200025C7, R11=0x104FF, R12=0x2000D888, R13 (SP)=0x200034A0, R14=0xFFFFFFFF, R15 (PC)=0x3624, XPSR=0xF9000000, MSP=0x200034A0, PSP=0x00, MSPLIM=0x00, PSPLIM=0x00, CFBP=0x00
T3234 008:263.014 - 0.275ms returns 0x00
T3234 008:263.738 JLINK_ReadMem(0x00003624, 0x4 Bytes, ...)
T3234 008:263.826    -- Read from flash cache (4 bytes @ 0x00003624)
T3234 008:263.896   Data:  08 B5 00 F0
T3234 008:263.966 - 0.251ms returns 0
T2498 008:295.896 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T2498 008:296.008 - 0.146ms returns 0x08
T2498 008:296.081 JLINK_GetNumWPUnits()
T2498 008:296.146 - 0.096ms returns 4
T2498 008:296.509 JLINK_GetNumWPUnits()
T2498 008:296.646 - 0.169ms returns 4
T2498 008:302.150 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T2498 008:302.275 - 0.159ms returns 0x08
T2498 008:302.344 JLINK_GetNumWPUnits()
T2498 008:302.401 - 0.085ms returns 4
T2498 008:302.459 JLINK_GetNumWPUnits()
T2498 008:302.515 - 0.083ms returns 4
T2498 008:305.322 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T2498 008:305.416 - 0.119ms returns 0x08
T2498 008:305.467 JLINK_GetNumWPUnits()
T2498 008:305.519 - 0.076ms returns 4
T2498 008:305.568 JLINK_GetNumWPUnits()
T2498 008:305.613 - 0.067ms returns 4
T2498 008:306.274 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T2498 008:306.356 - 0.106ms returns 0x08
T2498 008:306.405 JLINK_GetNumWPUnits()
T2498 008:306.451 - 0.068ms returns 4
T2498 008:306.500 JLINK_GetNumWPUnits()
T2498 008:306.550 - 0.073ms returns 4
T2498 008:307.247 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T2498 008:307.338 - 0.119ms returns 0x08
T2498 008:307.396 JLINK_GetNumWPUnits()
T2498 008:307.445 - 0.073ms returns 4
T2498 008:307.519 JLINK_GetNumWPUnits()
T2498 008:307.568 - 0.073ms returns 4
T2498 008:308.266 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T2498 008:308.364 - 0.133ms returns 0x08
T2498 008:308.437 JLINK_GetNumWPUnits()
T2498 008:308.499 - 0.092ms returns 4
T2498 008:308.563 JLINK_GetNumWPUnits()
T2498 008:308.620 - 0.085ms returns 4
T2498 008:309.670 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T2498 008:309.748 - 0.101ms returns 0x08
T2498 008:309.796 JLINK_GetNumWPUnits()
T2498 008:309.841 - 0.067ms returns 4
T2498 008:309.889 JLINK_GetNumWPUnits()
T2498 008:309.939 - 0.073ms returns 4
T2498 008:310.527 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T2498 008:310.652 - 0.165ms returns 0x08
T2498 008:310.731 JLINK_GetNumWPUnits()
T2498 008:310.796 - 0.097ms returns 4
T2498 008:310.864 JLINK_GetNumWPUnits()
T2498 008:310.954 - 0.121ms returns 4
T3234 009:215.853 JLINK_ReadReg(XPSR)
T3234 009:216.229 - 0.410ms returns 0xF9000000
T3234 009:218.051 JLINK_ReadReg(XPSR)
T3234 009:218.153 - 0.128ms returns 0xF9000000
T3234 010:280.712 JLINK_STRACE_Read(..., NumItems = 0x10000)
T3234 010:281.016 - 0.348ms NumItemsRead = 0x00
T3234 010:281.107 JLINK_IsHalted()
T3234 010:281.483 - 0.420ms returns TRUE
T3234 010:281.567 JLINK_GoEx(MaxEmulInsts = 0, Flags = 0x01)
T3234 010:281.752   CPU_WriteMem(4 bytes @ 0xE0002000)
T3234 010:282.167   CPU_ReadMem(4 bytes @ 0xE0001000)
T3234 010:282.528   CPU_WriteMem(4 bytes @ 0xE0002008)
T3234 010:282.635   CPU_WriteMem(4 bytes @ 0xE000200C)
T3234 010:282.736   CPU_WriteMem(4 bytes @ 0xE0002010)
T3234 010:282.827   CPU_WriteMem(4 bytes @ 0xE0002014)
T3234 010:282.913   CPU_WriteMem(4 bytes @ 0xE0002018)
T3234 010:283.000   CPU_WriteMem(4 bytes @ 0xE000201C)
T3234 010:283.086   CPU_WriteMem(4 bytes @ 0xE0002020)
T3234 010:283.173   CPU_WriteMem(4 bytes @ 0xE0002024)
T3234 010:284.411   CPU_WriteMem(4 bytes @ 0xE0001004)
T3234 010:285.150 - 3.625ms
T3234 010:380.865 JLINK_IsHalted()
T3234 010:383.676 - 2.907ms returns TRUE
T3234 010:383.828 JLINK_ReadReg(XPSR)
T3234 010:383.891   CPU_ReadMem(4 bytes @ 0xE000EE08)
T3234 010:384.268 - 0.469ms returns 0x69000000
T3234 010:384.327 JLINK_ReadReg(R15 (PC))
T3234 010:384.397 - 0.092ms returns 0x00001CEC
T3234 010:384.464 JLINK_ReadReg(XPSR)
T3234 010:384.521 - 0.079ms returns 0x69000000
T3234 010:384.570 JLINK_ReadReg(XPSR)
T3234 010:384.647 - 0.099ms returns 0x69000000
T3234 010:384.695 JLINK_ReadReg(R15 (PC))
T3234 010:384.761 - 0.088ms returns 0x00001CEC
T3234 010:384.820 JLINK_ReadReg(XPSR)
T3234 010:384.876 - 0.078ms returns 0x69000000
T3234 010:384.924 JLINK_ReadReg(XPSR)
T3234 010:384.990 - 0.088ms returns 0x69000000
T3234 010:385.038 JLINK_ReadMem(0x00001CEC, 0x1 Bytes, ...)
T3234 010:385.106    -- Read from flash cache (1 bytes @ 0x00001CEC)
T3234 010:385.170   Data:  08
T3234 010:385.234 - 0.220ms returns 0
T3234 010:385.285 JLINK_IsHalted()
T3234 010:385.349 - 0.085ms returns TRUE
T3234 010:385.397 JLINK_ReadReg(XPSR)
T3234 010:385.462 - 0.087ms returns 0x69000000
T3234 010:385.510 JLINK_ReadReg(XPSR)
T3234 010:385.595 - 0.108ms returns 0x69000000
T3234 010:385.645 JLINK_ReadReg(R15 (PC))
T3234 010:385.691 - 0.069ms returns 0x00001CEC
T3234 010:385.742 JLINK_ReadReg(XPSR)
T3234 010:385.789 - 0.070ms returns 0x69000000
T3234 010:385.839 JLINK_ReadReg(XPSR)
T3234 010:385.885 - 0.069ms returns 0x69000000
T3234 010:385.935 JLINK_ReadMem(0x00001CEC, 0x1 Bytes, ...)
T3234 010:385.980    -- Read from flash cache (1 bytes @ 0x00001CEC)
T3234 010:386.047   Data:  08
T3234 010:386.111 - 0.199ms returns 0
T3234 010:387.216 JLINK_ReadRegs(NumRegs = 22, Indexes: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 86, 87, 20)
T3234 010:387.325    -- R0=0x00, R1=0x00, R2=0x11F, R3=0x60, R4=0x00, R5=0x00, R6=0x00, R7=0x00, R8=0xF0, R9=0x270F, R10=0x200025C7, R11=0x104FF, R12=0x10, R13 (SP)=0x20003498, R14=0x362F, R15 (PC)=0x1CEC, XPSR=0x69000000, MSP=0x20003498, PSP=0x00, MSPLIM=0x200024A0, PSPLIM=0x00, CFBP=0x00
T3234 010:387.394 - 0.201ms returns 0x00
T3234 010:387.885 JLINK_ReadMem(0x00001CEC, 0x4 Bytes, ...)
T3234 010:387.944    -- Read from flash cache (4 bytes @ 0x00001CEC)
T3234 010:388.012   Data:  08 B5 FE F7
T3234 010:388.077 - 0.214ms returns 0
T3234 010:390.719 JLINK_ClrBPEx(BPHandle = 0x00000002)
T3234 010:390.820 - 0.126ms returns 0x00
T3234 010:470.772 JLINK_ReadReg(XPSR)
T3234 010:470.886 - 0.150ms returns 0x69000000
T3234 010:472.985 JLINK_ReadReg(XPSR)
T3234 010:473.098 - 0.148ms returns 0x69000000
T2498 011:392.509 JLINK_IsHalted()
T2498 011:392.948 - 0.471ms returns TRUE
T2498 011:393.009 JLINK_ReadReg(XPSR)
T2498 011:393.065 - 0.078ms returns 0x69000000
T2498 011:393.113 JLINK_ReadReg(R15 (PC))
T2498 011:393.175 - 0.086ms returns 0x00001CEC
T2498 011:393.237 JLINK_ReadReg(XPSR)
T2498 011:393.288 - 0.094ms returns 0x69000000
T2498 011:393.379 JLINK_ReadReg(XPSR)
T2498 011:393.458 - 0.102ms returns 0x69000000
T2498 011:393.508 JLINK_ReadReg(R15 (PC))
T2498 011:393.574 - 0.088ms returns 0x00001CEC
T2498 011:393.634 JLINK_ReadReg(XPSR)
T2498 011:393.690 - 0.078ms returns 0x69000000
T2498 011:393.738 JLINK_ReadReg(XPSR)
T2498 011:393.804 - 0.087ms returns 0x69000000
T2498 011:393.851 JLINK_ReadMem(0x00001CEC, 0x1 Bytes, ...)
T2498 011:393.919    -- Read from flash cache (1 bytes @ 0x00001CEC)
T2498 011:393.984   Data:  08
T2498 011:394.047 - 0.216ms returns 0
T2498 011:394.094 JLINK_IsHalted()
T2498 011:394.172 - 0.101ms returns TRUE
T2498 011:394.230 JLINK_ReadReg(XPSR)
T2498 011:394.320 - 0.113ms returns 0x69000000
T2498 011:394.370 JLINK_ReadReg(XPSR)
T2498 011:394.426 - 0.077ms returns 0x69000000
T2498 011:394.473 JLINK_ReadReg(R15 (PC))
T2498 011:394.539 - 0.087ms returns 0x00001CEC
T2498 011:394.597 JLINK_ReadReg(XPSR)
T2498 011:394.653 - 0.087ms returns 0x69000000
T2498 011:394.700 JLINK_ReadReg(XPSR)
T2498 011:394.765 - 0.087ms returns 0x69000000
T2498 011:394.813 JLINK_ReadMem(0x00001CEC, 0x1 Bytes, ...)
T2498 011:394.868    -- Read from flash cache (1 bytes @ 0x00001CEC)
T2498 011:394.934   Data:  08
T2498 011:394.999 - 0.208ms returns 0
T2498 011:395.136 JLINK_WriteMem(0xE0001FB0, 0x4 Bytes, ...)
T2498 011:395.186   Data:  55 CE AC C5
T2498 011:395.647   CPU_WriteMem(4 bytes @ 0xE0001FB0)
T2498 011:396.032 - 0.929ms returns 0x4
T2498 011:396.096 JLINK_WriteMem(0xE0001000, 0x4 Bytes, ...)
T2498 011:396.146   Data:  01 00 00 48
T2498 011:396.216   Debug reg: DWT_CTRL
T2498 011:396.295   CPU_WriteMem(4 bytes @ 0xE0001000)
T2498 011:396.616 - 0.550ms returns 0x4
T2498 011:396.677 JLINK_ReadMem(0xE0001000, 0x4 Bytes, ...)
T2498 011:396.730   CPU_ReadMem(4 bytes @ 0xE0001000)
T2498 011:397.030   Data:  01 00 00 40
T2498 011:397.105   Debug reg: DWT_CTRL
T2498 011:397.176 - 0.522ms returns 0
T2498 011:397.227 JLINK_WriteMem(0xE0001004, 0x4 Bytes, ...)
T2498 011:397.272   Data:  00 00 00 00
T2498 011:397.360   Debug reg: DWT_CYCCNT
T2498 011:397.437 - 0.233ms returns 0x4
T2498 011:397.490 JLINK_ReadMem(0xE0001004, 0x4 Bytes, ...)
T2498 011:397.539   Data:  00 00 00 00
T2498 011:397.606   Debug reg: DWT_CYCCNT
T2498 011:397.671 - 0.203ms returns 0
T3234 011:806.408 JLINK_STRACE_Read(..., NumItems = 0x10000)
T3234 011:806.534 - 0.157ms NumItemsRead = 0x00
T3234 011:806.611 JLINK_ReadMem(0xE0001004, 0x4 Bytes, ...)
T3234 011:806.693   Data:  00 00 00 00
T3234 011:806.786   Debug reg: DWT_CYCCNT
T3234 011:806.869 - 0.287ms returns 0
T3234 011:806.938 JLINK_IsHalted()
T3234 011:807.111 - 0.217ms returns TRUE
T3234 011:807.192 JLINK_GoEx(MaxEmulInsts = 0, Flags = 0x01)
T3234 011:807.275   CPU_ReadMem(4 bytes @ 0xE0001000)
T3234 011:807.698   CPU_WriteMem(4 bytes @ 0xE0002008)
T3234 011:808.072   CPU_WriteMem(4 bytes @ 0xE0001004)
T3234 011:809.025 - 1.874ms
T3234 011:911.617 JLINK_IsHalted()
T3234 011:911.999 - 0.413ms returns FALSE
T3234 011:912.057 JLINK_IsHalted()
T3234 011:912.409 - 0.401ms returns FALSE
T3234 012:021.539 JLINK_IsHalted()
T3234 012:021.954 - 0.444ms returns FALSE
T3234 012:022.011 JLINK_IsHalted()
T3234 012:022.336 - 0.364ms returns FALSE
T3234 012:130.388 JLINK_IsHalted()
T3234 012:130.785 - 0.426ms returns FALSE
T3234 012:130.842 JLINK_IsHalted()
T3234 012:131.168 - 0.364ms returns FALSE
T3234 012:240.254 JLINK_IsHalted()
T3234 012:240.651 - 0.427ms returns FALSE
T3234 012:240.709 JLINK_IsHalted()
T3234 012:241.069 - 0.399ms returns FALSE
T3234 012:349.070 JLINK_IsHalted()
T3234 012:349.478 - 0.438ms returns FALSE
T3234 012:349.535 JLINK_IsHalted()
T3234 012:349.859 - 0.362ms returns FALSE
T3234 012:458.919 JLINK_IsHalted()
T3234 012:459.435 - 0.550ms returns FALSE
T3234 012:459.499 JLINK_IsHalted()
T3234 012:459.855 - 0.387ms returns FALSE
T3234 012:568.026 JLINK_IsHalted()
T3234 012:568.444 - 0.475ms returns FALSE
T3234 012:568.534 JLINK_IsHalted()
T3234 012:568.886 - 0.381ms returns FALSE
T3234 012:677.479 JLINK_IsHalted()
T3234 012:677.868 - 0.427ms returns FALSE
T3234 012:677.937 JLINK_IsHalted()
T3234 012:678.311 - 0.418ms returns FALSE
T3234 012:787.439 JLINK_IsHalted()
T3234 012:787.831 - 0.422ms returns FALSE
T3234 012:787.889 JLINK_IsHalted()
T3234 012:788.280 - 0.421ms returns FALSE
T2498 012:808.726 JLINK_IsHalted()
T2498 012:809.138 - 0.449ms returns FALSE
T2498 012:809.204 JLINK_IsHalted()
T2498 012:809.509 - 0.336ms returns FALSE
T3234 012:896.321 JLINK_IsHalted()
T3234 012:896.722 - 0.431ms returns FALSE
T3234 012:896.780 JLINK_IsHalted()
T3234 012:897.137 - 0.386ms returns FALSE
T3234 013:005.279 JLINK_IsHalted()
T3234 013:005.689 - 0.444ms returns FALSE
T3234 013:005.754 JLINK_IsHalted()
T3234 013:006.126 - 0.432ms returns FALSE
T3234 013:114.941 JLINK_IsHalted()
T3234 013:115.343 - 0.431ms returns FALSE
T3234 013:115.400 JLINK_IsHalted()
T3234 013:115.839 - 0.469ms returns FALSE
T3234 013:224.828 JLINK_IsHalted()
T3234 013:225.233 - 0.441ms returns FALSE
T3234 013:225.299 JLINK_IsHalted()
T3234 013:225.595 - 0.326ms returns FALSE
T3234 013:333.730 JLINK_IsHalted()
T3234 013:334.074 - 0.374ms returns FALSE
T3234 013:334.133 JLINK_IsHalted()
T3234 013:334.443 - 0.338ms returns FALSE
T3234 013:443.434 JLINK_IsHalted()
T3234 013:443.867 - 0.462ms returns FALSE
T3234 013:443.925 JLINK_IsHalted()
T3234 013:444.283 - 0.397ms returns FALSE
T3234 013:552.362 JLINK_IsHalted()
T3234 013:552.758 - 0.426ms returns FALSE
T3234 013:552.816 JLINK_IsHalted()
T3234 013:553.208 - 0.422ms returns FALSE
T3234 013:662.268 JLINK_IsHalted()
T3234 013:662.675 - 0.436ms returns FALSE
T3234 013:662.733 JLINK_IsHalted()
T3234 013:663.085 - 0.381ms returns FALSE
T3234 013:771.202 JLINK_IsHalted()
T3234 013:771.602 - 0.446ms returns FALSE
T3234 013:771.684 JLINK_IsHalted()
T3234 013:771.978 - 0.324ms returns FALSE
T2498 013:810.486 JLINK_IsHalted()
T2498 013:810.898 - 0.451ms returns FALSE
T2498 013:810.965 JLINK_IsHalted()
T2498 013:811.281 - 0.345ms returns FALSE
T3234 013:881.079 JLINK_IsHalted()
T3234 013:881.467 - 0.418ms returns FALSE
T3234 013:881.525 JLINK_IsHalted()
T3234 013:881.863 - 0.368ms returns FALSE
T3234 013:989.719 JLINK_IsHalted()
T3234 013:990.134 - 0.445ms returns FALSE
T3234 013:990.192 JLINK_IsHalted()
T3234 013:990.559 - 0.405ms returns FALSE
T3234 014:099.515 JLINK_IsHalted()
T3234 014:099.945 - 0.459ms returns FALSE
T3234 014:100.002 JLINK_IsHalted()
T3234 014:100.360 - 0.396ms returns FALSE
T3234 014:208.426 JLINK_IsHalted()
T3234 014:208.824 - 0.428ms returns FALSE
T3234 014:208.882 JLINK_IsHalted()
T3234 014:209.204 - 0.362ms returns FALSE
T3234 014:318.347 JLINK_IsHalted()
T3234 014:318.763 - 0.445ms returns FALSE
T3234 014:318.820 JLINK_IsHalted()
T3234 014:319.163 - 0.372ms returns FALSE
T3234 014:427.577 JLINK_IsHalted()
T3234 014:427.970 - 0.424ms returns FALSE
T3234 014:428.029 JLINK_IsHalted()
T3234 014:428.372 - 0.369ms returns FALSE
T3234 014:536.961 JLINK_IsHalted()
T3234 014:537.369 - 0.448ms returns FALSE
T3234 014:537.436 JLINK_IsHalted()
T3234 014:537.750 - 0.344ms returns FALSE
T3234 014:646.863 JLINK_IsHalted()
T3234 014:647.269 - 0.444ms returns FALSE
T3234 014:647.335 JLINK_IsHalted()
T3234 014:647.676 - 0.370ms returns FALSE
T3234 014:755.823 JLINK_IsHalted()
T3234 014:756.173 - 0.387ms returns FALSE
T3234 014:756.240 JLINK_IsHalted()
T3234 014:756.546 - 0.336ms returns FALSE
T2498 014:811.504 JLINK_IsHalted()
T2498 014:811.885 - 0.412ms returns FALSE
T2498 014:811.945 JLINK_IsHalted()
T2498 014:812.270 - 0.366ms returns FALSE
T3234 014:865.461 JLINK_IsHalted()
T3234 014:865.865 - 0.442ms returns FALSE
T3234 014:865.932 JLINK_IsHalted()
T3234 014:866.309 - 0.421ms returns FALSE
T3234 014:974.314 JLINK_IsHalted()
T3234 014:974.735 - 0.453ms returns FALSE
T3234 014:974.796 JLINK_IsHalted()
T3234 014:975.124 - 0.368ms returns FALSE
T3234 015:084.146 JLINK_IsHalted()
T3234 015:084.552 - 0.436ms returns FALSE
T3234 015:084.609 JLINK_IsHalted()
T3234 015:084.960 - 0.390ms returns FALSE
T3234 015:192.979 JLINK_IsHalted()
T3234 015:193.395 - 0.445ms returns FALSE
T3234 015:193.452 JLINK_IsHalted()
T3234 015:193.809 - 0.396ms returns FALSE
T3234 015:302.978 JLINK_IsHalted()
T3234 015:303.300 - 0.350ms returns FALSE
T3234 015:303.356 JLINK_IsHalted()
T3234 015:303.639 - 0.310ms returns FALSE
T3234 015:411.544 JLINK_IsHalted()
T3234 015:411.910 - 0.401ms returns FALSE
T3234 015:411.974 JLINK_IsHalted()
T3234 015:412.278 - 0.336ms returns FALSE
T3234 015:521.637 JLINK_IsHalted()
T3234 015:522.058 - 0.459ms returns FALSE
T3234 015:522.127 JLINK_IsHalted()
T3234 015:522.456 - 0.360ms returns FALSE
T3234 015:630.367 JLINK_IsHalted()
T3234 015:630.763 - 0.431ms returns FALSE
T3234 015:630.830 JLINK_IsHalted()
T3234 015:631.180 - 0.389ms returns FALSE
T3234 015:740.246 JLINK_IsHalted()
T3234 015:740.673 - 0.457ms returns FALSE
T3234 015:740.730 JLINK_IsHalted()
T3234 015:741.105 - 0.405ms returns FALSE
T2498 015:812.620 JLINK_IsHalted()
T2498 015:813.049 - 0.484ms returns FALSE
T2498 015:813.145 JLINK_IsHalted()
T2498 015:813.483 - 0.380ms returns FALSE
T3234 015:849.445 JLINK_IsHalted()
T3234 015:849.804 - 0.408ms returns FALSE
T3234 015:849.890 JLINK_IsHalted()
T3234 015:850.202 - 0.339ms returns FALSE
T3234 015:958.896 JLINK_IsHalted()
T3234 015:959.294 - 0.427ms returns FALSE
T3234 015:959.351 JLINK_IsHalted()
T3234 015:959.711 - 0.396ms returns FALSE
T3234 016:068.749 JLINK_IsHalted()
T3234 016:069.167 - 0.448ms returns FALSE
T3234 016:069.225 JLINK_IsHalted()
T3234 016:069.558 - 0.372ms returns FALSE
T3234 016:177.677 JLINK_IsHalted()
T3234 016:178.131 - 0.486ms returns FALSE
T3234 016:178.190 JLINK_IsHalted()
T3234 016:178.540 - 0.379ms returns FALSE
T3234 016:286.627 JLINK_IsHalted()
T3234 016:287.040 - 0.443ms returns FALSE
T3234 016:287.098 JLINK_IsHalted()
T3234 016:287.454 - 0.417ms returns FALSE
T3234 016:396.738 JLINK_IsHalted()
T3234 016:397.150 - 0.454ms returns FALSE
T3234 016:397.223 JLINK_IsHalted()
T3234 016:397.505 - 0.320ms returns FALSE
T3234 016:506.112 JLINK_IsHalted()
T3234 016:506.550 - 0.476ms returns FALSE
T3234 016:506.616 JLINK_IsHalted()
T3234 016:506.913 - 0.336ms returns FALSE
T3234 016:615.006 JLINK_IsHalted()
T3234 016:615.419 - 0.443ms returns FALSE
T3234 016:615.477 JLINK_IsHalted()
T3234 016:615.800 - 0.362ms returns FALSE
T3234 016:724.891 JLINK_IsHalted()
T3234 016:725.306 - 0.444ms returns FALSE
T3234 016:725.363 JLINK_IsHalted()
T3234 016:725.801 - 0.467ms returns FALSE
T2498 016:813.931 JLINK_IsHalted()
T2498 016:814.315 - 0.416ms returns FALSE
T2498 016:814.376 JLINK_IsHalted()
T2498 016:814.739 - 0.395ms returns FALSE
T3234 016:833.604 JLINK_IsHalted()
T3234 016:833.987 - 0.412ms returns FALSE
T3234 016:834.044 JLINK_IsHalted()
T3234 016:834.356 - 0.342ms returns FALSE
T3234 016:943.005 JLINK_IsHalted()
T3234 016:943.408 - 0.433ms returns FALSE
T3234 016:943.466 JLINK_IsHalted()
T3234 016:943.803 - 0.366ms returns FALSE
T3234 017:052.241 JLINK_IsHalted()
T3234 017:052.622 - 0.410ms returns FALSE
T3234 017:052.680 JLINK_IsHalted()
T3234 017:052.991 - 0.340ms returns FALSE
T3234 017:162.175 JLINK_IsHalted()
T3234 017:162.547 - 0.401ms returns FALSE
T3234 017:162.605 JLINK_IsHalted()
T3234 017:162.916 - 0.367ms returns FALSE
T3234 017:271.067 JLINK_IsHalted()
T3234 017:271.475 - 0.438ms returns FALSE
T3234 017:271.533 JLINK_IsHalted()
T3234 017:271.858 - 0.383ms returns FALSE
T3234 017:380.667 JLINK_IsHalted()
T3234 017:381.105 - 0.467ms returns FALSE
T3234 017:381.163 JLINK_IsHalted()
T3234 017:381.476 - 0.343ms returns FALSE
T3234 017:490.612 JLINK_IsHalted()
T3234 017:491.033 - 0.451ms returns FALSE
T3234 017:491.091 JLINK_IsHalted()
T3234 017:491.449 - 0.408ms returns FALSE
T3234 017:599.544 JLINK_IsHalted()
T3234 017:599.916 - 0.402ms returns FALSE
T3234 017:599.973 JLINK_IsHalted()
T3234 017:600.340 - 0.397ms returns FALSE
T3234 017:709.380 JLINK_IsHalted()
T3234 017:709.764 - 0.414ms returns FALSE
T3234 017:709.822 JLINK_IsHalted()
T3234 017:710.194 - 0.413ms returns FALSE
T2498 017:815.600 JLINK_IsHalted()
T2498 017:816.037 - 0.478ms returns FALSE
T2498 017:816.107 JLINK_IsHalted()
T2498 017:816.451 - 0.374ms returns FALSE
T3234 017:818.310 JLINK_IsHalted()
T3234 017:818.684 - 0.422ms returns FALSE
T3234 017:818.771 JLINK_IsHalted()
T3234 017:819.111 - 0.380ms returns FALSE
T3234 017:928.064 JLINK_IsHalted()
T3234 017:928.477 - 0.443ms returns FALSE
T3234 017:928.536 JLINK_IsHalted()
T3234 017:928.868 - 0.362ms returns FALSE
T3234 018:036.966 JLINK_IsHalted()
T3234 018:037.370 - 0.433ms returns FALSE
T3234 018:037.428 JLINK_IsHalted()
T3234 018:037.782 - 0.399ms returns FALSE
T3234 018:146.378 JLINK_IsHalted()
T3234 018:146.794 - 0.465ms returns FALSE
T3234 018:146.875 JLINK_IsHalted()
T3234 018:147.238 - 0.395ms returns FALSE
T3234 018:255.639 JLINK_IsHalted()
T3234 018:256.037 - 0.427ms returns FALSE
T3234 018:256.094 JLINK_IsHalted()
T3234 018:256.449 - 0.394ms returns FALSE
T3234 018:365.479 JLINK_IsHalted()
T3234 018:365.892 - 0.442ms returns FALSE
T3234 018:365.949 JLINK_IsHalted()
T3234 018:366.283 - 0.372ms returns FALSE
T3234 018:474.465 JLINK_IsHalted()
T3234 018:474.855 - 0.421ms returns FALSE
T3234 018:474.914 JLINK_IsHalted()
T3234 018:475.290 - 0.410ms returns FALSE
T3234 018:583.392 JLINK_IsHalted()
T3234 018:583.766 - 0.424ms returns FALSE
T3234 018:583.875 JLINK_IsHalted()
T3234 018:584.196 - 0.350ms returns FALSE
T3234 018:692.968 JLINK_IsHalted()
T3234 018:693.397 - 0.458ms returns FALSE
T3234 018:693.454 JLINK_IsHalted()
T3234 018:693.835 - 0.414ms returns FALSE
T3234 018:802.894 JLINK_IsHalted()
T3234 018:803.290 - 0.427ms returns FALSE
T3234 018:803.348 JLINK_IsHalted()
T3234 018:803.673 - 0.364ms returns FALSE
T2498 018:817.201 JLINK_IsHalted()
T2498 018:817.643 - 0.484ms returns FALSE
T2498 018:817.717 JLINK_IsHalted()
T2498 018:818.069 - 0.382ms returns FALSE
T3234 018:911.780 JLINK_IsHalted()
T3234 018:912.167 - 0.417ms returns FALSE
T3234 018:912.225 JLINK_IsHalted()
T3234 018:912.583 - 0.387ms returns FALSE
T3234 019:021.575 JLINK_IsHalted()
T3234 019:021.978 - 0.432ms returns FALSE
T3234 019:022.035 JLINK_IsHalted()
T3234 019:022.401 - 0.403ms returns FALSE
T3234 019:130.303 JLINK_IsHalted()
T3234 019:130.708 - 0.434ms returns FALSE
T3234 019:130.765 JLINK_IsHalted()
T3234 019:131.107 - 0.375ms returns FALSE
T3234 019:240.266 JLINK_IsHalted()
T3234 019:240.672 - 0.435ms returns FALSE
T3234 019:240.729 JLINK_IsHalted()
T3234 019:241.092 - 0.401ms returns FALSE
T3234 019:349.170 JLINK_IsHalted()
T3234 019:349.590 - 0.451ms returns FALSE
T3234 019:349.649 JLINK_IsHalted()
T3234 019:349.990 - 0.371ms returns FALSE
T3234 019:459.043 JLINK_IsHalted()
T3234 019:459.466 - 0.452ms returns FALSE
T3234 019:459.523 JLINK_IsHalted()
T3234 019:459.866 - 0.372ms returns FALSE
T3234 019:567.774 JLINK_IsHalted()
T3234 019:568.174 - 0.430ms returns FALSE
T3234 019:568.231 JLINK_IsHalted()
T3234 019:568.601 - 0.411ms returns FALSE
T3234 019:677.668 JLINK_IsHalted()
T3234 019:678.058 - 0.421ms returns FALSE
T3234 019:678.117 JLINK_IsHalted()
T3234 019:678.441 - 0.363ms returns FALSE
T3234 019:787.465 JLINK_IsHalted()
T3234 019:787.827 - 0.402ms returns FALSE
T3234 019:787.898 JLINK_IsHalted()
T3234 019:788.239 - 0.373ms returns FALSE
T2498 019:818.762 JLINK_IsHalted()
T2498 019:819.180 - 0.459ms returns FALSE
T2498 019:819.249 JLINK_IsHalted()
T2498 019:819.594 - 0.385ms returns FALSE
T3234 019:896.405 JLINK_IsHalted()
T3234 019:896.812 - 0.454ms returns FALSE
T3234 019:896.898 JLINK_IsHalted()
T3234 019:897.284 - 0.425ms returns FALSE
T3234 020:005.351 JLINK_IsHalted()
T3234 020:005.765 - 0.443ms returns FALSE
T3234 020:005.822 JLINK_IsHalted()
T3234 020:006.131 - 0.339ms returns FALSE
T3234 020:114.896 JLINK_IsHalted()
T3234 020:115.298 - 0.431ms returns FALSE
T3234 020:115.355 JLINK_IsHalted()
T3234 020:115.692 - 0.376ms returns FALSE
T3234 020:224.828 JLINK_IsHalted()
T3234 020:225.228 - 0.429ms returns FALSE
T3234 020:225.285 JLINK_IsHalted()
T3234 020:225.652 - 0.407ms returns FALSE
T3234 020:333.727 JLINK_IsHalted()
T3234 020:334.132 - 0.434ms returns FALSE
T3234 020:334.189 JLINK_IsHalted()
T3234 020:334.583 - 0.423ms returns FALSE
T3234 020:443.737 JLINK_IsHalted()
T3234 020:444.137 - 0.429ms returns FALSE
T3234 020:444.194 JLINK_IsHalted()
T3234 020:444.575 - 0.424ms returns FALSE
T3234 020:552.341 JLINK_IsHalted()
T3234 020:552.727 - 0.436ms returns FALSE
T3234 020:552.816 JLINK_IsHalted()
T3234 020:553.142 - 0.372ms returns FALSE
T3234 020:662.257 JLINK_IsHalted()
T3234 020:662.657 - 0.429ms returns FALSE
T3234 020:662.714 JLINK_IsHalted()
T3234 020:663.037 - 0.362ms returns FALSE
T3234 020:771.224 JLINK_IsHalted()
T3234 020:771.636 - 0.449ms returns FALSE
T3234 020:771.703 JLINK_IsHalted()
T3234 020:772.107 - 0.435ms returns FALSE
T2498 020:820.485 JLINK_IsHalted()
T2498 020:820.902 - 0.446ms returns FALSE
T2498 020:820.960 JLINK_IsHalted()
T2498 020:821.277 - 1.599ms returns FALSE
T3234 020:880.877 JLINK_IsHalted()
T3234 020:881.292 - 0.446ms returns FALSE
T3234 020:881.350 JLINK_IsHalted()
T3234 020:881.706 - 0.386ms returns FALSE
T3234 020:989.793 JLINK_IsHalted()
T3234 020:990.200 - 0.437ms returns FALSE
T3234 020:990.258 JLINK_IsHalted()
T3234 020:990.625 - 0.405ms returns FALSE
T3234 021:099.876 JLINK_IsHalted()
T3234 021:100.257 - 0.411ms returns FALSE
T3234 021:100.315 JLINK_IsHalted()
T3234 021:100.690 - 0.401ms returns FALSE
T3234 021:208.462 JLINK_IsHalted()
T3234 021:208.871 - 0.438ms returns FALSE
T3234 021:208.928 JLINK_IsHalted()
T3234 021:209.251 - 0.361ms returns FALSE
T3234 021:318.251 JLINK_IsHalted()
T3234 021:318.683 - 0.480ms returns FALSE
T3234 021:318.760 JLINK_IsHalted()
T3234 021:319.093 - 0.372ms returns FALSE
T3234 021:427.178 JLINK_IsHalted()
T3234 021:427.572 - 0.423ms returns FALSE
T3234 021:427.629 JLINK_IsHalted()
T3234 021:428.018 - 0.418ms returns FALSE
T3234 021:537.102 JLINK_IsHalted()
T3234 021:537.492 - 0.420ms returns FALSE
T3234 021:537.550 JLINK_IsHalted()
T3234 021:537.900 - 0.380ms returns FALSE
T3234 021:645.972 JLINK_IsHalted()
T3234 021:646.369 - 0.427ms returns FALSE
T3234 021:646.427 JLINK_IsHalted()
T3234 021:646.787 - 0.390ms returns FALSE
T3234 021:755.686 JLINK_IsHalted()
T3234 021:756.108 - 0.458ms returns FALSE
T3234 021:756.194 JLINK_IsHalted()
T3234 021:756.533 - 0.377ms returns FALSE
T2498 021:822.896 JLINK_IsHalted()
T2498 021:823.308 - 0.471ms returns FALSE
T2498 021:823.401 JLINK_IsHalted()
T2498 021:823.754 - 0.393ms returns FALSE
T3234 021:864.691 JLINK_IsHalted()
T3234 021:865.110 - 0.446ms returns FALSE
T3234 021:865.165 JLINK_IsHalted()
T3234 021:865.471 - 0.345ms returns FALSE
T3234 021:974.197 JLINK_IsHalted()
T3234 021:974.540 - 0.380ms returns FALSE
T3234 021:974.608 JLINK_IsHalted()
T3234 021:974.908 - 0.335ms returns FALSE
T3234 022:084.227 JLINK_IsHalted()
T3234 022:084.634 - 0.436ms returns FALSE
T3234 022:084.691 JLINK_IsHalted()
T3234 022:085.016 - 0.364ms returns FALSE
T3234 022:193.025 JLINK_IsHalted()
T3234 022:193.428 - 0.432ms returns FALSE
T3234 022:193.485 JLINK_IsHalted()
T3234 022:193.847 - 0.401ms returns FALSE
T3234 022:303.018 JLINK_IsHalted()
T3234 022:303.437 - 0.449ms returns FALSE
T3234 022:303.495 JLINK_IsHalted()
T3234 022:303.845 - 0.395ms returns FALSE
T3234 022:412.070 JLINK_IsHalted()
T3234 022:412.448 - 0.430ms returns FALSE
T3234 022:412.532 JLINK_IsHalted()
T3234 022:412.861 - 0.372ms returns FALSE
T3234 022:521.585 JLINK_IsHalted()
T3234 022:521.992 - 0.436ms returns FALSE
T3234 022:522.049 JLINK_IsHalted()
T3234 022:522.387 - 0.368ms returns FALSE
T3234 022:630.479 JLINK_IsHalted()
T3234 022:630.896 - 0.447ms returns FALSE
T3234 022:630.954 JLINK_IsHalted()
T3234 022:631.330 - 0.406ms returns FALSE
T3234 022:740.356 JLINK_IsHalted()
T3234 022:740.762 - 0.436ms returns FALSE
T3234 022:740.820 JLINK_IsHalted()
T3234 022:741.180 - 0.389ms returns FALSE
T2498 022:824.584 JLINK_IsHalted()
T2498 022:824.961 - 0.425ms returns FALSE
T2498 022:825.057 JLINK_IsHalted()
T2498 022:825.412 - 0.388ms returns FALSE
T3234 022:849.262 JLINK_IsHalted()
T3234 022:849.664 - 0.432ms returns FALSE
T3234 022:849.721 JLINK_IsHalted()
T3234 022:850.063 - 0.371ms returns FALSE
T3234 022:959.122 JLINK_IsHalted()
T3234 022:959.499 - 0.406ms returns FALSE
T3234 022:959.556 JLINK_IsHalted()
T3234 022:959.963 - 0.455ms returns FALSE
T3234 023:068.786 JLINK_IsHalted()
T3234 023:069.198 - 0.441ms returns FALSE
T3234 023:069.255 JLINK_IsHalted()
T3234 023:069.613 - 0.402ms returns FALSE
T3234 023:177.627 JLINK_IsHalted()
T3234 023:178.029 - 0.432ms returns FALSE
T3234 023:178.087 JLINK_IsHalted()
T3234 023:178.450 - 0.402ms returns FALSE
T3234 023:286.572 JLINK_IsHalted()
T3234 023:286.978 - 0.435ms returns FALSE
T3234 023:287.036 JLINK_IsHalted()
T3234 023:287.395 - 0.389ms returns FALSE
T3234 023:395.950 JLINK_IsHalted()
T3234 023:396.361 - 0.447ms returns FALSE
T3234 023:396.425 JLINK_IsHalted()
T3234 023:396.773 - 0.384ms returns FALSE
T3234 023:506.189 JLINK_IsHalted()
T3234 023:506.595 - 0.436ms returns FALSE
T3234 023:506.653 JLINK_IsHalted()
T3234 023:507.098 - 0.481ms returns FALSE
T3234 023:615.017 JLINK_IsHalted()
T3234 023:615.424 - 0.436ms returns FALSE
T3234 023:615.481 JLINK_IsHalted()
T3234 023:615.878 - 0.438ms returns FALSE
T3234 023:724.936 JLINK_IsHalted()
T3234 023:725.352 - 0.445ms returns FALSE
T3234 023:725.409 JLINK_IsHalted()
T3234 023:725.769 - 0.389ms returns FALSE
T2498 023:826.211 JLINK_IsHalted()
T2498 023:826.634 - 0.464ms returns FALSE
T2498 023:826.706 JLINK_IsHalted()
T2498 023:827.048 - 0.388ms returns FALSE
T3234 023:833.889 JLINK_IsHalted()
T3234 023:834.297 - 0.440ms returns FALSE
T3234 023:834.357 JLINK_IsHalted()
T3234 023:834.687 - 0.360ms returns FALSE
T3234 023:942.730 JLINK_IsHalted()
T3234 023:943.087 - 0.391ms returns FALSE
T3234 023:943.150 JLINK_IsHalted()
T3234 023:943.455 - 0.337ms returns FALSE
T3234 024:052.179 JLINK_IsHalted()
T3234 024:052.598 - 0.460ms returns FALSE
T3234 024:052.671 JLINK_IsHalted()
T3234 024:053.009 - 0.367ms returns FALSE
T3234 024:162.273 JLINK_IsHalted()
T3234 024:162.643 - 0.415ms returns FALSE
T3234 024:162.722 JLINK_IsHalted()
T3234 024:163.054 - 0.375ms returns FALSE
T3234 024:271.132 JLINK_IsHalted()
T3234 024:271.535 - 0.432ms returns FALSE
T3234 024:271.592 JLINK_IsHalted()
T3234 024:271.985 - 0.438ms returns FALSE
T3234 024:381.062 JLINK_IsHalted()
T3234 024:381.435 - 0.421ms returns FALSE
T3234 024:381.516 JLINK_IsHalted()
T3234 024:381.853 - 0.371ms returns FALSE
T3234 024:490.000 JLINK_IsHalted()
T3234 024:490.450 - 0.510ms returns FALSE
T3234 024:490.558 JLINK_IsHalted()
T3234 024:490.895 - 0.391ms returns FALSE
T3234 024:599.955 JLINK_IsHalted()
T3234 024:600.366 - 0.476ms returns FALSE
T3234 024:600.468 JLINK_IsHalted()
T3234 024:600.782 - 0.352ms returns FALSE
T3234 024:708.858 JLINK_IsHalted()
T3234 024:709.245 - 0.435ms returns FALSE
T3234 024:709.330 JLINK_IsHalted()
T3234 024:709.655 - 0.366ms returns FALSE
T3234 024:817.813 JLINK_IsHalted()
T3234 024:818.139 - 0.362ms returns FALSE
T3234 024:818.207 JLINK_IsHalted()
T3234 024:818.512 - 0.340ms returns FALSE
T2498 024:828.138 JLINK_IsHalted()
T2498 024:828.516 - 0.420ms returns FALSE
T2498 024:828.589 JLINK_IsHalted()
T2498 024:828.922 - 0.370ms returns FALSE
T3234 024:927.765 JLINK_IsHalted()
T3234 024:928.170 - 0.457ms returns FALSE
T3234 024:928.265 JLINK_IsHalted()
T3234 024:928.572 - 0.360ms returns FALSE
T3234 025:036.743 JLINK_IsHalted()
T3234 025:037.158 - 0.460ms returns FALSE
T3234 025:037.236 JLINK_IsHalted()
T3234 025:037.556 - 0.356ms returns FALSE
T3234 025:146.728 JLINK_IsHalted()
T3234 025:147.170 - 0.484ms returns FALSE
T3234 025:147.241 JLINK_IsHalted()
T3234 025:147.591 - 0.403ms returns FALSE
T3234 025:255.704 JLINK_IsHalted()
T3234 025:256.104 - 0.430ms returns FALSE
T3234 025:256.162 JLINK_IsHalted()
T3234 025:256.496 - 0.378ms returns FALSE
T3234 025:365.560 JLINK_IsHalted()
T3234 025:365.990 - 0.460ms returns FALSE
T3234 025:366.048 JLINK_IsHalted()
T3234 025:366.375 - 0.366ms returns FALSE
T3234 025:474.414 JLINK_IsHalted()
T3234 025:474.811 - 0.427ms returns FALSE
T3234 025:474.868 JLINK_IsHalted()
T3234 025:475.228 - 0.398ms returns FALSE
T3234 025:583.360 JLINK_IsHalted()
T3234 025:583.764 - 0.434ms returns FALSE
T3234 025:583.821 JLINK_IsHalted()
T3234 025:584.162 - 0.370ms returns FALSE
T3234 025:693.218 JLINK_IsHalted()
T3234 025:693.601 - 0.421ms returns FALSE
T3234 025:693.668 JLINK_IsHalted()
T3234 025:693.993 - 0.361ms returns FALSE
T3234 025:802.749 JLINK_IsHalted()
T3234 025:803.085 - 0.381ms returns FALSE
T3234 025:803.168 JLINK_IsHalted()
T3234 025:803.457 - 0.323ms returns FALSE
T2498 025:830.174 JLINK_IsHalted()
T2498 025:830.583 - 0.470ms returns FALSE
T2498 025:830.690 JLINK_IsHalted()
T2498 025:831.021 - 0.369ms returns FALSE
T3234 025:911.725 JLINK_IsHalted()
T3234 025:912.141 - 0.455ms returns FALSE
T3234 025:912.207 JLINK_IsHalted()
T3234 025:912.559 - 0.388ms returns FALSE
T3234 026:021.702 JLINK_IsHalted()
T3234 026:022.106 - 0.433ms returns FALSE
T3234 026:022.163 JLINK_IsHalted()
T3234 026:022.508 - 0.374ms returns FALSE
T3234 026:130.670 JLINK_IsHalted()
T3234 026:131.052 - 0.414ms returns FALSE
T3234 026:131.112 JLINK_IsHalted()
T3234 026:131.444 - 0.359ms returns FALSE
T3234 026:239.649 JLINK_IsHalted()
T3234 026:240.028 - 0.431ms returns FALSE
T3234 026:240.111 JLINK_IsHalted()
T3234 026:240.429 - 0.354ms returns FALSE
T3234 026:349.047 JLINK_IsHalted()
T3234 026:349.504 - 0.628ms returns FALSE
T3234 026:349.771 JLINK_IsHalted()
T3234 026:350.197 - 0.456ms returns FALSE
T3234 026:458.526 JLINK_IsHalted()
T3234 026:458.891 - 0.406ms returns FALSE
T3234 026:458.964 JLINK_IsHalted()
T3234 026:459.271 - 0.340ms returns FALSE
T3234 026:568.470 JLINK_IsHalted()
T3234 026:568.854 - 0.423ms returns FALSE
T3234 026:568.921 JLINK_IsHalted()
T3234 026:569.225 - 0.335ms returns FALSE
T3234 026:677.670 JLINK_IsHalted()
T3234 026:678.112 - 0.476ms returns FALSE
T3234 026:678.174 JLINK_IsHalted()
T3234 026:678.503 - 0.368ms returns FALSE
T3234 026:786.493 JLINK_IsHalted()
T3234 026:786.875 - 0.424ms returns FALSE
T3234 026:786.950 JLINK_IsHalted()
T3234 026:787.262 - 0.350ms returns FALSE
T2498 026:831.874 JLINK_IsHalted()
T2498 026:832.244 - 0.401ms returns FALSE
T2498 026:832.304 JLINK_IsHalted()
T2498 026:832.614 - 0.341ms returns FALSE
T3234 026:896.458 JLINK_IsHalted()
T3234 026:896.891 - 0.490ms returns FALSE
T3234 026:896.991 JLINK_IsHalted()
T3234 026:897.318 - 0.385ms returns FALSE
T3234 027:005.396 JLINK_IsHalted()
T3234 027:005.729 - 0.370ms returns FALSE
T3234 027:005.803 JLINK_IsHalted()
T3234 027:006.107 - 0.339ms returns FALSE
T3234 027:115.354 JLINK_IsHalted()
T3234 027:115.726 - 0.411ms returns FALSE
T3234 027:115.795 JLINK_IsHalted()
T3234 027:116.145 - 0.381ms returns FALSE
T3234 027:224.231 JLINK_IsHalted()
T3234 027:224.580 - 0.388ms returns FALSE
T3234 027:224.667 JLINK_IsHalted()
T3234 027:224.970 - 0.332ms returns FALSE
T2C60 027:737.498 JLINK_Halt()
T2C60 027:740.085 - 2.659ms returns 0x00
T2C60 027:740.200 JLINK_ReadReg(XPSR)
T2C60 027:740.554   CPU_ReadMem(4 bytes @ 0xE000EE08)
T2C60 027:740.888 - 0.769ms returns 0x69000000
T2C60 027:757.589 JLINK_Close()
T2C60 027:834.042 - 76.530ms
T2C60 027:834.200   
T2C60 027:834.361   Closed
