  AppVersion = 78206
  FileVersion = 2
[GENERAL]
  aATEModuleSel[24] = 0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
  ConnectMode = 0
  CurrentFile = "C:\Users\T.Uemitsu\e2_studio\workspace\bootloader\Release\bootloader.elf"
  DataFileSAddr = 0x00000000
  GUIMode = 0
  HostName = ""
  TargetIF = 1
  USBPort = 0
  USBSerialNo = 0x00000000
  UseATEModuleSelection = 0
[JTAG]
  IRLen = 0
  MultipleTargets = 0
  NumDevices = 0
  Speed0 = 4000
  Speed1 = 4000
  TAP_Number = 0
  UseAdaptive0 = 0
  UseAdaptive1 = 0
  UseMaxSpeed0 = 0
  UseMaxSpeed1 = 0
[CPU]
  NumInitSteps = 1
  InitStep0_Action = "Reset"
  InitStep0_Value0 = 0x00000000
  InitStep0_Value1 = 0x00000000
  InitStep0_Comment = "Reset and halt target"
  NumExitSteps = 0
  UseScriptFile = 0
  ScriptFile = ""
  UseRAM = 1
  RAMAddr = 0x2000D000
  RAMSize = 0x00003000
  CheckCoreID = 1
  CoreID = 0x6BA02477
  CoreIDMask = 0x0F000FFF
  UseAutoSpeed = 0x00000001
  ClockSpeed = 0x00000000
  EndianMode = 0
  ChipName = "Renesas R7FA4M2AC"
[FLASH]
  NumBanks = 4
[FLASH0]
  aRangeSel[1] = 0-31
  BankName = "Internal option-setting memory"
  BankSelMode = 1
  BaseAddr = 0x0100A100
[FLASH1]
  aRangeSel[1] = 0-17
  BankName = "Internal program flash"
  BankSelMode = 1
  BaseAddr = 0x00000000
[FLASH2]
  aRangeSel[1] = 0-127
  BankName = "Internal data flash"
  BankSelMode = 1
  BaseAddr = 0x08000000
[FLASH3]
  aRangeSel[0] = 
  BankName = "External QSPI flash"
  BankSelMode = 1
  BaseAddr = 0x60000000
  LoaderName = "CLK@P305_nCS@P306_D0@P307_D1@P503_D2@P104_D3@P505"
[PRODUCTION]
  AutoPerformsDisconnect = 0
  AutoPerformsErase = 1
  AutoPerformsProgram = 1
  AutoPerformsSecure = 0
  AutoPerformsStartApp = 1
  AutoPerformsVerify = 1
  EnableFixedVTref = 0
  EnableTargetPower = 0
  EraseType = 1
  FixedVTref = 0x00000CE4
  MonitorVTref = 0
  MonitorVTrefMax = 0x0000157C
  MonitorVTrefMin = 0x000003E8
  OverrideTimeouts = 0
  ProgramSN = 0
  SerialFile = ""
  SNAddr = 0x00000000
  SNInc = 0x00000001
  SNLen = 0x00000004
  SNListFile = ""
  SNValue = 0x00000001
  StartAppType = 0
  TargetPowerDelay = 0x00000014
  TimeoutErase = 0x00003A98
  TimeoutProgram = 0x00002710
  TimeoutVerify = 0x00002710
  VerifyType = 1
[PERFORMANCE]
  DisableSkipBlankDataOnProgram = 0x00000000
  PerfromBlankCheckPriorEraseChip = 0x00000001
  PerfromBlankCheckPriorEraseSelectedSectors = 0x00000001
