T1EFC 000:002.586   SEGGER J-Link V7.86b Log File
T1EFC 000:002.869   DLL Compiled: Mar  1 2023 16:53:12
T1EFC 000:002.915   Logging started @ 2023-05-05 06:54
T1EFC 000:002.958 - 2.980ms
T1EFC 000:003.014 JLINK_GetDLLVersion()
T1EFC 000:003.061 - 0.069ms returns 78602
T1EFC 000:005.265 JLINK_OpenEx(...)
T1EFC 000:021.808   Firmware: J-Link V11 compiled Mar 28 2023 16:59:55
T1EFC 000:022.224   Firmware: J-Link V11 compiled Mar 28 2023 16:59:55
T1EFC 000:026.166   Hardware: V11.00
T1EFC 000:026.280   S/N: 851005873
T1EFC 000:026.361   OEM: SEGGER
T1EFC 000:026.428   Feature(s): RDI, FlashBP, FlashDL, JFlash, GDB
T1EFC 000:029.933   USB speed mode: High speed (480 MBit/s)
T1EFC 000:030.383   TELNET listener socket opened on port 19021
T1EFC 000:031.004   WEBSRV WEBSRV_Init(): Starting webserver thread(s)
T1EFC 000:031.498   WEBSRV Webserver running on local port 19080
T1EFC 000:504.956 - 499.786ms returns "O.K."
T1EFC 000:505.467 JLINK_ExecCommand("ProjectFile=C:\Users\T.Uemitsu\e2_studio\workspace\usb_bootloader/usb_bootloader.elf.jlink", ...). 
T1EFC 000:529.804 - 24.384ms returns 0x00
T1EFC 000:531.207 JLINK_ExecCommand("device=R7FA4M2AD", ...). 
T1EFC 000:531.729   Flash bank @ 0x60000000: SFL: Parsing sectorization info from ELF file
T1EFC 000:531.805     FlashDevice.SectorInfo[0]: .SectorSize = 0x00010000, .SectorStartAddr = 0x00000000
T1EFC 000:531.878   OFL: Init() N/A
T1EFC 000:531.945   OFL: UnInit() N/A
T1EFC 000:532.010   OFL: EraseSector() N/A
T1EFC 000:532.074   OFL: ProgramPage() N/A
T1EFC 000:532.139   OFL: EraseChip() N/A
T1EFC 000:532.204   OFL: BlankCheck() N/A
T1EFC 000:532.268   OFL: Verify() N/A
T1EFC 000:532.334   OFL: SEGGER_FL_Erase() present @ offset 0x000004DD
T1EFC 000:532.400   OFL: SEGGER_FL_Program() present @ offset 0x000004C1
T1EFC 000:532.465   OFL: SEGGER_FL_Read() N/A
T1EFC 000:532.530   OFL: SEGGER_OPEN_Read() N/A
T1EFC 000:532.607   OFL: SEGGER_FL_CalcCRC() present @ offset 0x00000505
T1EFC 000:532.693   OFL: SEGGER_FL_Start() present @ offset 0x0000051D
T1EFC 000:532.759   OFL: SEGGER_FL_GetFlashInfo() present @ offset 0x000001B9
T1EFC 000:532.827   OFL: SEGGER_FL_Verify() N/A
T1EFC 000:532.907   OFL: SEGGER_FL_CheckBlank() present @ offset 0x000004F1
T1EFC 000:532.971   OFL: SEGGER_FL_Prepare() present @ offset 0x000001DD
T1EFC 000:533.036   OFL: SEGGER_FL_Restore() present @ offset 0x0000038D
T1EFC 000:533.101   OFL: SEGGER_FL_EraseChip() N/A
T1EFC 000:537.454   Device "R7FA4M2AD" selected.
T1EFC 000:539.756 - 8.535ms returns 0x00
T1EFC 000:539.889 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 000:540.200   ConfigTargetSettings() start
T1EFC 000:540.296    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 000:540.341   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 000:614.613   ConfigTargetSettings() end - Took 74ms
T1EFC 000:615.847   InitTarget() start
T1EFC 000:615.943    J-Link Script File: Executing InitTarget()
T1EFC 000:615.991   JTAG selected. Identifying JTAG Chain...
T1EFC 000:617.365   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 000:617.928   Error: Scanning JTAG chain failed.
T1EFC 000:618.003   InitTarget() end - Took 2ms
T1EFC 000:618.068   Connect failed. Resetting via Reset pin and trying again.
T1EFC 000:680.710   ConfigTargetSettings() start
T1EFC 000:680.853    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 000:680.912   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 000:787.052   ConfigTargetSettings() end - Took 106ms
T1EFC 000:787.146   InitTarget() start
T1EFC 000:787.215    J-Link Script File: Executing InitTarget()
T1EFC 000:787.263   JTAG selected. Identifying JTAG Chain...
T1EFC 000:788.635   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 000:789.126   Error: Scanning JTAG chain failed.
T1EFC 000:789.209   InitTarget() end - Took 2ms
T1EFC 000:789.278 - 249.411ms returns 1
T1EFC 000:789.395 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T1EFC 000:789.874   ConfigTargetSettings() start
T1EFC 000:789.972    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 000:790.034   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 000:864.492   ConfigTargetSettings() end - Took 74ms
T1EFC 000:864.578   InitTarget() start
T1EFC 000:864.644    J-Link Script File: Executing InitTarget()
T1EFC 000:864.690   JTAG selected. Identifying JTAG Chain...
T1EFC 000:865.996   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 000:866.472   Error: Scanning JTAG chain failed.
T1EFC 000:866.547   InitTarget() end - Took 1ms
T1EFC 000:866.631   Connect failed. Resetting via Reset pin and trying again.
T1EFC 000:928.811   ConfigTargetSettings() start
T1EFC 000:928.932    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 000:928.976   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 001:031.198   ConfigTargetSettings() end - Took 102ms
T1EFC 001:031.312   InitTarget() start
T1EFC 001:031.404    J-Link Script File: Executing InitTarget()
T1EFC 001:031.467   JTAG selected. Identifying JTAG Chain...
T1EFC 001:032.754   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 001:033.249   Error: Scanning JTAG chain failed.
T1EFC 001:033.353   InitTarget() end - Took 2ms
T1EFC 001:033.441 - 244.076ms returns 1
T1EFC 001:033.563 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 001:033.797   ConfigTargetSettings() start
T1EFC 001:033.905    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 001:033.973   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 001:154.074   ConfigTargetSettings() end - Took 119ms
T1EFC 001:154.594   InitTarget() start
T1EFC 001:154.714    J-Link Script File: Executing InitTarget()
T1EFC 001:154.829   JTAG selected. Identifying JTAG Chain...
T1EFC 001:170.981   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 001:182.447   Error: Scanning JTAG chain failed.
T1EFC 001:182.623   InitTarget() end - Took 28ms
T1EFC 001:182.734   Connect failed. Resetting via Reset pin and trying again.
T1EFC 001:294.427   ConfigTargetSettings() start
T1EFC 001:294.571    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 001:294.664   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 001:534.443   ConfigTargetSettings() end - Took 240ms
T1EFC 001:534.572   InitTarget() start
T1EFC 001:534.672    J-Link Script File: Executing InitTarget()
T1EFC 001:534.739   JTAG selected. Identifying JTAG Chain...
T1EFC 001:541.846   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 001:545.614   Error: Scanning JTAG chain failed.
T1EFC 001:546.520   InitTarget() end - Took 11ms
T1EFC 001:546.636 - 513.103ms returns 1
T1EFC 001:546.785 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 001:547.057   ConfigTargetSettings() start
T1EFC 001:547.164    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 001:547.242   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 001:676.919   ConfigTargetSettings() end - Took 130ms
T1EFC 001:677.038   InitTarget() start
T1EFC 001:677.131    J-Link Script File: Executing InitTarget()
T1EFC 001:677.196   JTAG selected. Identifying JTAG Chain...
T1EFC 001:687.342   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 001:689.205   Error: Scanning JTAG chain failed.
T1EFC 001:689.386   InitTarget() end - Took 12ms
T1EFC 001:689.525   Connect failed. Resetting via Reset pin and trying again.
T1EFC 001:768.687   ConfigTargetSettings() start
T1EFC 001:769.002    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 001:769.241   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 001:918.178   ConfigTargetSettings() end - Took 149ms
T1EFC 001:918.285   InitTarget() start
T1EFC 001:918.371    J-Link Script File: Executing InitTarget()
T1EFC 001:918.433   JTAG selected. Identifying JTAG Chain...
T1EFC 001:920.821   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 001:921.718   Error: Scanning JTAG chain failed.
T1EFC 001:921.899   InitTarget() end - Took 4ms
T1EFC 001:922.045 - 375.315ms returns 1
T1EFC 001:922.158 JLINK_ReadMem(0x400E001C, 0x4 Bytes, ...)
T1EFC 001:924.380   ConfigTargetSettings() start
T1EFC 001:924.523    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 001:924.606   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 002:095.283   ConfigTargetSettings() end - Took 171ms
T1EFC 002:095.398   InitTarget() start
T1EFC 002:095.491    J-Link Script File: Executing InitTarget()
T1EFC 002:095.555   JTAG selected. Identifying JTAG Chain...
T1EFC 002:096.917   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 002:097.473   Error: Scanning JTAG chain failed.
T1EFC 002:097.607   InitTarget() end - Took 2ms
T1EFC 002:097.702   Connect failed. Resetting via Reset pin and trying again.
T1EFC 002:159.999   ConfigTargetSettings() start
T1EFC 002:161.408    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 002:162.146   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 002:283.149   ConfigTargetSettings() end - Took 122ms
T1EFC 002:283.234   InitTarget() start
T1EFC 002:283.303    J-Link Script File: Executing InitTarget()
T1EFC 002:283.350   JTAG selected. Identifying JTAG Chain...
T1EFC 002:284.756   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 002:285.195   Error: Scanning JTAG chain failed.
T1EFC 002:285.270   InitTarget() end - Took 2ms
T1EFC 002:285.337 - 363.201ms returns 1
T1EFC 002:285.627 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 002:286.037   ConfigTargetSettings() start
T1EFC 002:286.110    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 002:286.156   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 002:361.227   ConfigTargetSettings() end - Took 75ms
T1EFC 002:361.309   InitTarget() start
T1EFC 002:361.376    J-Link Script File: Executing InitTarget()
T1EFC 002:361.422   JTAG selected. Identifying JTAG Chain...
T1EFC 002:362.918   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 002:363.382   Error: Scanning JTAG chain failed.
T1EFC 002:363.460   InitTarget() end - Took 3ms
T1EFC 002:363.527   Connect failed. Resetting via Reset pin and trying again.
T1EFC 002:424.980   ConfigTargetSettings() start
T1EFC 002:425.113    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 002:425.164   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 002:511.131   ConfigTargetSettings() end - Took 86ms
T1EFC 002:511.231   InitTarget() start
T1EFC 002:511.300    J-Link Script File: Executing InitTarget()
T1EFC 002:511.347   JTAG selected. Identifying JTAG Chain...
T1EFC 002:512.688   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 002:513.195   Error: Scanning JTAG chain failed.
T1EFC 002:513.282   InitTarget() end - Took 2ms
T1EFC 002:513.349 - 227.752ms returns 1
T1EFC 002:513.491 JLINK_ReadMem(0x400E0018, 0x4 Bytes, ...)
T1EFC 002:513.741   ConfigTargetSettings() start
T1EFC 002:513.838    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 002:513.885   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 002:603.102   ConfigTargetSettings() end - Took 90ms
T1EFC 002:603.211   InitTarget() start
T1EFC 002:603.294    J-Link Script File: Executing InitTarget()
T1EFC 002:603.354   JTAG selected. Identifying JTAG Chain...
T1EFC 002:604.651   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 002:605.157   Error: Scanning JTAG chain failed.
T1EFC 002:605.258   InitTarget() end - Took 2ms
T1EFC 002:605.343   Connect failed. Resetting via Reset pin and trying again.
T1EFC 002:667.563   ConfigTargetSettings() start
T1EFC 002:667.703    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 002:667.754   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 002:779.248   ConfigTargetSettings() end - Took 111ms
T1EFC 002:779.350   InitTarget() start
T1EFC 002:779.437    J-Link Script File: Executing InitTarget()
T1EFC 002:779.500   JTAG selected. Identifying JTAG Chain...
T1EFC 002:780.772   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 002:781.262   Error: Scanning JTAG chain failed.
T1EFC 002:781.359   InitTarget() end - Took 2ms
T1EFC 002:781.445 - 267.984ms returns 1
T1EFC 002:781.583 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 002:781.813   ConfigTargetSettings() start
T1EFC 002:781.905    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 002:781.964   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 002:858.886   ConfigTargetSettings() end - Took 77ms
T1EFC 002:859.002   InitTarget() start
T1EFC 002:859.094    J-Link Script File: Executing InitTarget()
T1EFC 002:859.158   JTAG selected. Identifying JTAG Chain...
T1EFC 002:860.774   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 002:861.320   Error: Scanning JTAG chain failed.
T1EFC 002:861.460   InitTarget() end - Took 3ms
T1EFC 002:861.553   Connect failed. Resetting via Reset pin and trying again.
T1EFC 002:923.394   ConfigTargetSettings() start
T1EFC 002:923.633    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 002:923.741   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 002:996.649   ConfigTargetSettings() end - Took 72ms
T1EFC 002:996.737   InitTarget() start
T1EFC 002:996.806    J-Link Script File: Executing InitTarget()
T1EFC 002:996.854   JTAG selected. Identifying JTAG Chain...
T1EFC 002:998.259   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 002:998.770   Error: Scanning JTAG chain failed.
T1EFC 002:998.852   InitTarget() end - Took 2ms
T1EFC 002:998.920 - 217.360ms returns 1
T1EFC 002:999.038 JLINK_ReadMem(0x400E0020, 0x4 Bytes, ...)
T1EFC 002:999.237   ConfigTargetSettings() start
T1EFC 002:999.312    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 002:999.391   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 003:068.529   ConfigTargetSettings() end - Took 70ms
T1EFC 003:068.638   InitTarget() start
T1EFC 003:068.726    J-Link Script File: Executing InitTarget()
T1EFC 003:068.787   JTAG selected. Identifying JTAG Chain...
T1EFC 003:070.127   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 003:070.672   Error: Scanning JTAG chain failed.
T1EFC 003:070.770   InitTarget() end - Took 2ms
T1EFC 003:070.855   Connect failed. Resetting via Reset pin and trying again.
T1EFC 003:132.532   ConfigTargetSettings() start
T1EFC 003:132.682    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 003:132.741   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 003:201.832   ConfigTargetSettings() end - Took 69ms
T1EFC 003:201.945   InitTarget() start
T1EFC 003:202.037    J-Link Script File: Executing InitTarget()
T1EFC 003:202.102   JTAG selected. Identifying JTAG Chain...
T1EFC 003:203.419   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 003:204.301   Error: Scanning JTAG chain failed.
T1EFC 003:204.431   InitTarget() end - Took 2ms
T1EFC 003:204.525 - 205.516ms returns 1
T1EFC 003:204.656 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 003:204.996   ConfigTargetSettings() start
T1EFC 003:205.096    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 003:205.154   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 003:265.473   ConfigTargetSettings() end - Took 61ms
T1EFC 003:265.596   InitTarget() start
T1EFC 003:265.684    J-Link Script File: Executing InitTarget()
T1EFC 003:265.745   JTAG selected. Identifying JTAG Chain...
T1EFC 003:267.112   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 003:267.564   Error: Scanning JTAG chain failed.
T1EFC 003:267.645   InitTarget() end - Took 2ms
T1EFC 003:267.714   Connect failed. Resetting via Reset pin and trying again.
T1EFC 003:329.339   ConfigTargetSettings() start
T1EFC 003:329.492    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 003:329.540   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 003:382.115   ConfigTargetSettings() end - Took 53ms
T1EFC 003:382.194   InitTarget() start
T1EFC 003:382.260    J-Link Script File: Executing InitTarget()
T1EFC 003:382.305   JTAG selected. Identifying JTAG Chain...
T1EFC 003:383.767   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 003:384.382   Error: Scanning JTAG chain failed.
T1EFC 003:384.498   InitTarget() end - Took 2ms
T1EFC 003:384.563 - 179.928ms returns 1
T1EFC 003:384.634 JLINK_ReadMem(0x400E0028, 0x4 Bytes, ...)
T1EFC 003:384.947   ConfigTargetSettings() start
T1EFC 003:385.022    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 003:385.066   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 003:434.805   ConfigTargetSettings() end - Took 49ms
T1EFC 003:434.883   InitTarget() start
T1EFC 003:434.954    J-Link Script File: Executing InitTarget()
T1EFC 003:435.000   JTAG selected. Identifying JTAG Chain...
T1EFC 003:436.762   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 003:437.414   Error: Scanning JTAG chain failed.
T1EFC 003:437.531   InitTarget() end - Took 2ms
T1EFC 003:437.596   Connect failed. Resetting via Reset pin and trying again.
T1EFC 003:499.292   ConfigTargetSettings() start
T1EFC 003:499.480    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 003:499.554   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 003:562.695   ConfigTargetSettings() end - Took 63ms
T1EFC 003:562.808   InitTarget() start
T1EFC 003:562.900    J-Link Script File: Executing InitTarget()
T1EFC 003:562.964   JTAG selected. Identifying JTAG Chain...
T1EFC 003:564.532   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 003:565.048   Error: Scanning JTAG chain failed.
T1EFC 003:565.154   InitTarget() end - Took 2ms
T1EFC 003:565.242 - 180.635ms returns 1
T1EFC 003:565.882 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 003:566.115   ConfigTargetSettings() start
T1EFC 003:566.264    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 003:566.371   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 003:630.155   ConfigTargetSettings() end - Took 63ms
T1EFC 003:630.240   InitTarget() start
T1EFC 003:630.307    J-Link Script File: Executing InitTarget()
T1EFC 003:630.353   JTAG selected. Identifying JTAG Chain...
T1EFC 003:631.616   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 003:632.087   Error: Scanning JTAG chain failed.
T1EFC 003:632.161   InitTarget() end - Took 2ms
T1EFC 003:632.227   Connect failed. Resetting via Reset pin and trying again.
T1EFC 003:693.461   ConfigTargetSettings() start
T1EFC 003:693.589    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 003:693.634   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 003:743.513   ConfigTargetSettings() end - Took 50ms
T1EFC 003:743.598   InitTarget() start
T1EFC 003:743.664    J-Link Script File: Executing InitTarget()
T1EFC 003:743.710   JTAG selected. Identifying JTAG Chain...
T1EFC 003:745.131   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 003:745.762   Error: Scanning JTAG chain failed.
T1EFC 003:745.870   InitTarget() end - Took 1ms
T1EFC 003:745.935 - 180.075ms returns 1
T1EFC 003:746.006 JLINK_ReadMem(0x400E0024, 0x4 Bytes, ...)
T1EFC 003:746.293   ConfigTargetSettings() start
T1EFC 003:746.378    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 003:746.423   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 003:795.151   ConfigTargetSettings() end - Took 49ms
T1EFC 003:795.229   InitTarget() start
T1EFC 003:795.294    J-Link Script File: Executing InitTarget()
T1EFC 003:795.339   JTAG selected. Identifying JTAG Chain...
T1EFC 003:796.944   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 003:797.417   Error: Scanning JTAG chain failed.
T1EFC 003:797.497   InitTarget() end - Took 3ms
T1EFC 003:797.562   Connect failed. Resetting via Reset pin and trying again.
T1EFC 003:858.758   ConfigTargetSettings() start
T1EFC 003:858.939    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 003:858.994   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 003:910.780   ConfigTargetSettings() end - Took 52ms
T1EFC 003:910.859   InitTarget() start
T1EFC 003:910.923    J-Link Script File: Executing InitTarget()
T1EFC 003:910.968   JTAG selected. Identifying JTAG Chain...
T1EFC 003:912.416   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 003:913.027   Error: Scanning JTAG chain failed.
T1EFC 003:913.128   InitTarget() end - Took 2ms
T1EFC 003:913.193 - 167.208ms returns 1
T1EFC 003:913.353 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 003:913.642   ConfigTargetSettings() start
T1EFC 003:913.740    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 003:913.795   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 003:967.097   ConfigTargetSettings() end - Took 53ms
T1EFC 003:967.175   InitTarget() start
T1EFC 003:967.240    J-Link Script File: Executing InitTarget()
T1EFC 003:967.285   JTAG selected. Identifying JTAG Chain...
T1EFC 003:968.713   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 003:969.317   Error: Scanning JTAG chain failed.
T1EFC 003:969.422   InitTarget() end - Took 2ms
T1EFC 003:969.487   Connect failed. Resetting via Reset pin and trying again.
T1EFC 004:030.519   ConfigTargetSettings() start
T1EFC 004:030.641    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 004:030.686   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 004:081.774   ConfigTargetSettings() end - Took 50ms
T1EFC 004:081.885   InitTarget() start
T1EFC 004:081.984    J-Link Script File: Executing InitTarget()
T1EFC 004:082.048   JTAG selected. Identifying JTAG Chain...
T1EFC 004:083.391   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 004:083.901   Error: Scanning JTAG chain failed.
T1EFC 004:084.005   InitTarget() end - Took 2ms
T1EFC 004:084.107 - 170.784ms returns 1
T1EFC 004:084.201 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T1EFC 004:084.447   ConfigTargetSettings() start
T1EFC 004:084.532    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 004:084.605   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 004:133.923   ConfigTargetSettings() end - Took 50ms
T1EFC 004:134.002   InitTarget() start
T1EFC 004:134.067    J-Link Script File: Executing InitTarget()
T1EFC 004:134.112   JTAG selected. Identifying JTAG Chain...
T1EFC 004:135.676   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 004:136.292   Error: Scanning JTAG chain failed.
T1EFC 004:136.398   InitTarget() end - Took 2ms
T1EFC 004:136.462   Connect failed. Resetting via Reset pin and trying again.
T1EFC 004:197.518   ConfigTargetSettings() start
T1EFC 004:197.641    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 004:197.686   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 004:247.138   ConfigTargetSettings() end - Took 49ms
T1EFC 004:247.218   InitTarget() start
T1EFC 004:247.283    J-Link Script File: Executing InitTarget()
T1EFC 004:247.328   JTAG selected. Identifying JTAG Chain...
T1EFC 004:248.938   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 004:249.624   Error: Scanning JTAG chain failed.
T1EFC 004:249.745   InitTarget() end - Took 3ms
T1EFC 004:249.810 - 165.630ms returns 1
T1EFC 004:249.889 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 004:250.145   ConfigTargetSettings() start
T1EFC 004:250.231    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 004:250.276   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 004:301.355   ConfigTargetSettings() end - Took 51ms
T1EFC 004:301.434   InitTarget() start
T1EFC 004:301.498    J-Link Script File: Executing InitTarget()
T1EFC 004:301.544   JTAG selected. Identifying JTAG Chain...
T1EFC 004:302.968   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 004:303.600   Error: Scanning JTAG chain failed.
T1EFC 004:303.713   InitTarget() end - Took 3ms
T1EFC 004:303.779   Connect failed. Resetting via Reset pin and trying again.
T1EFC 004:365.451   ConfigTargetSettings() start
T1EFC 004:365.565    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 004:365.610   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 004:416.920   ConfigTargetSettings() end - Took 50ms
T1EFC 004:416.999   InitTarget() start
T1EFC 004:417.064    J-Link Script File: Executing InitTarget()
T1EFC 004:417.109   JTAG selected. Identifying JTAG Chain...
T1EFC 004:418.495   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 004:419.133   Error: Scanning JTAG chain failed.
T1EFC 004:419.246   InitTarget() end - Took 3ms
T1EFC 004:419.310 - 169.442ms returns 1
T1EFC 004:419.380 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T1EFC 004:419.666   ConfigTargetSettings() start
T1EFC 004:419.752    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 004:419.799   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 004:477.573   ConfigTargetSettings() end - Took 58ms
T1EFC 004:477.652   InitTarget() start
T1EFC 004:477.717    J-Link Script File: Executing InitTarget()
T1EFC 004:477.762   JTAG selected. Identifying JTAG Chain...
T1EFC 004:479.162   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 004:479.685   Error: Scanning JTAG chain failed.
T1EFC 004:479.763   InitTarget() end - Took 2ms
T1EFC 004:479.831   Connect failed. Resetting via Reset pin and trying again.
T1EFC 004:541.315   ConfigTargetSettings() start
T1EFC 004:541.461    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 004:541.506   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 004:589.901   ConfigTargetSettings() end - Took 48ms
T1EFC 004:589.980   InitTarget() start
T1EFC 004:590.045    J-Link Script File: Executing InitTarget()
T1EFC 004:590.090   JTAG selected. Identifying JTAG Chain...
T1EFC 004:591.596   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 004:592.236   Error: Scanning JTAG chain failed.
T1EFC 004:592.349   InitTarget() end - Took 3ms
T1EFC 004:592.413 - 173.055ms returns 1
T1EFC 004:592.493 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 004:592.738   ConfigTargetSettings() start
T1EFC 004:592.825    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 004:592.882   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 004:650.752   ConfigTargetSettings() end - Took 57ms
T1EFC 004:650.835   InitTarget() start
T1EFC 004:650.903    J-Link Script File: Executing InitTarget()
T1EFC 004:650.950   JTAG selected. Identifying JTAG Chain...
T1EFC 004:652.280   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 004:652.798   Error: Scanning JTAG chain failed.
T1EFC 004:652.882   InitTarget() end - Took 2ms
T1EFC 004:652.950   Connect failed. Resetting via Reset pin and trying again.
T1EFC 004:727.969   ConfigTargetSettings() start
T1EFC 004:728.091    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 004:728.137   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 004:802.427   ConfigTargetSettings() end - Took 74ms
T1EFC 004:802.511   InitTarget() start
T1EFC 004:802.579    J-Link Script File: Executing InitTarget()
T1EFC 004:802.625   JTAG selected. Identifying JTAG Chain...
T1EFC 004:803.893   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 004:804.360   Error: Scanning JTAG chain failed.
T1EFC 004:804.434   InitTarget() end - Took 2ms
T1EFC 004:804.501 - 212.030ms returns 1
T1EFC 004:804.562 JLINK_ReadMem(0x400E001C, 0x4 Bytes, ...)
T1EFC 004:804.730   ConfigTargetSettings() start
T1EFC 004:804.802    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 004:804.848   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 004:856.006   ConfigTargetSettings() end - Took 51ms
T1EFC 004:856.086   InitTarget() start
T1EFC 004:856.154    J-Link Script File: Executing InitTarget()
T1EFC 004:856.200   JTAG selected. Identifying JTAG Chain...
T1EFC 004:857.509   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 004:857.982   Error: Scanning JTAG chain failed.
T1EFC 004:858.058   InitTarget() end - Took 2ms
T1EFC 004:858.126   Connect failed. Resetting via Reset pin and trying again.
T1EFC 004:920.048   ConfigTargetSettings() start
T1EFC 004:920.166    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 004:920.216   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 004:978.124   ConfigTargetSettings() end - Took 58ms
T1EFC 004:978.221   InitTarget() start
T1EFC 004:978.303    J-Link Script File: Executing InitTarget()
T1EFC 004:978.361   JTAG selected. Identifying JTAG Chain...
T1EFC 004:979.753   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 004:980.235   Error: Scanning JTAG chain failed.
T1EFC 004:980.317   InitTarget() end - Took 2ms
T1EFC 004:980.385 - 175.846ms returns 1
T1EFC 004:980.777 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 004:980.988   ConfigTargetSettings() start
T1EFC 004:981.086    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 004:981.142   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 005:033.789   ConfigTargetSettings() end - Took 52ms
T1EFC 005:033.901   InitTarget() start
T1EFC 005:033.993    J-Link Script File: Executing InitTarget()
T1EFC 005:034.054   JTAG selected. Identifying JTAG Chain...
T1EFC 005:035.531   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 005:036.021   Error: Scanning JTAG chain failed.
T1EFC 005:036.132   InitTarget() end - Took 2ms
T1EFC 005:036.220   Connect failed. Resetting via Reset pin and trying again.
T1EFC 005:097.814   ConfigTargetSettings() start
T1EFC 005:097.942    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 005:097.993   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 005:156.735   ConfigTargetSettings() end - Took 58ms
T1EFC 005:156.816   InitTarget() start
T1EFC 005:156.979    J-Link Script File: Executing InitTarget()
T1EFC 005:157.027   JTAG selected. Identifying JTAG Chain...
T1EFC 005:158.572   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 005:159.115   Error: Scanning JTAG chain failed.
T1EFC 005:159.202   InitTarget() end - Took 2ms
T1EFC 005:159.269 - 178.514ms returns 1
T1EFC 005:159.341 JLINK_ReadMem(0x400E0018, 0x4 Bytes, ...)
T1EFC 005:159.618   ConfigTargetSettings() start
T1EFC 005:159.703    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 005:159.748   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 005:209.476   ConfigTargetSettings() end - Took 49ms
T1EFC 005:209.576   InitTarget() start
T1EFC 005:209.640    J-Link Script File: Executing InitTarget()
T1EFC 005:209.685   JTAG selected. Identifying JTAG Chain...
T1EFC 005:211.068   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 005:211.552   Error: Scanning JTAG chain failed.
T1EFC 005:211.632   InitTarget() end - Took 2ms
T1EFC 005:211.697   Connect failed. Resetting via Reset pin and trying again.
T1EFC 005:272.468   ConfigTargetSettings() start
T1EFC 005:272.587    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 005:272.632   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 005:320.865   ConfigTargetSettings() end - Took 48ms
T1EFC 005:320.943   InitTarget() start
T1EFC 005:321.008    J-Link Script File: Executing InitTarget()
T1EFC 005:321.053   JTAG selected. Identifying JTAG Chain...
T1EFC 005:322.414   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 005:322.926   Error: Scanning JTAG chain failed.
T1EFC 005:323.006   InitTarget() end - Took 2ms
T1EFC 005:323.070 - 163.751ms returns 1
T1EFC 005:323.147 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 005:323.397   ConfigTargetSettings() start
T1EFC 005:323.479    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 005:323.523   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 005:373.693   ConfigTargetSettings() end - Took 50ms
T1EFC 005:373.777   InitTarget() start
T1EFC 005:373.844    J-Link Script File: Executing InitTarget()
T1EFC 005:373.890   JTAG selected. Identifying JTAG Chain...
T1EFC 005:375.156   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 005:375.659   Error: Scanning JTAG chain failed.
T1EFC 005:375.748   InitTarget() end - Took 2ms
T1EFC 005:375.817   Connect failed. Resetting via Reset pin and trying again.
T1EFC 005:436.535   ConfigTargetSettings() start
T1EFC 005:436.698    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 005:436.755   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 005:488.578   ConfigTargetSettings() end - Took 52ms
T1EFC 005:488.684   InitTarget() start
T1EFC 005:488.797    J-Link Script File: Executing InitTarget()
T1EFC 005:488.877   JTAG selected. Identifying JTAG Chain...
T1EFC 005:490.262   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 005:490.738   Error: Scanning JTAG chain failed.
T1EFC 005:490.818   InitTarget() end - Took 2ms
T1EFC 005:490.889 - 167.771ms returns 1
T1EFC 005:491.138 JLINK_ReadMem(0x400E0020, 0x4 Bytes, ...)
T1EFC 005:491.366   ConfigTargetSettings() start
T1EFC 005:491.465    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 005:491.513   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 005:544.260   ConfigTargetSettings() end - Took 52ms
T1EFC 005:544.340   InitTarget() start
T1EFC 005:544.405    J-Link Script File: Executing InitTarget()
T1EFC 005:544.454   JTAG selected. Identifying JTAG Chain...
T1EFC 005:545.912   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 005:546.542   Error: Scanning JTAG chain failed.
T1EFC 005:546.698   InitTarget() end - Took 3ms
T1EFC 005:546.778   Connect failed. Resetting via Reset pin and trying again.
T1EFC 005:608.755   ConfigTargetSettings() start
T1EFC 005:608.896    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 005:608.944   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 005:660.413   ConfigTargetSettings() end - Took 52ms
T1EFC 005:660.495   InitTarget() start
T1EFC 005:660.561    J-Link Script File: Executing InitTarget()
T1EFC 005:660.606   JTAG selected. Identifying JTAG Chain...
T1EFC 005:662.057   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 005:662.669   Error: Scanning JTAG chain failed.
T1EFC 005:662.780   InitTarget() end - Took 2ms
T1EFC 005:662.844 - 171.728ms returns 1
T1EFC 005:662.925 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 005:663.214   ConfigTargetSettings() start
T1EFC 005:663.299    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 005:663.344   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 005:725.555   ConfigTargetSettings() end - Took 62ms
T1EFC 005:725.666   InitTarget() start
T1EFC 005:725.758    J-Link Script File: Executing InitTarget()
T1EFC 005:725.822   JTAG selected. Identifying JTAG Chain...
T1EFC 005:727.131   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 005:727.673   Error: Scanning JTAG chain failed.
T1EFC 005:727.776   InitTarget() end - Took 2ms
T1EFC 005:727.863   Connect failed. Resetting via Reset pin and trying again.
T1EFC 005:790.135   ConfigTargetSettings() start
T1EFC 005:790.283    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 005:790.353   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 005:868.067   ConfigTargetSettings() end - Took 78ms
T1EFC 005:868.200   InitTarget() start
T1EFC 005:868.296    J-Link Script File: Executing InitTarget()
T1EFC 005:868.360   JTAG selected. Identifying JTAG Chain...
T1EFC 005:870.528   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 005:871.148   Error: Scanning JTAG chain failed.
T1EFC 005:871.442   InitTarget() end - Took 3ms
T1EFC 005:871.544 - 208.650ms returns 1
T1EFC 005:871.715 JLINK_ReadMem(0x400E0028, 0x4 Bytes, ...)
T1EFC 005:871.992   ConfigTargetSettings() start
T1EFC 005:872.115    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 005:872.183   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 005:950.334   ConfigTargetSettings() end - Took 78ms
T1EFC 005:950.441   InitTarget() start
T1EFC 005:950.530    J-Link Script File: Executing InitTarget()
T1EFC 005:950.593   JTAG selected. Identifying JTAG Chain...
T1EFC 005:951.984   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 005:952.488   Error: Scanning JTAG chain failed.
T1EFC 005:952.574   InitTarget() end - Took 2ms
T1EFC 005:952.644   Connect failed. Resetting via Reset pin and trying again.
T1EFC 006:014.950   ConfigTargetSettings() start
T1EFC 006:015.074    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 006:015.121   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 006:075.229   ConfigTargetSettings() end - Took 60ms
T1EFC 006:075.433   InitTarget() start
T1EFC 006:075.518    J-Link Script File: Executing InitTarget()
T1EFC 006:075.565   JTAG selected. Identifying JTAG Chain...
T1EFC 006:076.892   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 006:077.329   Error: Scanning JTAG chain failed.
T1EFC 006:077.405   InitTarget() end - Took 2ms
T1EFC 006:077.472 - 205.779ms returns 1
T1EFC 006:077.580 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 006:077.774   ConfigTargetSettings() start
T1EFC 006:077.848    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 006:077.899   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 006:128.300   ConfigTargetSettings() end - Took 50ms
T1EFC 006:128.379   InitTarget() start
T1EFC 006:128.444    J-Link Script File: Executing InitTarget()
T1EFC 006:128.489   JTAG selected. Identifying JTAG Chain...
T1EFC 006:129.844   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 006:130.333   Error: Scanning JTAG chain failed.
T1EFC 006:130.415   InitTarget() end - Took 2ms
T1EFC 006:130.481   Connect failed. Resetting via Reset pin and trying again.
T1EFC 006:191.518   ConfigTargetSettings() start
T1EFC 006:191.662    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 006:191.714   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 006:241.837   ConfigTargetSettings() end - Took 50ms
T1EFC 006:241.919   InitTarget() start
T1EFC 006:241.984    J-Link Script File: Executing InitTarget()
T1EFC 006:242.029   JTAG selected. Identifying JTAG Chain...
T1EFC 006:243.438   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 006:244.024   Error: Scanning JTAG chain failed.
T1EFC 006:244.133   InitTarget() end - Took 2ms
T1EFC 006:244.197 - 166.638ms returns 1
T1EFC 006:244.266 JLINK_ReadMem(0x400E0024, 0x4 Bytes, ...)
T1EFC 006:244.525   ConfigTargetSettings() start
T1EFC 006:244.610    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 006:244.654   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 006:294.591   ConfigTargetSettings() end - Took 50ms
T1EFC 006:294.679   InitTarget() start
T1EFC 006:294.747    J-Link Script File: Executing InitTarget()
T1EFC 006:294.794   JTAG selected. Identifying JTAG Chain...
T1EFC 006:296.159   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 006:296.738   Error: Scanning JTAG chain failed.
T1EFC 006:296.826   InitTarget() end - Took 2ms
T1EFC 006:296.891   Connect failed. Resetting via Reset pin and trying again.
T1EFC 006:357.877   ConfigTargetSettings() start
T1EFC 006:358.037    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 006:358.122   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 006:406.711   ConfigTargetSettings() end - Took 48ms
T1EFC 006:406.789   InitTarget() start
T1EFC 006:406.858    J-Link Script File: Executing InitTarget()
T1EFC 006:406.904   JTAG selected. Identifying JTAG Chain...
T1EFC 006:408.296   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 006:408.882   Error: Scanning JTAG chain failed.
T1EFC 006:408.988   InitTarget() end - Took 2ms
T1EFC 006:409.053 - 164.809ms returns 1
T1EFC 006:409.288 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 006:409.563   ConfigTargetSettings() start
T1EFC 006:409.648    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 006:409.694   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 006:467.026   ConfigTargetSettings() end - Took 57ms
T1EFC 006:467.131   InitTarget() start
T1EFC 006:467.217    J-Link Script File: Executing InitTarget()
T1EFC 006:467.278   JTAG selected. Identifying JTAG Chain...
T1EFC 006:468.755   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 006:469.278   Error: Scanning JTAG chain failed.
T1EFC 006:469.364   InitTarget() end - Took 2ms
T1EFC 006:469.433   Connect failed. Resetting via Reset pin and trying again.
T1EFC 006:531.450   ConfigTargetSettings() start
T1EFC 006:531.564    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 006:531.610   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 006:586.557   ConfigTargetSettings() end - Took 55ms
T1EFC 006:586.637   InitTarget() start
T1EFC 006:586.703    J-Link Script File: Executing InitTarget()
T1EFC 006:586.751   JTAG selected. Identifying JTAG Chain...
T1EFC 006:588.446   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 006:589.066   Error: Scanning JTAG chain failed.
T1EFC 006:589.180   InitTarget() end - Took 2ms
T1EFC 006:589.244 - 179.977ms returns 1
T1EFC 006:589.316 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T1EFC 006:589.652   ConfigTargetSettings() start
T1EFC 006:589.726    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 006:589.770   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 006:639.985   ConfigTargetSettings() end - Took 50ms
T1EFC 006:640.063   InitTarget() start
T1EFC 006:640.128    J-Link Script File: Executing InitTarget()
T1EFC 006:640.172   JTAG selected. Identifying JTAG Chain...
T1EFC 006:641.629   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 006:642.238   Error: Scanning JTAG chain failed.
T1EFC 006:642.371   InitTarget() end - Took 2ms
T1EFC 006:642.436   Connect failed. Resetting via Reset pin and trying again.
T1EFC 006:703.509   ConfigTargetSettings() start
T1EFC 006:703.629    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 006:703.673   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 006:754.992   ConfigTargetSettings() end - Took 51ms
T1EFC 006:755.071   InitTarget() start
T1EFC 006:755.135    J-Link Script File: Executing InitTarget()
T1EFC 006:755.180   JTAG selected. Identifying JTAG Chain...
T1EFC 006:756.645   TotalIRLen = ?, IRPrint = 0x..FFFFFFFFFFFFFFFFFFFFFFF1
T1EFC 006:757.246   Error: Scanning JTAG chain failed.
T1EFC 006:757.349   InitTarget() end - Took 2ms
T1EFC 006:757.413 - 168.118ms returns 1
T1EFC 006:758.338 JLINK_TIF_GetAvailable(...)
T1EFC 006:758.599 - 0.294ms
T1EFC 006:758.661 JLINK_TIF_Select(JLINKARM_TIF_SWD)
T1EFC 006:759.780 - 1.150ms returns 0x00
T1EFC 006:759.840 JLINK_SetSpeed(4000)
T1EFC 006:760.007 - 0.205ms
T1EFC 006:760.072 JLINK_SetEndian(ARM_ENDIAN_LITTLE)
T1EFC 006:760.116 - 0.065ms returns 0
T1EFC 006:760.162 JLINK_SetInitRegsOnReset(OFF)
T1EFC 006:760.205 - 0.065ms returns 1
T1EFC 006:760.251 JLINK_SetResetType(JLINKARM_RESET_TYPE_NO_RESET)
T1EFC 006:760.295 - 0.064ms returns JLINKARM_RESET_TYPE_NORMAL
T1EFC 006:760.342 JLINK_ExecCommand("EnableFlashBPs", ...). 
T1EFC 006:760.389 - 0.022ms returns 0x00
T1EFC 006:760.436 JLINK_ExecCommand("SetAllowFlashCache = 1", ...). 
T1EFC 006:760.484 - 0.023ms returns 0x01
T1EFC 006:760.530 JLINK_ExecCommand("SetRestartOnClose = 0", ...). 
T1EFC 006:760.578 - 0.023ms returns 0x01
T1EFC 006:760.623 JLINK_EnableSoftBPs(ON)
T1EFC 006:760.666 - 0.064ms
T1EFC 006:760.712 JLINK_Connect()
T1EFC 006:761.076   ConfigTargetSettings() start
T1EFC 006:761.147    J-Link Script File: Executing ConfigTargetSettings()
T1EFC 006:761.192   Configuring FlashDLNoRMWThreshold=0x200 in order to make sure that option bytes programming is done via read-modify-write
T1EFC 006:810.087   ConfigTargetSettings() end - Took 49ms
T1EFC 006:810.169   InitTarget() start
T1EFC 006:810.234    J-Link Script File: Executing InitTarget()
T1EFC 006:810.280   SWD selected. Executing JTAG -> SWD switching sequence.
T1EFC 006:812.462   DAP initialized successfully.
T1EFC 006:812.573   Determining TrustZone configuration...
T1EFC 006:813.574     Secure Debug: Enabled (SSD)
T1EFC 006:813.648   Determining currently configured transfer type by reading the AHB-AP CSW register.
T1EFC 006:814.320     --> Correct transfer type configured. Done.
T1EFC 006:814.394   InitTarget() end - Took 4ms
T1EFC 006:814.850   Found SW-DP with ID 0x6BA02477
T1EFC 006:816.478   DPIDR: 0x6BA02477
T1EFC 006:816.553   CoreSight SoC-400 or earlier
T1EFC 006:816.619   Scanning AP map to find all available APs
T1EFC 006:817.322   AP[2]: Stopped AP scan as end of AP map has been reached
T1EFC 006:817.395   AP[0]: AHB-AP (IDR: 0x84770001)
T1EFC 006:817.460   AP[1]: APB-AP (IDR: 0x54770002)
T1EFC 006:817.536   Iterating through AP map to find AHB-AP to use
T1EFC 006:818.075   AP[0]: Core found
T1EFC 006:818.147   AP[0]: AHB-AP ROM base: 0xE00FE000
T1EFC 006:818.437   CPUID register: 0x410FD214. Implementer code: 0x41 (ARM)
T1EFC 006:818.509   Feature set: Mainline
T1EFC 006:818.799   Cache: No cache
T1EFC 006:818.849   Found Cortex-M33 r0p4, Little endian.
T1EFC 006:819.272   -- Max. mem block: 0x00004D70
T1EFC 006:820.035   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T1EFC 006:820.519   CPU_WriteMem(4 bytes @ 0xE000EDF0)
T1EFC 006:820.874   CPU_ReadMem(4 bytes @ 0xE0002000)
T1EFC 006:821.405   FPUnit: 8 code (BP) slots and 0 literal slots
T1EFC 006:821.478   CPU_ReadMem(4 bytes @ 0xE000EDFC)
T1EFC 006:821.786   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T1EFC 006:822.129   CPU_ReadMem(4 bytes @ 0xE0001000)
T1EFC 006:822.498   CPU_ReadMem(4 bytes @ 0xE0001000)
T1EFC 006:823.021   CPU_ReadMem(4 bytes @ 0xE0001028)
T1EFC 006:823.386   CPU_ReadMem(4 bytes @ 0xE0001038)
T1EFC 006:823.753   CPU_ReadMem(4 bytes @ 0xE0001048)
T1EFC 006:824.274   CPU_ReadMem(4 bytes @ 0xE0001058)
T1EFC 006:824.647   CPU_WriteMem(4 bytes @ 0xE0001000)
T1EFC 006:825.010   CPU_ReadMem(4 bytes @ 0xE000ED88)
T1EFC 006:825.386   CPU_WriteMem(4 bytes @ 0xE000ED88)
T1EFC 006:825.902   CPU_ReadMem(4 bytes @ 0xE000ED88)
T1EFC 006:826.253   CPU_WriteMem(4 bytes @ 0xE000ED88)
T1EFC 006:826.628   CPU_ReadMem(4 bytes @ 0xE000EFB8)
T1EFC 006:827.151   Security extension: implemented
T1EFC 006:827.222   Secure debug: enabled
T1EFC 006:827.288   CoreSight components:
T1EFC 006:827.353   ROMTbl[0] @ E00FE000
T1EFC 006:827.419   CPU_ReadMem(64 bytes @ 0xE00FE000)
T1EFC 006:827.953   CPU_ReadMem(32 bytes @ 0xE0044FE0)
T1EFC 006:828.387   CPU_ReadMem(4 bytes @ 0xE0044FBC)
T1EFC 006:828.752   CPU_ReadMem(4 bytes @ 0xE0044FCC)
T1EFC 006:829.128   [0][0]: E0044000 CID B105900D PID 005BB906 DEVARCH 00000000 DEVTYPE 14 CTI (?)
T1EFC 006:829.222   CPU_ReadMem(32 bytes @ 0xE0047FE0)
T1EFC 006:829.685   CPU_ReadMem(4 bytes @ 0xE0047FBC)
T1EFC 006:830.004   CPU_ReadMem(4 bytes @ 0xE0047FCC)
T1EFC 006:830.331   [0][1]: E0047000 CID B105900D PID 003BB908 DEVARCH 00000000 DEVTYPE 12 CSTF
T1EFC 006:830.407   CPU_ReadMem(32 bytes @ 0xE0048FE0)
T1EFC 006:830.858   CPU_ReadMem(4 bytes @ 0xE0048FBC)
T1EFC 006:831.196   CPU_ReadMem(4 bytes @ 0xE0048FCC)
T1EFC 006:831.552   [0][2]: E0048000 CID B105900D PID 001BB961 DEVARCH 00000000 DEVTYPE 21 ETB
T1EFC 006:831.626   CPU_ReadMem(32 bytes @ 0xE0049FE0)
T1EFC 006:832.057   [0][3]: E0049000 CID B105F00D PID 001BB101 TSG
T1EFC 006:832.131   CPU_ReadMem(32 bytes @ 0xE0040FE0)
T1EFC 006:832.553   CPU_ReadMem(4 bytes @ 0xE0040FBC)
T1EFC 006:832.882   CPU_ReadMem(4 bytes @ 0xE0040FCC)
T1EFC 006:833.212   [0][4]: E0040000 CID B105900D PID 000BBD21 DEVARCH 00000000 DEVTYPE 11 TPIU
T1EFC 006:833.285   CPU_ReadMem(32 bytes @ 0xE00FFFE0)
T1EFC 006:833.714   [0][5]: E00FF000 CID B105100D PID 000BB4C9 ROM Table
T1EFC 006:833.788   ROMTbl[1] @ E00FF000
T1EFC 006:833.856   CPU_ReadMem(64 bytes @ 0xE00FF000)
T1EFC 006:834.418   CPU_ReadMem(32 bytes @ 0xE000EFE0)
T1EFC 006:834.866   CPU_ReadMem(4 bytes @ 0xE000EFBC)
T1EFC 006:835.205   CPU_ReadMem(4 bytes @ 0xE000EFCC)
T1EFC 006:835.601   [1][0]: E000E000 CID B105900D PID 000BBD21 DEVARCH 47702A04 DEVTYPE 00 Cortex-M33
T1EFC 006:835.681   CPU_ReadMem(32 bytes @ 0xE0001FE0)
T1EFC 006:836.207   CPU_ReadMem(4 bytes @ 0xE0001FBC)
T1EFC 006:836.594   CPU_ReadMem(4 bytes @ 0xE0001FCC)
T1EFC 006:836.934   [1][1]: E0001000 CID B105900D PID 000BBD21 DEVARCH 47701A02 DEVTYPE 00 DWT
T1EFC 006:837.007   CPU_ReadMem(32 bytes @ 0xE0002FE0)
T1EFC 006:837.414   CPU_ReadMem(4 bytes @ 0xE0002FBC)
T1EFC 006:837.729   CPU_ReadMem(4 bytes @ 0xE0002FCC)
T1EFC 006:838.026   [1][2]: E0002000 CID B105900D PID 000BBD21 DEVARCH 47701A03 DEVTYPE 00 FPB
T1EFC 006:838.099   CPU_ReadMem(32 bytes @ 0xE0000FE0)
T1EFC 006:838.555   CPU_ReadMem(4 bytes @ 0xE0000FBC)
T1EFC 006:838.881   CPU_ReadMem(4 bytes @ 0xE0000FCC)
T1EFC 006:839.202   [1][3]: E0000000 CID B105900D PID 000BBD21 DEVARCH 47701A01 DEVTYPE 43 ITM
T1EFC 006:839.284   CPU_ReadMem(32 bytes @ 0xE0041FE0)
T1EFC 006:839.707   CPU_ReadMem(4 bytes @ 0xE0041FBC)
T1EFC 006:840.030   CPU_ReadMem(4 bytes @ 0xE0041FCC)
T1EFC 006:840.353   [1][5]: E0041000 CID B105900D PID 002BBD21 DEVARCH 47724A13 DEVTYPE 13 ETM
T1EFC 006:840.426   CPU_ReadMem(32 bytes @ 0xE0042FE0)
T1EFC 006:840.881   CPU_ReadMem(4 bytes @ 0xE0042FBC)
T1EFC 006:841.201   CPU_ReadMem(4 bytes @ 0xE0042FCC)
T1EFC 006:841.557   [1][6]: E0042000 CID B105900D PID 000BBD21 DEVARCH 47701A14 DEVTYPE 14 CSS600-CTI
T1EFC 006:841.644 - 80.963ms returns 0x00
T1EFC 006:841.720 JLINK_ResetPullsRESET(ON)
T1EFC 006:841.783 - 0.095ms
T1EFC 006:841.851 JLINK_Halt()
T1EFC 006:844.476 - 2.652ms returns 0x00
T1EFC 006:844.533 JLINK_IsHalted()
T1EFC 006:844.884 - 0.378ms returns TRUE
T1EFC 006:844.941 JLINK_Reset()
T1EFC 006:844.996   CPU_WriteMem(4 bytes @ 0xE000EDF0)
T1EFC 006:845.327   CPU_ReadMem(4 bytes @ 0xE000ED44)
T1EFC 006:845.679   CPU_ReadMem(4 bytes @ 0xE000EE08)
T1EFC 006:846.028   CPU_WriteMem(4 bytes @ 0xE000EE08)
T1EFC 006:846.445   Reset: ARMv8M core with Security Extension enabled detected.
T1EFC 006:846.548   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T1EFC 006:846.939   Reset: Halt core after reset via DEMCR.VC_CORERESET.
T1EFC 006:847.436   Reset: Reset device via AIRCR.SYSRESETREQ.
T1EFC 006:847.522   CPU_WriteMem(4 bytes @ 0xE000ED0C)
T1EFC 006:900.722   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T1EFC 006:901.212   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T1EFC 006:901.699   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T1EFC 006:907.902   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T1EFC 006:911.470   CPU_WriteMem(4 bytes @ 0xE0002000)
T1EFC 006:911.980   CPU_ReadMem(4 bytes @ 0xE000EDFC)
T1EFC 006:912.421   CPU_ReadMem(4 bytes @ 0xE0001000)
T1EFC 006:912.851   CPU_ReadMem(4 bytes @ 0xE000EE08)
T1EFC 006:913.296 - 68.385ms
T1EFC 006:913.359 JLINK_SetEndian(ARM_ENDIAN_LITTLE)
T1EFC 006:913.423 - 0.086ms returns 0
T1EFC 006:913.532 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 006:913.597   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T1EFC 006:913.997   Data:  03 00 13 00
T1EFC 006:914.072   Debug reg: DHCSR
T1EFC 006:914.135 - 0.625ms returns 0
T1EFC 006:914.203 JLINK_ReadMem(0x010080F0, 0x10 Bytes, ...)
T1EFC 006:914.256   CPU_ReadMem(16 bytes @ 0x010080F0)
T1EFC 006:914.678   Data:  52 37 46 41 34 4D 32 41 44 33 43 4E 45 20 20 20
T1EFC 006:914.753 - 0.571ms returns 0
T1EFC 006:914.809 JLINK_IsHalted()
T1EFC 006:914.854 - 0.068ms returns TRUE
T1EFC 006:915.237 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 006:915.292   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T1EFC 006:915.702   Data:  03 00 13 00
T1EFC 006:915.776   Debug reg: DHCSR
T1EFC 006:915.841 - 0.624ms returns 0
T1EFC 006:915.890 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T1EFC 006:915.941   CPU_ReadMem(4 bytes @ 0x400E002C)
T1EFC 006:916.334   Data:  01 00 00 00
T1EFC 006:916.404 - 0.535ms returns 0
T1EFC 006:916.457 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T1EFC 006:916.508   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T1EFC 006:916.901   Data:  03 00 13 00
T1EFC 006:916.971   Debug reg: DHCSR
T1EFC 006:917.035 - 0.599ms returns 0
T1EFC 006:917.084 JLINK_ReadMem(0x400E002C, 0x4 Bytes, ...)
T1EFC 006:917.134   CPU_ReadMem(4 bytes @ 0x400E002C)
T1EFC 006:917.494   Data:  01 00 00 00
T1EFC 006:917.564 - 0.501ms returns 0
T1EFC 006:917.613 JLINK_MeasureCPUSpeed(RAMAddr = 0xFFFFFFFF)
T1EFC 006:917.663   CPU_ReadMem(16 bytes @ 0x2000D000)
T1EFC 006:918.106   CPU_ReadMem(64 bytes @ 0x2000D000)
T1EFC 006:918.732    -- Updating C cache (64 bytes @ 0x2000D000)
T1EFC 006:918.802    -- Read from C cache (6 bytes @ 0x2000D000)
T1EFC 006:918.869   CPU_ReadMem(4 bytes @ 0xE000ED90)
T1EFC 006:919.262   CPU_ReadMem(4 bytes @ 0xE000ED94)
T1EFC 006:919.673   CPU_WriteMem(16 bytes @ 0x2000D000)
T1EFC 006:920.160   CPU_WriteMem(6 bytes @ 0x2000D000)
T1EFC 006:920.633   CPU_ReadMem(64 bytes @ 0x2000D000)
T1EFC 006:921.248    -- Updating C cache (64 bytes @ 0x2000D000)
T1EFC 006:921.318    -- Read from C cache (6 bytes @ 0x2000D000)
T1EFC 006:921.394   CPU_ReadMem(4 bytes @ 0xE000EE08)
T1EFC 006:921.783   CPU_WriteMem(4 bytes @ 0xE0002008)
T1EFC 006:921.854   CPU_WriteMem(4 bytes @ 0xE000200C)
T1EFC 006:921.919   CPU_WriteMem(4 bytes @ 0xE0002010)
T1EFC 006:921.984   CPU_WriteMem(4 bytes @ 0xE0002014)
T1EFC 006:922.049   CPU_WriteMem(4 bytes @ 0xE0002018)
T1EFC 006:922.114   CPU_WriteMem(4 bytes @ 0xE000201C)
T1EFC 006:922.179   CPU_WriteMem(4 bytes @ 0xE0002020)
T1EFC 006:922.276   CPU_WriteMem(4 bytes @ 0xE0002024)
T1EFC 006:923.720   CPU_WriteMem(4 bytes @ 0xE0001004)
T1EFC 006:929.314   CPU_ReadMem(4 bytes @ 0xE0001004)
T1EFC 006:929.747   CPU_ReadMem(4 bytes @ 0xE000EE08)
T1EFC 006:930.165   CPU_WriteMem(4 bytes @ 0xE0002008)
T1EFC 006:930.593   CPU_WriteMem(4 bytes @ 0xE000200C)
T1EFC 006:930.999   CPU_WriteMem(4 bytes @ 0xE0002010)
T1EFC 006:931.370   CPU_WriteMem(4 bytes @ 0xE0002014)
T1EFC 006:931.745   CPU_WriteMem(4 bytes @ 0xE0002018)
T1EFC 006:932.094   CPU_WriteMem(4 bytes @ 0xE000201C)
T1EFC 006:932.456   CPU_WriteMem(4 bytes @ 0xE0002020)
T1EFC 006:932.823   CPU_WriteMem(4 bytes @ 0xE0002024)
T1EFC 006:933.219   CPU_ReadMem(4 bytes @ 0xE000EE08)
T1EFC 006:933.569   CPU_ReadMem(4 bytes @ 0xE000EE08)
T1EFC 006:933.922   CPU_WriteMem(4 bytes @ 0xE0001004)
T1EFC 006:959.546   CPU_ReadMem(4 bytes @ 0xE0001004)
T1EFC 006:960.023   CPU_WriteMem(6 bytes @ 0x2000D000)
T1EFC 006:960.464   ClockFreq: 2068500 Hz
T1EFC 006:960.537 - 42.946ms returns 2068500
T1EFC 006:960.604 JLINK_ReadReg(XPSR)
T1EFC 006:960.667   CPU_ReadMem(4 bytes @ 0xE000EE08)
T1EFC 006:961.054 - 0.480ms returns 0xF9000000
T32C8 007:064.053 JLINK_ReadReg(XPSR)
T32C8 007:064.160   CPU_ReadMem(4 bytes @ 0xE000EE08)
T32C8 007:064.589 - 0.590ms returns 0xF9000000
T32C8 007:111.997 JLINK_ReadReg(XPSR)
T32C8 007:112.112   CPU_ReadMem(4 bytes @ 0xE000EE08)
T32C8 007:112.510 - 0.553ms returns 0xF9000000
T32C8 007:396.992 JLINK_SetEndian(ARM_ENDIAN_LITTLE)
T32C8 007:397.132 - 0.179ms returns 0
T32C8 007:397.521 JLINK_BeginDownload(Flags = 0x00000000)
T32C8 007:397.604 - 0.116ms
T32C8 007:432.612 JLINK_ReadMem(0xE000EDF0, 0x4 Bytes, ...)
T32C8 007:432.743   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T32C8 007:433.141   Data:  03 00 13 00
T32C8 007:433.243   Debug reg: DHCSR
T32C8 007:433.330 - 0.747ms returns 0
T32C8 007:434.990 JLINK_WriteMem(0x00000000, 0xBB0 Bytes, ...)
T32C8 007:435.102   Data:  00 38 00 20 35 6E 00 00 61 6C 00 00 31 6E 00 00 ...
T32C8 007:435.548   completely In flash
T32C8 007:435.657 - 0.696ms returns 0xBB0
T32C8 007:436.682 JLINK_WriteMem(0x00000BB0, 0xB90 Bytes, ...)
T32C8 007:436.787   Data:  0D F1 2B 00 FF F7 04 FC 00 28 3F F4 36 AD 00 21 ...
T32C8 007:436.885   completely In flash
T32C8 007:436.973 - 0.321ms returns 0xB90
T32C8 007:437.713 JLINK_WriteMem(0x00001740, 0xBB0 Bytes, ...)
T32C8 007:437.807   Data:  4F F0 FF 32 30 46 39 46 B5 4B 06 F0 15 F8 00 28 ...
T32C8 007:437.927   completely In flash
T32C8 007:438.017 - 0.333ms returns 0xBB0
T32C8 007:438.825 JLINK_WriteMem(0x000022F0, 0xBC0 Bytes, ...)
T32C8 007:438.919   Data:  28 46 00 F0 97 F9 00 21 28 46 00 F0 5D F9 10 F0 ...
T32C8 007:439.015   completely In flash
T32C8 007:439.107 - 0.311ms returns 0xBC0
T32C8 007:439.866 JLINK_WriteMem(0x00002EB0, 0xBA0 Bytes, ...)
T32C8 007:439.958   Data:  70 47 4A B1 07 4B 03 EB 41 01 0B 88 23 F4 00 73 ...
T32C8 007:440.073   completely In flash
T32C8 007:440.162 - 0.326ms returns 0xBA0
T32C8 007:440.942 JLINK_WriteMem(0x00003A50, 0xBC0 Bytes, ...)
T32C8 007:441.034   Data:  CD E7 00 F0 E3 F8 E4 E7 10 2E 00 20 E0 29 00 20 ...
T32C8 007:441.126   completely In flash
T32C8 007:441.216 - 0.303ms returns 0xBC0
T32C8 007:442.016 JLINK_WriteMem(0x00004610, 0xBA0 Bytes, ...)
T32C8 007:442.142   Data:  0C 4C A8 78 FF F7 E0 F8 94 F8 40 30 D8 00 04 EB ...
T32C8 007:442.296   completely In flash
T32C8 007:442.395 - 0.410ms returns 0xBA0
T32C8 007:443.578 JLINK_WriteMem(0x000051B0, 0xBA0 Bytes, ...)
T32C8 007:443.679   Data:  A4 E7 47 4B 1B 88 23 43 AC D1 49 49 43 4B 09 68 ...
T32C8 007:443.788   completely In flash
T32C8 007:443.894 - 0.347ms returns 0xBA0
T32C8 007:444.684 JLINK_WriteMem(0x00005D50, 0xBA0 Bytes, ...)
T32C8 007:444.771   Data:  50 F8 21 10 0B 42 0F D0 20 46 01 A9 FF F7 16 FF ...
T32C8 007:444.883   completely In flash
T32C8 007:444.980 - 0.327ms returns 0xBA0
T32C8 007:445.769 JLINK_WriteMem(0x000068F0, 0xBD0 Bytes, ...)
T32C8 007:445.856   Data:  03 F1 60 43 00 FA 02 F2 03 F5 61 43 C3 F8 80 21 ...
T32C8 007:445.957   completely In flash
T32C8 007:446.049 - 0.310ms returns 0xBD0
T32C8 007:447.027 JLINK_WriteMem(0x000074C0, 0xA94 Bytes, ...)
T32C8 007:447.231   Data:  41 F4 70 01 4F F0 00 00 70 BD 41 F0 FE 41 41 F4 ...
T32C8 007:447.402   completely In flash
T32C8 007:447.511 - 0.517ms returns 0xA94
T32C8 007:448.577 JLINK_WriteMem(0x00007F54, 0x938 Bytes, ...)
T32C8 007:448.669   Data:  4F F4 2A 43 16 49 B1 F8 84 C0 A1 F8 84 30 B1 F8 ...
T32C8 007:448.772   completely In flash
T32C8 007:448.872 - 0.325ms returns 0x938
T32C8 007:449.968 JLINK_WriteMem(0x0100A100, 0x38 Bytes, ...)
T32C8 007:450.094   Data:  FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF FF ...
T32C8 007:450.593   completely In flash
T32C8 007:450.711 - 0.775ms returns 0x38
T32C8 007:451.913 JLINK_WriteMem(0x0100A200, 0xD0 Bytes, ...)
T32C8 007:452.047   Data:  FB FC FF FF FF FF FF FF FF FF FF FF FF FF FF FF ...
T32C8 007:452.161   completely In flash
T32C8 007:452.257 - 0.374ms returns 0xD0
T32C8 007:472.082 JLINK_EndDownload()
T32C8 007:472.495   CPU_ReadMem(4 bytes @ 0xE000ED90)
T32C8 007:472.908   CPU_ReadMem(4 bytes @ 0xE000ED94)
T32C8 007:473.385    -- --------------------------------------
T32C8 007:473.513   Flash bank @ 0x0100A100: Default: L2 verify disabled because algorithm performs L1 verify
T32C8 007:473.605    -- Start of determining dirty areas in flash cache
T32C8 007:473.696    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A100 if necessary
T32C8 007:473.785    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A110 if necessary
T32C8 007:473.875    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A120 if necessary
T32C8 007:473.964    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A130 if necessary
T32C8 007:474.058    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A200 if necessary
T32C8 007:474.147    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A210 if necessary
T32C8 007:474.242    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A220 if necessary
T32C8 007:474.330    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A230 if necessary
T32C8 007:474.420    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A240 if necessary
T32C8 007:474.509    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A250 if necessary
T32C8 007:474.597    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A260 if necessary
T32C8 007:474.686    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A270 if necessary
T32C8 007:474.774    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A280 if necessary
T32C8 007:475.052    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A290 if necessary
T32C8 007:475.146    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A2A0 if necessary
T32C8 007:475.236    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A2B0 if necessary
T32C8 007:475.323    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x0100A2C0 if necessary
T32C8 007:475.410    -- End of determining dirty areas
T32C8 007:475.497    -- Start of preparing flash programming
T32C8 007:475.584    -- Calculating RAM usage
T32C8 007:475.683    -- RAM usage = 3476 Bytes
T32C8 007:475.773    -- Preserving CPU registers
T32C8 007:491.519    -- Determining CPU clock frequency
T32C8 007:533.588    -- Preparing target
T32C8 007:533.737    -- Preserving target RAM temporarily used for programming
T32C8 007:546.729    -- Downloading RAMCode
T32C8 007:561.716    -- Preparing RAMCode
T32C8 007:569.120    -- CPU frequency = 100000 kHz
T32C8 007:569.278    -- End of preparing flash programming
T32C8 007:569.646   Looking for J-Link GUI Server exe at: C:\Users\T.Uemitsu\.eclipse\com.renesas.platform_780075259\DebugComp\RA\ARM\Segger_v7.86.2\JLinkGUIServer.exe
T32C8 007:570.209   Looking for J-Link GUI Server exe at: C:\Program Files\SEGGER\JLink\JLinkGUIServer.exe
T32C8 007:570.384   Forking J-Link GUI Server: C:\Program Files\SEGGER\JLink\JLinkGUIServer.exe
T32C8 007:675.738   J-Link GUI Server info: "J-Link GUI server V7.88 "
T32C8 007:856.277    -- CPU is running at 100000 kHz.
T32C8 007:856.431    -- Start of comparing flash
T32C8 007:856.521    -- CRC check was estimated as fastest method
T32C8 007:898.474    -- Comparing range 0x100A100 - 0x100A13F (4 Sectors, 64 Bytes), using multi-block CRC calculation
T32C8 007:906.540    -- All CRCs match
T32C8 007:907.152    -- Comparing range 0x100A200 - 0x100A2CF (13 Sectors, 208 Bytes), using multi-block CRC calculation
T32C8 007:911.672    -- All CRCs match
T32C8 007:912.272    -- Comparing range 0x100A100 - 0x100A13F (4 Sectors, 64 Bytes), using alternative multi-block CRC calculation
T32C8 007:915.920    -- All CRCs match
T32C8 007:916.483    -- Comparing range 0x100A200 - 0x100A2CF (13 Sectors, 208 Bytes), using alternative multi-block CRC calculation
T32C8 007:920.505    -- All CRCs match
T32C8 007:920.629    -- End of comparing flash
T32C8 007:920.699    -- Start of erasing sectors
T32C8 007:920.767    -- End of erasing sectors
T32C8 007:920.837    -- Start of flash programming
T32C8 007:920.903    -- End of flash programming
T32C8 007:920.970    -- Start of restoring
T32C8 007:921.036    -- Restoring RAMCode
T32C8 007:925.271    -- Restoring target memory
T32C8 007:937.456    -- Restore target
T32C8 007:937.579    -- Restoring CPU registers
T32C8 007:937.983    -- End of restoring
T32C8 007:938.096    -- Bank 0 @ 0x0100A100: Skipped. Contents already match
T32C8 007:938.185    -- Bank 0 @ 0x0100A100: Skipped. Contents already match
T32C8 007:940.244    -- --------------------------------------
T32C8 007:940.393   Flash bank @ 0x00000000: Default: L2 verify disabled because algorithm performs L1 verify
T32C8 007:940.479    -- Start of determining dirty areas in flash cache
T32C8 007:940.574    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x00000000 if necessary
T32C8 007:940.672    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x00002000 if necessary
T32C8 007:940.770    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x00004000 if necessary
T32C8 007:940.927    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x00006000 if necessary
T32C8 007:941.022    -- Filling invalid ranges in sector buffer (flash cache) for sector @ 0x00008000 if necessary
T32C8 007:941.237    -- End of determining dirty areas
T32C8 007:941.310    -- Start of preparing flash programming
T32C8 007:941.377    -- Calculating RAM usage
T32C8 007:941.478    -- RAM usage = 4500 Bytes
T32C8 007:941.555    -- Preserving CPU registers
T32C8 007:941.788    -- Determining CPU clock frequency
T32C8 007:979.332    -- Preparing target
T32C8 007:979.646    -- Preserving target RAM temporarily used for programming
T32C8 007:996.919    -- Downloading RAMCode
T32C8 008:013.267    -- Preparing RAMCode
T32C8 008:022.165    -- CPU frequency = 100000 kHz
T32C8 008:022.271    -- End of preparing flash programming
T32C8 008:026.213    -- CPU is running at 100000 kHz.
T32C8 008:026.390    -- Start of comparing flash
T32C8 008:026.507    -- CRC check was estimated as fastest method
T32C8 008:041.337    -- Comparing range 0x0000 - 0x9FFF (5 Sectors, 40 KB), using multi-block CRC calculation
T32C8 008:059.468    -- All CRCs match
T32C8 008:060.471    -- Comparing range 0x0000 - 0x9FFF (5 Sectors, 40 KB), using alternative multi-block CRC calculation
T32C8 008:076.413    -- All CRCs match
T32C8 008:076.547    -- End of comparing flash
T32C8 008:076.646    -- Start of erasing sectors
T32C8 008:076.739    -- End of erasing sectors
T32C8 008:076.830    -- Start of flash programming
T32C8 008:076.922    -- End of flash programming
T32C8 008:077.011    -- Start of restoring
T32C8 008:077.620    -- Restoring RAMCode
T32C8 008:084.375    -- Restoring target memory
T32C8 008:100.100    -- Restore target
T32C8 008:100.263    -- Restoring CPU registers
T32C8 008:100.726    -- End of restoring
T32C8 008:100.833    -- Bank 1 @ 0x00000000: Skipped. Contents already match
T32C8 008:100.928    -- Bank 1 @ 0x00000000: Skipped. Contents already match
T32C8 008:123.914 - 651.887ms returns 0 (0x0)
T32C8 008:124.290 JLINK_WriteReg(R15 (PC), 0x00006E34)
T32C8 008:124.372 - 0.114ms returns 0
T32C8 008:124.439 JLINK_WriteReg(XPSR, 0x01000000)
T32C8 008:124.510 - 0.103ms returns 0
T32C8 008:124.582 JLINK_ResetPullsRESET(ON)
T32C8 008:124.646 - 0.097ms
T32C8 008:124.713 JLINK_Halt()
T32C8 008:124.772 - 0.087ms returns 0x00
T32C8 008:124.833 JLINK_IsHalted()
T32C8 008:124.893 - 0.091ms returns TRUE
T32C8 008:124.961 JLINK_Reset()
T32C8 008:125.119   CPU_WriteMem(4 bytes @ 0xE000EDF0)
T32C8 008:127.346   CPU_ReadMem(4 bytes @ 0xE000ED44)
T32C8 008:128.582   CPU_ReadMem(4 bytes @ 0xE000EE08)
T32C8 008:129.279   CPU_WriteMem(4 bytes @ 0xE000EE08)
T32C8 008:129.916   Reset: ARMv8M core with Security Extension enabled detected.
T32C8 008:130.123   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T32C8 008:130.701   Reset: Halt core after reset via DEMCR.VC_CORERESET.
T32C8 008:131.462   Reset: Reset device via AIRCR.SYSRESETREQ.
T32C8 008:131.631   CPU_WriteMem(4 bytes @ 0xE000ED0C)
T32C8 008:185.540   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T32C8 008:185.937   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T32C8 008:186.325   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T32C8 008:192.669   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T32C8 008:195.972   CPU_WriteMem(4 bytes @ 0xE0002000)
T32C8 008:196.416   CPU_ReadMem(4 bytes @ 0xE000EDFC)
T32C8 008:196.780   CPU_ReadMem(4 bytes @ 0xE0001000)
T32C8 008:197.134   CPU_ReadMem(4 bytes @ 0xE000EE08)
T32C8 008:197.478 - 72.553ms
T32C8 008:197.557 JLINK_SetEndian(ARM_ENDIAN_LITTLE)
T32C8 008:197.619 - 0.093ms returns 0
T32C8 008:198.632 JLINK_ResetPullsRESET(ON)
T32C8 008:198.729 - 0.127ms
T32C8 008:198.793 JLINK_Halt()
T32C8 008:198.856 - 0.094ms returns 0x00
T32C8 008:198.920 JLINK_IsHalted()
T32C8 008:198.982 - 0.091ms returns TRUE
T32C8 008:199.045 JLINK_Reset()
T32C8 008:199.123   CPU_WriteMem(4 bytes @ 0xE000EDF0)
T32C8 008:199.505   CPU_ReadMem(4 bytes @ 0xE000ED44)
T32C8 008:199.850   CPU_ReadMem(4 bytes @ 0xE000EE08)
T32C8 008:200.184   CPU_WriteMem(4 bytes @ 0xE000EE08)
T32C8 008:200.830   Reset: ARMv8M core with Security Extension enabled detected.
T32C8 008:200.951   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T32C8 008:201.370   Reset: Halt core after reset via DEMCR.VC_CORERESET.
T32C8 008:201.941   Reset: Reset device via AIRCR.SYSRESETREQ.
T32C8 008:202.055   CPU_WriteMem(4 bytes @ 0xE000ED0C)
T32C8 008:256.177   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T32C8 008:256.732   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T32C8 008:257.122   CPU_WriteMem(4 bytes @ 0xE000EDFC)
T32C8 008:262.818   CPU_ReadMem(4 bytes @ 0xE000EDF0)
T32C8 008:266.446   CPU_WriteMem(4 bytes @ 0xE0002000)
T32C8 008:266.803   CPU_ReadMem(4 bytes @ 0xE000EDFC)
T32C8 008:267.128   CPU_ReadMem(4 bytes @ 0xE0001000)
T32C8 008:267.477   CPU_ReadMem(4 bytes @ 0xE000EE08)
T32C8 008:267.803 - 68.786ms
T32C8 008:267.870 JLINK_SetEndian(ARM_ENDIAN_LITTLE)
T32C8 008:267.927 - 0.080ms returns 0
T32C8 008:290.497 JLINK_ReadMem(0x00006E34, 0x4 Bytes, ...)
T32C8 008:290.615    -- Read from flash cache (4 bytes @ 0x00006E34)
T32C8 008:290.701   Data:  08 B5 00 F0
T32C8 008:290.795 - 0.326ms returns 0
T32C8 008:304.367 JLINK_ReadReg(XPSR)
T32C8 008:304.492   CPU_ReadMem(4 bytes @ 0xE000EE08)
T32C8 008:304.904 - 0.585ms returns 0xF9000000
T32C8 009:028.684 JLINK_ReadRegs(NumRegs = 22, Indexes: 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 16, 17, 18, 86, 87, 20)
T32C8 009:028.901    -- R0=0x00, R1=0x00, R2=0x00, R3=0x00, R4=0x00, R5=0x00, R6=0x00, R7=0x00, R8=0x70000, R9=0x01, R10=0x2000379C, R11=0x2000379C, R12=0x2000D888, R13 (SP)=0x20003800, R14=0xFFFFFFFF, R15 (PC)=0x6E34, XPSR=0xF9000000, MSP=0x20003800, PSP=0x00, MSPLIM=0x00, PSPLIM=0x00, CFBP=0x00
T32C8 009:029.040 - 0.397ms returns 0x00
T32C8 009:029.889 JLINK_ReadMem(0x00006E34, 0x4 Bytes, ...)
T32C8 009:030.042    -- Read from flash cache (4 bytes @ 0x00006E34)
T32C8 009:030.161   Data:  08 B5 00 F0
T32C8 009:030.268 - 0.415ms returns 0
T0394 009:068.655 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T0394 009:068.821 - 0.217ms returns 0x08
T0394 009:068.914 JLINK_GetNumWPUnits()
T0394 009:068.976 - 0.091ms returns 4
T0394 009:069.041 JLINK_GetNumWPUnits()
T0394 009:069.103 - 0.091ms returns 4
T0394 009:070.169 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T0394 009:070.273 - 0.135ms returns 0x08
T0394 009:070.339 JLINK_GetNumWPUnits()
T0394 009:070.405 - 0.096ms returns 4
T0394 009:070.471 JLINK_GetNumWPUnits()
T0394 009:070.532 - 0.091ms returns 4
T0394 009:071.636 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T0394 009:071.735 - 0.132ms returns 0x08
T0394 009:071.805 JLINK_GetNumWPUnits()
T0394 009:071.866 - 0.092ms returns 4
T0394 009:071.933 JLINK_GetNumWPUnits()
T0394 009:071.995 - 0.091ms returns 4
T0394 009:073.174 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T0394 009:073.298 - 0.162ms returns 0x08
T0394 009:073.379 JLINK_GetNumWPUnits()
T0394 009:073.445 - 0.098ms returns 4
T0394 009:073.513 JLINK_GetNumWPUnits()
T0394 009:073.572 - 0.090ms returns 4
T0394 009:076.102 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T0394 009:076.349 - 0.322ms returns 0x08
T0394 009:076.470 JLINK_GetNumWPUnits()
T0394 009:076.567 - 0.128ms returns 4
T0394 009:076.637 JLINK_GetNumWPUnits()
T0394 009:076.741 - 0.135ms returns 4
T0394 009:078.806 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T0394 009:078.919 - 0.149ms returns 0x08
T0394 009:078.997 JLINK_GetNumWPUnits()
T0394 009:079.063 - 0.096ms returns 4
T0394 009:079.129 JLINK_GetNumWPUnits()
T0394 009:079.209 - 0.111ms returns 4
T0394 009:081.218 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T0394 009:081.333 - 0.146ms returns 0x08
T0394 009:081.399 JLINK_GetNumWPUnits()
T0394 009:081.459 - 0.091ms returns 4
T0394 009:081.523 JLINK_GetNumWPUnits()
T0394 009:081.584 - 0.089ms returns 4
T0394 009:083.952 JLINK_GetNumBPUnits(Type = 0xFFFFFF00)
T0394 009:084.082 - 0.161ms returns 0x08
T0394 009:084.149 JLINK_GetNumWPUnits()
T0394 009:084.212 - 0.093ms returns 4
T0394 009:084.277 JLINK_GetNumWPUnits()
T0394 009:084.337 - 0.090ms returns 4
T32C8 009:539.587 JLINK_ReadReg(XPSR)
T32C8 009:540.195 - 0.681ms returns 0xF9000000
T32C8 009:550.968 JLINK_ReadReg(XPSR)
T32C8 009:551.120 - 0.184ms returns 0xF9000000
T32C8 012:613.332 JLINK_STRACE_Read(..., NumItems = 0x10000)
T32C8 012:613.957 - 0.697ms NumItemsRead = 0x00
T32C8 012:614.083 JLINK_IsHalted()
T32C8 012:615.256 - 1.269ms returns TRUE
T32C8 012:615.417 JLINK_GoEx(MaxEmulInsts = 0, Flags = 0x01)
T32C8 012:615.526   CPU_ReadMem(4 bytes @ 0xE0001000)
T32C8 012:615.959   CPU_WriteMem(4 bytes @ 0xE0001004)
T32C8 012:617.154 - 1.836ms
T32C8 012:724.223 JLINK_IsHalted()
T32C8 012:724.597 - 0.403ms returns FALSE
T32C8 012:724.655 JLINK_IsHalted()
T32C8 012:724.956 - 0.329ms returns FALSE
T32C8 012:833.416 JLINK_IsHalted()
T32C8 012:833.873 - 0.526ms returns FALSE
T32C8 012:833.980 JLINK_IsHalted()
T32C8 012:834.316 - 0.367ms returns FALSE
T32C8 012:942.522 JLINK_IsHalted()
T32C8 012:942.965 - 0.479ms returns FALSE
T32C8 012:943.032 JLINK_IsHalted()
T32C8 012:943.351 - 0.361ms returns FALSE
T32C8 013:051.739 JLINK_IsHalted()
T32C8 013:053.228 - 1.558ms returns FALSE
T32C8 013:053.345 JLINK_IsHalted()
T32C8 013:053.774 - 0.476ms returns FALSE
T32C8 013:161.595 JLINK_IsHalted()
T32C8 013:162.007 - 0.449ms returns FALSE
T32C8 013:162.076 JLINK_IsHalted()
T32C8 013:162.388 - 0.337ms returns FALSE
T32C8 013:270.700 JLINK_IsHalted()
T32C8 013:271.094 - 0.430ms returns FALSE
T32C8 013:271.164 JLINK_IsHalted()
T32C8 013:271.475 - 0.343ms returns FALSE
T32C8 013:380.615 JLINK_IsHalted()
T32C8 013:381.035 - 0.449ms returns FALSE
T32C8 013:381.092 JLINK_IsHalted()
T32C8 013:381.465 - 0.412ms returns FALSE
T32C8 013:488.992 JLINK_IsHalted()
T32C8 013:489.404 - 0.465ms returns FALSE
T32C8 013:489.499 JLINK_IsHalted()
T32C8 013:489.848 - 0.388ms returns FALSE
T32C8 013:598.939 JLINK_IsHalted()
T32C8 013:600.131 - 1.247ms returns FALSE
T32C8 013:600.229 JLINK_IsHalted()
T32C8 013:600.636 - 0.458ms returns FALSE
T0394 013:618.675 JLINK_IsHalted()
T0394 013:619.205 - 0.592ms returns FALSE
T0394 013:619.317 JLINK_IsHalted()
T0394 013:619.675 - 0.405ms returns FALSE
T32C8 013:707.838 JLINK_IsHalted()
T32C8 013:708.221 - 0.427ms returns FALSE
T32C8 013:708.303 JLINK_IsHalted()
T32C8 013:708.639 - 0.375ms returns FALSE
T32C8 013:817.735 JLINK_IsHalted()
T32C8 013:818.203 - 0.523ms returns FALSE
T32C8 013:818.300 JLINK_IsHalted()
T32C8 013:818.672 - 0.413ms returns FALSE
T32C8 013:926.646 JLINK_IsHalted()
T32C8 013:927.147 - 0.552ms returns FALSE
T32C8 013:927.240 JLINK_IsHalted()
T32C8 013:927.571 - 0.370ms returns FALSE
T32C8 014:036.083 JLINK_IsHalted()
T32C8 014:053.606 - 17.736ms returns FALSE
T32C8 014:053.923 JLINK_IsHalted()
T32C8 014:054.483 - 0.758ms returns FALSE
T32C8 014:161.029 JLINK_IsHalted()
T32C8 014:161.444 - 0.456ms returns FALSE
T32C8 014:161.519 JLINK_IsHalted()
T32C8 014:161.859 - 0.373ms returns FALSE
T32C8 014:270.839 JLINK_IsHalted()
T32C8 014:271.244 - 0.440ms returns FALSE
T32C8 014:271.314 JLINK_IsHalted()
T32C8 014:271.638 - 0.357ms returns FALSE
T32C8 014:379.843 JLINK_IsHalted()
T32C8 014:380.261 - 0.447ms returns FALSE
T32C8 014:380.318 JLINK_IsHalted()
T32C8 014:380.699 - 0.425ms returns FALSE
T32C8 014:489.044 JLINK_IsHalted()
T32C8 014:489.530 - 0.516ms returns FALSE
T32C8 014:489.588 JLINK_IsHalted()
T32C8 014:489.968 - 0.419ms returns FALSE
T32C8 014:599.006 JLINK_IsHalted()
T32C8 014:599.479 - 0.546ms returns FALSE
T32C8 014:599.581 JLINK_IsHalted()
T32C8 014:599.947 - 0.399ms returns FALSE
T0394 014:620.376 JLINK_IsHalted()
T0394 014:620.772 - 0.435ms returns FALSE
T0394 014:620.842 JLINK_IsHalted()
T0394 014:621.181 - 0.377ms returns FALSE
T32C8 014:707.988 JLINK_IsHalted()
T32C8 014:708.404 - 0.464ms returns FALSE
T32C8 014:708.496 JLINK_IsHalted()
T32C8 014:708.876 - 0.426ms returns FALSE
T32C8 014:817.127 JLINK_IsHalted()
T32C8 014:817.546 - 0.448ms returns FALSE
T32C8 014:817.603 JLINK_IsHalted()
T32C8 014:817.962 - 0.397ms returns FALSE
T32C8 014:927.305 JLINK_IsHalted()
T32C8 014:927.775 - 0.505ms returns FALSE
T32C8 014:927.838 JLINK_IsHalted()
T32C8 014:928.218 - 0.413ms returns FALSE
T32C8 015:035.958 JLINK_IsHalted()
T32C8 015:036.333 - 0.413ms returns FALSE
T32C8 015:036.401 JLINK_IsHalted()
T32C8 015:036.731 - 0.364ms returns FALSE
T32C8 015:146.022 JLINK_IsHalted()
T32C8 015:146.445 - 0.452ms returns FALSE
T32C8 015:146.503 JLINK_IsHalted()
T32C8 015:146.855 - 0.381ms returns FALSE
T32C8 015:254.996 JLINK_IsHalted()
T32C8 015:255.423 - 0.457ms returns FALSE
T32C8 015:255.481 JLINK_IsHalted()
T32C8 015:255.902 - 0.459ms returns FALSE
T32C8 015:364.048 JLINK_IsHalted()
T32C8 015:364.467 - 0.449ms returns FALSE
T32C8 015:364.525 JLINK_IsHalted()
T32C8 015:364.906 - 0.420ms returns FALSE
T32C8 015:473.940 JLINK_IsHalted()
T32C8 015:474.393 - 0.483ms returns FALSE
T32C8 015:474.451 JLINK_IsHalted()
T32C8 015:474.821 - 0.399ms returns FALSE
T32C8 015:583.402 JLINK_IsHalted()
T32C8 015:583.825 - 0.460ms returns FALSE
T32C8 015:583.891 JLINK_IsHalted()
T32C8 015:584.219 - 0.373ms returns FALSE
T0394 015:621.846 JLINK_IsHalted()
T0394 015:622.268 - 0.470ms returns FALSE
T0394 015:622.345 JLINK_IsHalted()
T0394 015:622.737 - 0.426ms returns FALSE
T32C8 015:692.438 JLINK_IsHalted()
T32C8 015:692.862 - 0.457ms returns FALSE
T32C8 015:692.923 JLINK_IsHalted()
T32C8 015:693.293 - 0.400ms returns FALSE
T32C8 015:801.532 JLINK_IsHalted()
T32C8 015:801.946 - 0.445ms returns FALSE
T32C8 015:802.005 JLINK_IsHalted()
T32C8 015:802.388 - 0.415ms returns FALSE
T32C8 015:911.801 JLINK_IsHalted()
T32C8 015:912.257 - 0.516ms returns FALSE
T32C8 015:912.366 JLINK_IsHalted()
T32C8 015:912.724 - 0.395ms returns FALSE
T32C8 016:020.276 JLINK_IsHalted()
T32C8 016:020.685 - 0.439ms returns FALSE
T32C8 016:020.743 JLINK_IsHalted()
T32C8 016:021.109 - 0.395ms returns FALSE
T32C8 016:130.233 JLINK_IsHalted()
T32C8 016:130.680 - 0.478ms returns FALSE
T32C8 016:130.739 JLINK_IsHalted()
T32C8 016:131.114 - 0.405ms returns FALSE
T32C8 016:239.434 JLINK_IsHalted()
T32C8 016:239.813 - 0.414ms returns FALSE
T32C8 016:239.879 JLINK_IsHalted()
T32C8 016:240.213 - 0.367ms returns FALSE
T32C8 016:348.471 JLINK_IsHalted()
T32C8 016:348.909 - 0.468ms returns FALSE
T32C8 016:348.967 JLINK_IsHalted()
T32C8 016:349.312 - 0.382ms returns FALSE
T32C8 016:458.408 JLINK_IsHalted()
T32C8 016:458.817 - 0.439ms returns FALSE
T32C8 016:458.875 JLINK_IsHalted()
T32C8 016:459.227 - 0.382ms returns FALSE
T32C8 016:567.148 JLINK_IsHalted()
T32C8 016:567.601 - 0.482ms returns FALSE
T32C8 016:567.659 JLINK_IsHalted()
T32C8 016:568.028 - 0.399ms returns FALSE
T0394 016:623.533 JLINK_IsHalted()
T0394 016:623.995 - 0.511ms returns FALSE
T0394 016:624.084 JLINK_IsHalted()
T0394 016:624.482 - 0.427ms returns FALSE
T32C8 016:677.031 JLINK_IsHalted()
T32C8 016:677.609 - 0.628ms returns FALSE
T32C8 016:677.775 JLINK_IsHalted()
T32C8 016:678.163 - 0.433ms returns FALSE
T32C8 016:786.111 JLINK_IsHalted()
T32C8 016:786.533 - 0.452ms returns FALSE
T32C8 016:786.591 JLINK_IsHalted()
T32C8 016:786.974 - 0.413ms returns FALSE
T32C8 016:896.001 JLINK_IsHalted()
T32C8 016:896.403 - 0.449ms returns FALSE
T32C8 016:896.491 JLINK_IsHalted()
T32C8 016:896.823 - 0.373ms returns FALSE
T32C8 017:004.894 JLINK_IsHalted()
T32C8 017:005.267 - 0.412ms returns FALSE
T32C8 017:005.339 JLINK_IsHalted()
T32C8 017:005.664 - 0.358ms returns FALSE
T32C8 017:114.493 JLINK_IsHalted()
T32C8 017:114.919 - 0.456ms returns FALSE
T32C8 017:114.978 JLINK_IsHalted()
T32C8 017:115.380 - 0.437ms returns FALSE
T32C8 017:223.362 JLINK_IsHalted()
T32C8 017:223.841 - 0.510ms returns FALSE
T32C8 017:223.917 JLINK_IsHalted()
T32C8 017:224.292 - 0.406ms returns FALSE
T32C8 017:333.483 JLINK_IsHalted()
T32C8 017:333.903 - 0.450ms returns FALSE
T32C8 017:333.960 JLINK_IsHalted()
T32C8 017:334.347 - 0.417ms returns FALSE
T32C8 017:442.480 JLINK_IsHalted()
T32C8 017:442.897 - 0.447ms returns FALSE
T32C8 017:442.955 JLINK_IsHalted()
T32C8 017:443.361 - 0.445ms returns FALSE
T32C8 017:552.233 JLINK_IsHalted()
T32C8 017:552.622 - 0.420ms returns FALSE
T32C8 017:552.682 JLINK_IsHalted()
T32C8 017:553.002 - 0.351ms returns FALSE
T0394 017:624.827 JLINK_IsHalted()
T0394 017:625.298 - 0.520ms returns FALSE
T0394 017:625.384 JLINK_IsHalted()
T0394 017:625.767 - 0.417ms returns FALSE
T32C8 017:661.425 JLINK_IsHalted()
T32C8 017:661.840 - 0.444ms returns FALSE
T32C8 017:661.897 JLINK_IsHalted()
T32C8 017:662.266 - 0.399ms returns FALSE
T32C8 017:770.393 JLINK_IsHalted()
T32C8 017:770.838 - 0.474ms returns FALSE
T32C8 017:770.895 JLINK_IsHalted()
T32C8 017:771.264 - 0.398ms returns FALSE
T32C8 017:880.550 JLINK_IsHalted()
T32C8 017:880.961 - 0.441ms returns FALSE
T32C8 017:881.018 JLINK_IsHalted()
T32C8 017:881.391 - 0.420ms returns FALSE
T32C8 017:989.798 JLINK_IsHalted()
T32C8 017:990.210 - 0.441ms returns FALSE
T32C8 017:990.267 JLINK_IsHalted()
T32C8 017:990.637 - 0.400ms returns FALSE
T32C8 018:099.112 JLINK_IsHalted()
T32C8 018:099.539 - 0.464ms returns FALSE
T32C8 018:099.607 JLINK_IsHalted()
T32C8 018:099.946 - 0.369ms returns FALSE
T32C8 018:208.151 JLINK_IsHalted()
T32C8 018:208.548 - 0.427ms returns FALSE
T32C8 018:208.606 JLINK_IsHalted()
T32C8 018:208.965 - 0.398ms returns FALSE
T32C8 018:317.445 JLINK_IsHalted()
T32C8 018:317.891 - 0.476ms returns FALSE
T32C8 018:317.949 JLINK_IsHalted()
T32C8 018:318.335 - 0.418ms returns FALSE
T32C8 018:426.566 JLINK_IsHalted()
T32C8 018:427.015 - 0.479ms returns FALSE
T32C8 018:427.073 JLINK_IsHalted()
T32C8 018:427.435 - 0.391ms returns FALSE
T32C8 018:536.516 JLINK_IsHalted()
T32C8 018:536.956 - 0.471ms returns FALSE
T32C8 018:537.015 JLINK_IsHalted()
T32C8 018:537.385 - 0.401ms returns FALSE
T0394 018:626.683 JLINK_IsHalted()
T0394 018:627.068 - 0.415ms returns FALSE
T0394 018:627.126 JLINK_IsHalted()
T0394 018:627.540 - 0.447ms returns FALSE
T32C8 018:646.222 JLINK_IsHalted()
T32C8 018:646.673 - 0.494ms returns FALSE
T32C8 018:646.748 JLINK_IsHalted()
T32C8 018:647.092 - 0.383ms returns FALSE
T32C8 018:755.248 JLINK_IsHalted()
T32C8 018:755.653 - 0.435ms returns FALSE
T32C8 018:755.711 JLINK_IsHalted()
T32C8 018:756.071 - 0.401ms returns FALSE
T32C8 018:864.129 JLINK_IsHalted()
T32C8 018:864.574 - 0.474ms returns FALSE
T32C8 018:864.632 JLINK_IsHalted()
T32C8 018:865.001 - 0.398ms returns FALSE
T32C8 018:974.142 JLINK_IsHalted()
T32C8 018:974.582 - 0.470ms returns FALSE
T32C8 018:974.639 JLINK_IsHalted()
T32C8 018:974.985 - 0.385ms returns FALSE
T32C8 019:083.521 JLINK_IsHalted()
T32C8 019:083.953 - 0.461ms returns FALSE
T32C8 019:084.010 JLINK_IsHalted()
T32C8 019:084.390 - 0.409ms returns FALSE
T32C8 019:192.383 JLINK_IsHalted()
T32C8 019:192.820 - 0.478ms returns FALSE
T32C8 019:192.893 JLINK_IsHalted()
T32C8 019:193.248 - 0.400ms returns FALSE
T32C8 019:302.419 JLINK_IsHalted()
T32C8 019:302.827 - 0.438ms returns FALSE
T32C8 019:302.885 JLINK_IsHalted()
T32C8 019:303.256 - 0.400ms returns FALSE
T32C8 019:411.671 JLINK_IsHalted()
T32C8 019:412.214 - 0.581ms returns FALSE
T32C8 019:412.281 JLINK_IsHalted()
T32C8 019:412.659 - 0.407ms returns FALSE
T32C8 019:520.607 JLINK_IsHalted()
T32C8 019:521.042 - 0.464ms returns FALSE
T32C8 019:521.099 JLINK_IsHalted()
T32C8 019:521.468 - 0.408ms returns FALSE
T0394 019:628.489 JLINK_IsHalted()
T0394 019:628.959 - 0.510ms returns FALSE
T0394 019:629.029 JLINK_IsHalted()
T0394 019:629.408 - 0.408ms returns FALSE
T32C8 019:630.024 JLINK_IsHalted()
T32C8 019:630.405 - 0.414ms returns FALSE
T32C8 019:630.467 JLINK_IsHalted()
T32C8 019:630.856 - 0.429ms returns FALSE
T32C8 019:739.959 JLINK_IsHalted()
T32C8 019:740.409 - 0.484ms returns FALSE
T32C8 019:740.471 JLINK_IsHalted()
T32C8 019:740.851 - 0.410ms returns FALSE
T32C8 019:849.005 JLINK_IsHalted()
T32C8 019:849.403 - 0.428ms returns FALSE
T32C8 019:849.460 JLINK_IsHalted()
T32C8 019:849.832 - 0.410ms returns FALSE
T32C8 019:957.983 JLINK_IsHalted()
T32C8 019:958.403 - 0.449ms returns FALSE
T32C8 019:958.460 JLINK_IsHalted()
T32C8 019:958.824 - 0.394ms returns FALSE
T32C8 020:067.953 JLINK_IsHalted()
T32C8 020:068.380 - 0.457ms returns FALSE
T32C8 020:068.437 JLINK_IsHalted()
T32C8 020:068.813 - 0.414ms returns FALSE
T32C8 020:176.662 JLINK_IsHalted()
T32C8 020:177.085 - 0.462ms returns FALSE
T32C8 020:177.155 JLINK_IsHalted()
T32C8 020:177.498 - 0.374ms returns FALSE
T32C8 020:285.865 JLINK_IsHalted()
T32C8 020:286.312 - 0.477ms returns FALSE
T32C8 020:286.370 JLINK_IsHalted()
T32C8 020:286.767 - 0.446ms returns FALSE
T32C8 020:395.858 JLINK_IsHalted()
T32C8 020:396.267 - 0.439ms returns FALSE
T32C8 020:396.325 JLINK_IsHalted()
T32C8 020:396.695 - 0.400ms returns FALSE
T32C8 020:504.818 JLINK_IsHalted()
T32C8 020:505.239 - 0.450ms returns FALSE
T32C8 020:505.296 JLINK_IsHalted()
T32C8 020:505.674 - 0.407ms returns FALSE
T32C8 020:614.118 JLINK_IsHalted()
T32C8 020:614.558 - 0.470ms returns FALSE
T32C8 020:614.615 JLINK_IsHalted()
T32C8 020:614.963 - 0.393ms returns FALSE
T0394 020:630.457 JLINK_IsHalted()
T0394 020:630.866 - 0.459ms returns FALSE
T0394 020:630.944 JLINK_IsHalted()
T0394 020:631.350 - 0.447ms returns FALSE
T32C8 020:724.048 JLINK_IsHalted()
T32C8 020:724.456 - 0.437ms returns FALSE
T32C8 020:724.513 JLINK_IsHalted()
T32C8 020:724.878 - 0.415ms returns FALSE
T32C8 020:833.124 JLINK_IsHalted()
T32C8 020:833.549 - 0.455ms returns FALSE
T32C8 020:833.607 JLINK_IsHalted()
T32C8 020:834.002 - 0.442ms returns FALSE
T32C8 020:942.267 JLINK_IsHalted()
T32C8 020:942.686 - 0.449ms returns FALSE
T32C8 020:942.743 JLINK_IsHalted()
T32C8 020:943.115 - 0.411ms returns FALSE
T32C8 021:052.065 JLINK_IsHalted()
T32C8 021:052.469 - 0.433ms returns FALSE
T32C8 021:052.526 JLINK_IsHalted()
T32C8 021:052.839 - 0.340ms returns FALSE
T32C8 021:160.955 JLINK_IsHalted()
T32C8 021:161.506 - 0.626ms returns FALSE
T32C8 021:161.638 JLINK_IsHalted()
T32C8 021:162.034 - 0.457ms returns FALSE
T32C8 021:270.998 JLINK_IsHalted()
T32C8 021:271.412 - 0.445ms returns FALSE
T32C8 021:271.471 JLINK_IsHalted()
T32C8 021:271.791 - 0.351ms returns FALSE
T32C8 021:379.820 JLINK_IsHalted()
T32C8 021:380.264 - 0.485ms returns FALSE
T32C8 021:380.337 JLINK_IsHalted()
T32C8 021:380.675 - 0.375ms returns FALSE
T32C8 021:489.725 JLINK_IsHalted()
T32C8 021:490.167 - 0.490ms returns FALSE
T32C8 021:490.249 JLINK_IsHalted()
T32C8 021:490.588 - 0.377ms returns FALSE
T32C8 021:598.756 JLINK_IsHalted()
T32C8 021:599.177 - 0.450ms returns FALSE
T32C8 021:599.234 JLINK_IsHalted()
T32C8 021:599.603 - 0.399ms returns FALSE
T0394 021:632.114 JLINK_IsHalted()
T0394 021:632.582 - 0.504ms returns FALSE
T0394 021:632.648 JLINK_IsHalted()
T0394 021:633.026 - 0.408ms returns FALSE
T32C8 021:708.284 JLINK_IsHalted()
T32C8 021:708.720 - 0.474ms returns FALSE
T32C8 021:708.788 JLINK_IsHalted()
T32C8 021:709.129 - 0.398ms returns FALSE
T32C8 021:817.291 JLINK_IsHalted()
T32C8 021:817.721 - 0.460ms returns FALSE
T32C8 021:817.780 JLINK_IsHalted()
T32C8 021:818.150 - 0.400ms returns FALSE
T32C8 021:927.265 JLINK_IsHalted()
T32C8 021:927.684 - 0.448ms returns FALSE
T32C8 021:927.741 JLINK_IsHalted()
T32C8 021:928.120 - 0.408ms returns FALSE
T32C8 022:036.110 JLINK_IsHalted()
T32C8 022:036.545 - 0.465ms returns FALSE
T32C8 022:036.602 JLINK_IsHalted()
T32C8 022:036.970 - 0.397ms returns FALSE
T32C8 022:145.749 JLINK_IsHalted()
T32C8 022:146.159 - 0.460ms returns FALSE
T32C8 022:146.241 JLINK_IsHalted()
T32C8 022:146.574 - 0.364ms returns FALSE
T32C8 022:255.143 JLINK_IsHalted()
T32C8 022:255.569 - 0.456ms returns FALSE
T32C8 022:255.627 JLINK_IsHalted()
T32C8 022:255.994 - 0.396ms returns FALSE
T32C8 022:364.904 JLINK_IsHalted()
T32C8 022:365.330 - 0.458ms returns FALSE
T32C8 022:365.390 JLINK_IsHalted()
T32C8 022:365.742 - 0.382ms returns FALSE
T32C8 022:474.301 JLINK_IsHalted()
T32C8 022:474.713 - 0.441ms returns FALSE
T32C8 022:474.770 JLINK_IsHalted()
T32C8 022:475.147 - 0.406ms returns FALSE
T32C8 022:583.308 JLINK_IsHalted()
T32C8 022:583.713 - 0.435ms returns FALSE
T32C8 022:583.771 JLINK_IsHalted()
T32C8 022:584.168 - 0.427ms returns FALSE
T0394 022:633.602 JLINK_IsHalted()
T0394 022:634.005 - 0.434ms returns FALSE
T0394 022:634.084 JLINK_IsHalted()
T0394 022:634.458 - 0.424ms returns FALSE
T32C8 022:692.745 JLINK_IsHalted()
T32C8 022:693.193 - 0.478ms returns FALSE
T32C8 022:693.251 JLINK_IsHalted()
T32C8 022:693.618 - 0.397ms returns FALSE
T32C8 022:801.735 JLINK_IsHalted()
T32C8 022:802.169 - 0.466ms returns FALSE
T32C8 022:802.229 JLINK_IsHalted()
T32C8 022:802.597 - 0.406ms returns FALSE
T32C8 022:911.256 JLINK_IsHalted()
T32C8 022:911.646 - 0.429ms returns FALSE
T32C8 022:911.715 JLINK_IsHalted()
T32C8 022:912.066 - 0.388ms returns FALSE
T32C8 023:021.207 JLINK_IsHalted()
T32C8 023:021.615 - 0.438ms returns FALSE
T32C8 023:021.673 JLINK_IsHalted()
T32C8 023:022.032 - 0.389ms returns FALSE
T32C8 023:130.064 JLINK_IsHalted()
T32C8 023:130.520 - 0.482ms returns FALSE
T32C8 023:130.574 JLINK_IsHalted()
T32C8 023:130.949 - 0.401ms returns FALSE
T32C8 023:239.512 JLINK_IsHalted()
T32C8 023:239.925 - 0.446ms returns FALSE
T32C8 023:239.989 JLINK_IsHalted()
T32C8 023:240.320 - 0.362ms returns FALSE
T32C8 023:348.597 JLINK_IsHalted()
T32C8 023:349.027 - 0.460ms returns FALSE
T32C8 023:349.085 JLINK_IsHalted()
T32C8 023:349.452 - 0.406ms returns FALSE
T32C8 023:458.521 JLINK_IsHalted()
T32C8 023:458.985 - 0.500ms returns FALSE
T32C8 023:459.053 JLINK_IsHalted()
T32C8 023:459.405 - 0.388ms returns FALSE
T32C8 023:567.436 JLINK_IsHalted()
T32C8 023:567.869 - 0.525ms returns FALSE
T32C8 023:568.008 JLINK_IsHalted()
T32C8 023:568.420 - 0.470ms returns FALSE
T0394 023:634.843 JLINK_IsHalted()
T0394 023:635.306 - 0.496ms returns FALSE
T0394 023:635.377 JLINK_IsHalted()
T0394 023:635.739 - 0.393ms returns FALSE
T32C8 023:677.091 JLINK_IsHalted()
T32C8 023:677.533 - 0.472ms returns FALSE
T32C8 023:677.591 JLINK_IsHalted()
T32C8 023:677.991 - 0.429ms returns FALSE
T32C8 023:786.008 JLINK_IsHalted()
T32C8 023:786.433 - 0.455ms returns FALSE
T32C8 023:786.491 JLINK_IsHalted()
T32C8 023:786.882 - 0.436ms returns FALSE
T32C8 023:896.168 JLINK_IsHalted()
T32C8 023:896.567 - 0.431ms returns FALSE
T32C8 023:896.627 JLINK_IsHalted()
T32C8 023:896.969 - 0.400ms returns FALSE
T32C8 024:005.106 JLINK_IsHalted()
T32C8 024:005.542 - 0.467ms returns FALSE
T32C8 024:005.602 JLINK_IsHalted()
T32C8 024:006.013 - 0.442ms returns FALSE
T32C8 024:114.053 JLINK_IsHalted()
T32C8 024:114.468 - 0.445ms returns FALSE
T32C8 024:114.526 JLINK_IsHalted()
T32C8 024:114.880 - 0.383ms returns FALSE
T32C8 024:223.983 JLINK_IsHalted()
T32C8 024:224.428 - 0.475ms returns FALSE
T32C8 024:224.490 JLINK_IsHalted()
T32C8 024:224.847 - 0.394ms returns FALSE
T32C8 024:333.414 JLINK_IsHalted()
T32C8 024:333.873 - 0.498ms returns FALSE
T32C8 024:333.942 JLINK_IsHalted()
T32C8 024:334.303 - 0.392ms returns FALSE
T32C8 024:442.452 JLINK_IsHalted()
T32C8 024:442.876 - 0.455ms returns FALSE
T32C8 024:442.935 JLINK_IsHalted()
T32C8 024:443.307 - 0.405ms returns FALSE
T32C8 024:551.537 JLINK_IsHalted()
T32C8 024:551.983 - 0.476ms returns FALSE
T32C8 024:552.040 JLINK_IsHalted()
T32C8 024:552.389 - 0.388ms returns FALSE
T0394 024:636.114 JLINK_IsHalted()
T0394 024:636.518 - 0.445ms returns FALSE
T0394 024:636.612 JLINK_IsHalted()
T0394 024:636.959 - 0.378ms returns FALSE
T32C8 024:661.422 JLINK_IsHalted()
T32C8 024:661.846 - 0.453ms returns FALSE
T32C8 024:661.903 JLINK_IsHalted()
T32C8 024:662.269 - 0.395ms returns FALSE
T1EFC 025:209.812 JLINK_Halt()
T1EFC 025:212.557 - 2.798ms returns 0x00
T1EFC 025:212.642 JLINK_ReadReg(XPSR)
T1EFC 025:213.001   CPU_ReadMem(4 bytes @ 0xE000EE08)
T1EFC 025:213.384 - 0.796ms returns 0x89000000
T1EFC 025:220.580 JLINK_Close()
T1EFC 025:342.442 - 122.555ms
T1EFC 025:343.238   
T1EFC 025:343.302   Closed
